46
Shipping
7
2005-10-01
2005-10-01
false

Additional Requirements for Passenger Vessels
C

Subpart C
Shipping
COAST GUARD, DEPARTMENT OF HOMELAND SECURITY (CONTINUED)
LIFESAVING APPLIANCES AND ARRANGEMENTS
LIFESAVING SYSTEMS FOR CERTAIN INSPECTED VESSELS

Subpart C—Additional Requirements for Passenger Vessels
§ 199.200
General.
Passenger vessels and special purpose vessels described in § 199.10(e), must meet the requirements in this subpart in addition to the requirements in subparts A and B of this part.
[CGD 84-069, 61 FR 25313, May 20, 1996, as amended by USCG-1999-6216, 64 FR 53229, Oct. 1, 1999]
§ 199.201
Survival craft.
(a) Each survival craft must be approved and equipped as follows:
(1) Each lifeboat must be approved under approval series 160.135 and equipped as specified in table 199.175 of this part.
(2) Each inflatable liferaft must be approved under approval series 160.151 and equipped with—
(i) A SOLAS A pack; or
(ii) For a passenger vessel on a short international voyage, a SOLAS B pack.
(3) Each rigid liferaft must be approved under approval series 160.118 and equipped as specified in table 199.175 of this part.
(4) Each marine evacuation system must be approved under approval series 160.175.
(5) Each liferaft must have a capacity of six persons or more.
(b) Each passenger vessel must carry the following:
(1) A combination of lifeboats and liferafts that have an aggregate capacity sufficient to accommodate the total number of persons on board, provided that—
(i) On each side of the vessel, lifeboats with an aggregate capacity sufficient to accommodate at least 37.5 percent of the total number of persons on board are carried; and
(ii) Any liferafts that are provided in combination with the lifeboats are served by launching appliances or marine evacuation systems equally distributed on each side of the vessel.
(2) In addition to the survival craft required in paragraph (b)(1) of this section, additional liferafts must be provided that have a aggregate capacity sufficient to accommodate at least 25 percent of the total number of persons on board. The additional liferafts—
(i) Must be served by at least one launching appliance or marine evacuation system on each side of the vessel. These launching appliances or marine evacuation systems must be those described under paragraph (b)(1)(ii) of this section or be equivalent approved appliances capable of being used on both sides of the vessel; and
(ii) Are not required to be stowed in accordance with § 199.130(c)(4).
(c) Each passenger vessel engaged on a short international voyage that also complies with the standards of subdivision requirements for vessels on short international voyages as described in subchapter S of this chapter may, as an alternative to the lifeboat requirements in paragraph (b)(1)(i) of this section, carry lifeboats with an aggregate capacity sufficient to accommodate at least 30 percent of the total number of persons on board. These lifeboats must be equally distributed, as far as practicable, on each side of the vessel.
(d) Each passenger vessel that is less than 500 tons gross tonnage and is certificated to permit less than 200 persons on board is not required to meet the requirements of paragraphs (b) or (c) of this section if it meets the following:
(1) On each side of the vessel—
(i) Liferafts are carried with an aggregate capacity sufficient to accommodate the total number of persons on board and are stowed in a position providing for easy side-to-side transfer at a single open deck level; or
(ii) Liferafts are carried with an aggregate capacity sufficient to accommodate 150 percent of the total number of persons on board. If the rescue boat required under § 199.202 is also a lifeboat, its capacity may be included to meet the aggregate capacity requirement.
(2) If the largest survival craft on either side of the vessel is lost or rendered unserviceable, there must be survival craft available for use on each side of the vessel, including those which are stowed in a position providing for side-to-side transfer at a single open deck level, with a capacity sufficient to accommodate the total number of persons on board.
§ 199.202
Rescue boats.
(a) Each passenger vessel of 500 tons gross tonnage and over must carry on each side of the vessel at least one rescue boat approved under approval series 160.156 that is equipped as specified in table 199.175 of this part.
(b) Each passenger vessel of less than 500 tons gross tonnage must carry at least one rescue boat approved under approval series 160.156 that is equipped as specified in table 199.175 of this part.
(c) A lifeboat is accepted as a rescue boat if, in addition to being approved under approval series 160.135, it is also approved under approval series 160.156.
§ 199.203
Marshalling of liferafts.
(a) Each passenger vessel must have a lifeboat or rescue boat for each six liferafts when—
(1) Each lifeboat and rescue boat is loaded with its full complement of persons; and
(2) The minimum number of liferafts necessary to accommodate the remainder of the persons on board have been launched.
(b) A passenger vessel engaged on a short international voyage that also complies with the standards of subdivision requirements for vessels on short international voyages as described in subchapter S of this chapter may have a lifeboat or rescue boat for each nine liferafts when—
(1) Each lifeboat and rescue boat is loaded with its full complement of persons; and
(2) The minimum number of liferafts necessary to accommodate the remainder of the persons on board have been launched.
§ 199.211
Lifebuoys.
(a) Each passenger vessel must carry the number of lifebuoys prescribed in table 199.211 of this section.
Table 199.211—Requirements for Lifebuoys for Passenger Vessels
Length of vessel in meters (feet) | Minimum number of lifebuoys
Under 60 (196) | 8
60(196) and under 120(393) | 12
120(393) and under 180 (590) | 18
180 (590) and under 240 (787) | 24
240 (787) and over | 30
(b) Notwithstanding § 199.70(a)(3)(ii), each passenger vessel under 60 meters (196 feet) in length must carry at least six lifebuoys with self-igniting lights.
[CGD 84-069, 61 FR 25313, May 20, 1996; 61 FR 40281, Aug. 1, 1996]
§ 199.212
Lifejackets.
(a) In addition to the lifejackets required under § 199.70(b), each passenger vessel must carry lifejackets for at least 5 percent of the total number of persons on board. These lifejackets must be stowed in conspicuous places on deck or at muster stations.
(b) Where lifejackets for persons other than the crew are stowed in staterooms located remotely from direct routes between public spaces and muster stations, any additional lifejackets required by § 199.70(b)(2)(v) for these persons must be stowed in the public spaces, near muster stations, or on direct routes between them. These lifejackets must be stowed so that their distribution and donning does not impede orderly movement to muster stations and survival craft embarkation stations.
§ 199.214
Immersion suits and thermal protective aids.
(a) Each passenger vessel must carry at least three immersion suits approved under approval series 160.171 for each lifeboat on the vessel.
(b) In addition to the requirements in paragraph (a) of this section, each passenger vessel must carry a thermal protective aid approved under approval series 160.174 for each person not provided with an immersion suit.
(c) The immersion suits and thermal protective aids required under paragraphs (a) and (b) of this section are not required if the passenger vessel operates only on routes between 32 degrees north and 32 degrees south latitude.
§ 199.217
Muster list and emergency instructions.
(a) The format of each passenger vessel muster list required under § 199.80 must be approved by the OCMI.
(b) The passenger vessel muster list or emergency instructions must include procedures for locating and rescuing persons other than the crew who may be trapped in their staterooms.
(c) As an alternative to the requirements in § 199.80(c), the passenger vessel emergency instructions may meet the requirements of MSC Circular 699 (Guidelines for Passenger Safety Instructions).
§ 199.220
Survival craft and rescue boat embarkation arrangements.
(a) Survival craft embarkation arrangements must be designed for—
(1) Each lifeboat to be boarded and launched either directly from the stowed position or from an embarkation deck, but not both; and
(2) Davit-launched liferafts to be boarded and launched from a position immediately adjacent to the stowed positions or from a position where, as described under § 199.130(c)(4), the liferaft is transferred before launching.
(b) Each rescue boat must be able to be boarded and launched directly from the stowed position with the number of persons assigned to crew the rescue boat on board. Notwithstanding paragraph (a)(1) of this section, if the rescue boat is also a lifeboat and the other lifeboats are boarded and launched from an embarkation deck, the arrangements must be such that the rescue boat can also be boarded and launched from the embarkation deck.
[CGD 84-069, 61 FR 25313, May 20, 1996, as amended by USCG-1999-6216, 64 FR 53229, Oct. 1, 1999]
§ 199.230
Stowage of survival craft.
(a) To meet the requirements of § 199.130(b)(1), each lifeboat on a passenger vessel of 80 meters (262 feet) in length and upwards must be stowed where the after-end of the lifeboat is at least 1.5 times the length of the lifeboat forward of the vessel's propeller.
(b) The stowage height of a survival craft must take into account the vessel's escape provisions, the vessel's size, and the weather conditions likely to be encountered in the vessel's intended area of operation.
(c) The height of the davit head of each davit when it is in position to launch the survival craft should, as far as practicable, not exceed 15 meters (49 feet) to the waterline when the vessel is in its lightest seagoing condition.
§ 199.240
Muster stations.
Each passenger vessel must, in addition to meeting the requirements of § 199.110, have muster stations that—
(a) Are near the embarkation stations, unless a muster station is also an embarkation station;
(b) Permit ready access to the embarkation station, unless a muster station is also an embarkation station; and
(c) Have sufficient room to marshal and instruct passengers and special personnel.
§ 199.245
Survival craft embarkation and launching arrangements.
(a) Each davit-launched liferaft must be arranged to be rapidly boarded by its full complement of persons.
(b) All survival craft required for abandonment by the total number of persons on board must be capable of being launched with the survival crafts' full complement of persons and equipment within a period of 30 minutes from the time the abandon-ship signal is given.
§ 199.250
Drills.
(a) An abandon-ship drill and a fire drill, as described in § 199.180, must be conducted on each passenger vessel at least weekly.
(b) The entire crew does not have to be involved in every drill, but each crewmember must participate in an abandon-ship drill and a fire drill each month.
(c) Passengers and special personnel must be strongly encouraged to attend abandon-ship and fire drills.