    [From the U.S. Government Printing Office, www.gpo.gov]

                       State of South Carolina
                         Monitoring Strategy
                                       for
                             Fiscal Year 1990

                            Technical Report No.   001-89
               _E-~~~~~~~~~ ~COAST/AL ZiE271
                                            INFOR6MATI C   ii.  --R

                             Bureau of Water Pollution Control
                          Office of Environmental Quality Control
                 South Carolina Department of Health and Environmental Control
                                    2600 Bull Street
       TD                            Columbia, South Carolina 29201
       224
       .S6
       S72
       1990
    �)

                   STATE OF SOUTH CAROLINA
                     MONITORING STRATEGY
                             FOR

                      FISCAL YEAR 1990

              U. S. DEPARTMENT OF COMMERCE NOAA
              COASTAL SERVICES CENTER
              2234 SOUTH HOBSON AVENUE
              CHARLESTON, SC 29405-2413

                  Technical Report No. 001-89

                          July 1989

                'rIoperty of csc Library

               Bureau of Water Pollution Control
            Office of Environmental Quality Control
              South Carolina Department of Health
                   and Environmental Control

     ~.              F  ,v[. FlrARTMENT OF COMMERCE NOAA
    .;            '' Ae ' ~  W SERvICES CENTER
                    : :  !LJTH HOBSON AVENUE
                      :-, iTON  SC 29405-2413

                            TABLE OF CONTENTS

                                                              Pagie

    List of Tables ..............................iii

    List of Figures..............................iv

    1.   Monitoring Strategy, South Carolina Department
        of Health and Environmental Control ..1...............
    II.  Overview of the South Carolina Water Quality
        Monitoring Program..........................                                    3
    III. Fixed Monitoring Network.......................                                 8

        A. Primary Stations.........................                                    8
        B. Secondary Stations ........................11
        C. Sediment Stations.........................12
        D. Schedule for the Ambient Monitoring Program
            for FY 89 by Laboratory District.................16
        E. Basic Water Monitoring Program ..................19
        F. Biological Monitoring.......................20
        G. Shellfish Monitoring........................27

    IV.  Intensive Surveys and Special Water Quality Studies..........30

        A. Point Source Wasteload Allocations ................30
        B. Special Water Quality Studies...................31
        C. Lake Edgar A. Brown........................31
        D. Clean Lakes Program........................32

    V.  Wastewater Discharge Compliance Monitoring ..............34

        A. Compliance Schedule Tracking ...................34
        B. NPDES Self-Monitoring.......................35
        C.  Federal Compliance Evaluation Inspections (CEI)..........35
        D. State Operation and Maintenance Inspections............37
        E. Compliance Sampling Inspections..................39
        F. Performance Audit Inspections...................41
        G. Technical and/or Diagnostic Evaluations..............41
        H. Pretreatment Program Audit and/or Inspection ...........42

    VI. Quality Assurance/Quality Control Procedures .............43

    VII. Emergency Response ..........................45

        A.  Spill Response Team                             .......................45
        B.  Spill Prevention Control and Countermeasures (SPCC) ..........46
        C. Fish Kill Program.........................47
        D. Technical Assistance ........................48

    VIII. Complaint Investigations.......................50

                                  -1-

    IX. Drinking Water Supplies Monitoring Program ..............53

       A. Microbiological..........................53
       B. Inorganic Chemical.........................53
       C. Organic Chemical .........................53

    X. Ground-Water Protection ........................54

       A. Permit Issuance ..........................54
       B. Enforcement ................ ...........55
       C. Water Supply ...........................55
       D. 106 Program............................55
       E. Underground Injection Control Program ...............56
       F. Underground Storage Tank Program .................57

    XI.  Solid and Hazardous Wastes Facility Monitoring Program ........57

       A. Solid Waste Facilities ......................57
       B. Hazardous Waste Land Disposal Facilities .............58
    XII. Laboratory Support...........................60

       A. Laboratory Services........................60
       B. Analytical Services Quality Assurance Program...........60
       C. Sample Containers and Preservation ................61
       D. Laboratory Evaluation Program ...................63

    XIII. Data Handling ............................65

       A. Ambient Stream Data........................65
       B. Special Study Data.........................65
       C. Compliance Sampling........................65
       D. NPDES Compliance and Self Monitoring ...............65
        E. Federal Operation and Maintenance Inspections...........65
        F. State Operation and Maintenance Inspections............65
       G. Fish Kills......66
       H. Oil and Hazardous Mat'e'rialis'........................66
        1. Biological Monitoring.......................66

    XIV. Appendices ..............................67

       A.   South Carolina Department of Health and Environmental
           Control Primary and Secondary Stream Station Descriptions
           listed by Laboratory District

        B.   Primary and Secondary Stations Listed by Region Showing
           Individual Parameter Coverage

       C.   Trend Biological Monitoring Program Station Descriptions

       D.   Shellfish Station Descriptions Listed by Area

        E.   List of Facilities Requiring Federal Compliance Sampling
           Inspections by EQC District

                                -ii-

                                 LIST OF TABLES

    Table                                                                         Page

     1.  Sediment Stations.........................14

     2.      Fixed-Station Biological Monitoring Program
             Biological Community Coverage and Sampling Frequency.......22

     3.      Fixed-Station Biological Monitoring Program
             Species Requirements and Sample Size Restrictions
             for Tissue Analyses .......................23

     4.      Fixed-Station Biological Monitoring Program
             Proposed Number of Tissue Analyses by Station Type........23

     S.      Fixed-Station Biological Monitoring Program
             Organic Chemical Parameter Coverage and Proposed
             Sampling Frequency for Tissue Analyses..............24

     6.      Fixed-Station Biological Monitoring Program
             Inorganic Chemical Parameter Coverage and
             Proposed Sampling Frequency for Tissue Analyses .........25

     7.      Fixed-Station Shellfish Monitoring Program
             Physical and Bacteriological Parameter Coverage
             and Sampling Frequency......................29

     8.      Office of Environmental Quality Control
             EQC District Directory......................51

     9.      Sample Chain-of-Custody and Data Flow -
             Division of Analytical Services .................62

                                 LIST OF FIGURES

    South Carolina Department of Health and Environmental Control
     Trend Monitoring Network - Primary Stations................10

    South Carolina Department of Health and Environmental Control
     Trend Monitoring Network - Secondary Stations...............13

    Primary Stream Monitoring Stations - Lower Savannah District ........A3
    Secondary Stream Monitoring Stations - Lower Savannah District .......A5

    Primary Stream Monitoring Stations - Trident District............A8
    Secondary Stream Monitoring Stations - Trident District...........All

    Primary Stream Monitoring Stations - Central Midlands District .......A14
    Secondary Stream Monitoring Station - Central Midlands District            ...... AI

    Primary Stream Monitoring Stations - Pee Dee District............A17
    Secondary Stream Monitoring Stations - Pee Dee District...........A20

    Primary Stream Monitoring Stations - Appalachia II District.........A23
    Secondary Stream Monitoring Stations - Appalachia II District........A24

    Primary Stream Monitoring Stations - Catawba District ............A28
    Secondary Stream Monitoring Stations -Catawba District...........A31

    I. MONITORING STRATEGY -SOUTH CAROLINA DEPARTMENT OF HEALTH AND
      ENVIRONMENTAL CONTROL

      Puroose of This Strateczv

           The purpose of this strategy is to establish overall goals and
      objectives  for  those  key  elements  of  the  environmental   quality
      monitoring program which are most needed to achieve the goals of the
      South Carolina Pollution Control Act (PCA), the Clean Water Act (CWA),
      implement applicable State and Federal regulations, and implement the
      EPA Environmental Monitoring Policy. Water quality monitoring provides
      the data needed to regulate sources of water pollution, assess the
      quality  of  the  State's  waters  and  evaluate  the  environmental
      effectiveness   of  the  South  Carolina  Department   of  Health  and
      Environmental Control (SCOHEC) water quality programs.

      Scooe of This Strateqv
          1'Environmental  quality  monitoring"  is  defined  as  the  set  of
      activities which provides chemical, physical, geological, biological,
      and other environmental  data required by environmental  managers.   For
      the purpose of this strategy, water quality monitoring is limited to
      those activities involved in the State implementation of the Pollution
      Control  and Clean Water Acts  in  inland/coastal  waters.   "Regulatory
      monitoring" is the collection and analysis of ambient data needed for
      establishing environmental quality-based permit requirements and for
      assessing-~and enforcing compliance with permits.  Regulatory monitoring
      also provides data necessary for addressing environmental quality-based
      assessments of ambient water related to point source and, to a lesser
      degree, nonpoint source influences. Regulatory monitoring for assessing
      and enforcing compliance with permits is included in this strategy.

      Statement of StrateQv

      Ma.ior Obiectives: This strategy establishes three major objectives for
      S`CDHEC's environmental monitoring program:
      1.   Advance the Regulatory Monitoring Program:

                Regulatory   monitoring   for   establishing   and   enforcing
           environmental quality-based permit requirements is the highest
           priority of this strategy.  The goal is to provide comprehensive,
           reliable  data  to  SCDHEC  and  EPA  for  environmental   quality
           management,  construction  grant  and permit  decisions.   Attention
           .shoulId be given to identifying new problems as well as to
           controlling known problems.

      2.   Conduct Sound Assessments:

                Environmental quality assessments are defined as the analysis
           of environmental data to determine the quality of the ambient
           environment.  Assessments may use a number of different kinds of
           data,  e.g.,  concentrations  o f  pollutants  in  receiving  Waters,
           number of reported fish kills, and the amount of impact detected in
           natural  biological communities.   Projections of future conditions
           may also be done using detected ambient trends and data on expected
           pollution loads.

    3.   Evaluate Control Programs:

              SCDHEC  will  utilize  its  formal  program  management  and
         reporting   systems   for  guiding   SCDHEC  environmental   quality
         monitoring   activities   and   for   evaluating   SCDHEC   program
         performance.

              Program   evaluation   studies   use   environmental   quality
         assessments to evaluate the 'effects of pollution control  programs
         on environmental  conditions.   Program evaluation studies will  be
         performed as needed to evaluate the environmental results of major
         SCDHEC programs.  To the extent feasible, data will be extracted
         from on-going SCDHEC regulatory monitoring studies.

         Additional goals required for the accomplishment of the objectives
    outlined above include:

     Imorovinci Data Ouality: Quality assurance/quality control will continue
    to be a high priority.  The goal  is that all data used by SCDHEC for
    decision making will be of known and sufficient quality for the intended
    uses.

    Data Manaciement: The goal is that data systems will be made more useful
    so that SCOHEC managers will be able to use ambient data and assessments
    to determine  the  environmental  impacts  of decisions.   This  will  be
    accomplished by cross-linking existing data systems and developing
    . interactive  data  retrieval  and  analysis  mechanisms  usable  by  line
    managers and staff.

    I.OVERVIEW OF THE SOUTH CAROLINA WATER OUALITY MONITORING PROGRAM

           Under the Pollution Control and Clean Water Acts, SCDHEC has been
      delegated certain water quality monitoring duties. These include regu-
      latory monitoring, water quality assessment and program evaluation as
      needed to fulfill the requirements of the aforementioned Acts.  Within
      this framework specific responsibilities are as follows:

      A.   As first priority, the collection and analysis of data as needed to
           make water quality management decisions:

           1.   Identification of waters not fully supporting designated uses
                and priority waterbodies, i.e., those waters most needing
                water quality-based controls or other actions to protect the
                designated use, and preliminary determination of the reason(s)
                for  nonsupport  when   this  occurs.    Inclusion   of  this
                information in the biennial Section 305(b) Report to Congress.
                Focus is on toxics as well as conventional pollutants. Simple
                screening techniques may be appropriate for many situations.

           2.   Development of needed water quality-based controls for both
                conventional  and toxic pollutants.   For toxics, use of both
                the pollutant-specific and the biomonitoring techniques, as
                appropri ate.

           3.   As needed to supplement State and Regional  regulatory moni-
                toring, writing effluent and ambient data collection require-
                ments into permits for identifying waters in need of controls,
                developing controls, and assessing the effectiveness of these
                controls to ensure the use is maintained or restored.

      B.   Performance of any additional  monitoring needed for the Section
           305(b) Report to Congress, including monitoring needed to determine
           the status of waters not meeting designated uses and the
           preliminary reason(s) for nonattainment.

      C.   Ensuring  that  needed  environmental  data  are  provided  to  EPA,
           including appropriate assessment data; appropriate screening data;
           and all regulatory data, including data needed for approvals of
           water quality standards and wasteload allocations/total maximum
           daily loads.

      D.   Ensuring that appropriate quality assurance/quality control proce-
           dures have been followed for all data used in State decision making
           and for all data reported to EPA, including data reported by dis-
           chargers.

           To accomplish these responsibilities, several types of monitoring
      activities are carried out by SCOHEC's Water Quality Monitoring Section,
      Facilities Compliance Section, and Bureau of District Services person-
      nel. "Monitoring" is a simple term describing a multifaceted area
      composed  of  widely  diverse  activities.   While  there  are  different
      approaches and philosophies of water quality monitoring, it should
      always be remembered that monitoring is not an end in itself but is only
      a tool or mechanism to achieve a particular set of goals and objectives.

                                     -3-

        The primary goal is the attainment and maintenance of fishable/swimmable
        waters wherever possible as mandated by the Clean Water Act (CWA).

             The philosophy of water quality monitoring in South Carolina has
        been the recognition that monitoring is basically a service activity for
        the generation of accurate and timely data needed by program and admini-
        strative decision areas.  Monitoring is a-multifaceted discipline that
        requires a great deal of attention to each of those "facets" in order
        for the resulting  data to be useful.   Beyond this,  however,  is the
        necessity to use the monitoring area as a vehicle for a cohesive,
        interrelated approach to water pollution control via the diverse types
        of data that are a product of the monitoring system. It is through the
        monitoring program that sample acquisition, data management/reporting,
        program needs, committed tasks, and other such Departmental functions
        all meet. Thus, it is at this natural point of confluence that much
        opportunity is afforded for integration of sometimes apparently
        non-related tasks or programs into a step-wise, interrelated approach to
        the protection of water quality in the State.

             South Carolina's monitoring activities can be separated into three
        broad categories based on the types and intended uses of the data col-
        lected. In the following sections, each of these categories is defined,
        including a brief discussion of how the generated data are used.

      1. Monitoring for Water Quality-Based Controls

             The development of discharge controls based on receiving water
        quality  is  a very  high  priority.   It  involves  the  collection  and
        analysis of effluent and ambient data to develop water quality-based
        National Pollutant Discharge Elimination System (NPDES) permit limits.
        This involves the calculation of Total Maximum Daily Loads (TMDL) for
        specific waterbodies and Wasteload Allocations (WLA) for point source
        discharges.

             SCDHEC uses trend monitoring data and special study data,
        especially intensive survey data,  in developing WLAs and TMDLs.  The
        kinds of data collected for this type of monitoring may include physical
        and chemical characterization of effluent and receiving waters, stream
        hydraulics, macroinvertebrate and fish community assessment of the
        receiving stream, periphyton/phytoplankton sampling, and static and/or
        flow-through toxicity bioassays of effluents and receiving waters.

             These data are used by the Modelling Section in predictive
        mathematical models to help determine waste treatment levels needed to
        maintain instream standards.  The modelling results are then passed to
        engineers in the Domestic Wastewater, and Industrial and Agricultural
        Wastewater Divisions to be used as the basis for setting final NPDES
        permit limits.

    2.   Monitoring for NPDES Permit Compliance and Enforcement

             The NPDES permit is the principal regulatory tool for controlling
        the quantity of pollutants discharged to the State's waters and for
        obtaining  data  on  point-source  discharges.   Data  supplied  by  the
        discharger in the form of routine Discharge Monitoring Reports (DMR) and

                                       -4-

        data collected by SCDHEC personnel from. Compliance Sampling Inspections
        (State  CSI  and  Federal  3560),  Federal  Operation  and  Maintenance
        Evaluations (7500), State Operation and Maintenance Inspections (0&M),
        Performance  Audit  Inspections  (PAI),  Technical   and/or  Diagnostic
        Evaluations (TE), and Pretreatment Program Audit and Inspections are
        reviewed by the Facilities Compliance Section to determine the
        compliance status of a discharger.

             In all instances of effluent'noncompliance, enforcement actions are
        supported by all of the above data supplied by the Facilities Compliance
        Section and all trend monitoring, special studies, and biological
        monitoring data supplied by the Water Quality Monitoring Section.  The
        majority of the routine inspections and physicochemical trend monitoring
        activities are conducted by the Bureau of District Services personnel.
        Data secured and supplied by these monitoring activities are utilized in
        the  majority  of  SCOHEC's  Environmental  Quality  Control  enforcement
        activities.

    3.   Water Quality Assessment

             State administrators need to assess the quality of the aquatic
        environment so that they can make decisions concerning water program
        prioritj'es and provide reports to the public on the state of the
        environment, important trends over time, and accomplishments. They also
        need to evaluate the effectiveness of control measures.  Water quality
        assessments provide the data base necessary for making these kind of
        decisions. Water quality assessments can be broken down into two main
        types; routine long-term trend monitoring and special intensive surveys.

             Long-term trend monitoring is accomplished through the Fixed
        Monitoring Network which consists of Primary Stations, Secondary
        Stations, Sediment Stations, Basic Water Monitoring Program Stations,
         and Biological Monitoring Stations.  Data collected by this Network are
         used in the development of designated use classifications and water
        quality standards, which are in turn used to establish specific
        waterbody  use  classifications.   Review  of  these  trend  data  help
        determine if existing water quality is adequate to protect existing and
        designated uses and if appropriate standards have been set.  Used in
         such a manner, trend data provide valuable feedback to the NPDES permit
        writing section as an indication of necessary discharge restrictions.

             The data network also forms the basis of the biennial Report to
         Congress describing the quality of the State of South Carolina waters,
         as required by Section 305(b) of the Clean Water Act.  For this report,
         trend monitoring data at all primary stations is used to determine the
         extent to which State waters meet the goals of the CWA and achieve the
         State designated  use classifications  and standards.   In this manner,
         priority waterbodies (those not -meeting designated use goals) may be
         identified  for  special  study.   Also,  those  waterbodies  with  water
         quality exceeding designated use classifications and standards, may be
         identified and upgraded to new use classifications.

             Special Intensive Surveys are designed to address and answer
         special  concerns.   They are used to assess current  conditions,  sub-
         stantiate enforcement decisions, follow-up specific actions, respond to
         complaints or short-term problems, and collect data for use in the

                                        -5-

        calculation of TMDLs and WLAs.  They-are often conducted in conjunction
        with compliance sampling to document ambient conditions and sources of
        environmental impact. They are often initiated to investigate apparent
        problems indicated by the trend monitoring data and to determine the
        causes of nonsupport of designated uses.  The data typically collected
        during such surveys can be physical and chemical water quality
        parameters, hydraulic stream characteristics, biological sampling,
        effluent and compliance sampling, and toxicity testing.

             Thus, water quality assessment is a broad term describing a great
        multitude  of  monitoring  and  sampling  activities.   Water  quality
        assessment data can be used to fulfill a variety of goals; assessment of
        current conditions, assessment of long-term trends, determination of
        priority waterbodies, determination of designated use attainment/
        non-usable attainment areas, and identification of continuing or new
        problem areas.

             By integrating all of these monitoring programs it is possible to
        identify the sources of pollution and the reasons for nonattainment of
        designated uses, to completely answer specific issues, determine the
        efficiency of pollutant abatement programs, and allow administrative
        overview of program effectiveness.

             At this point, some discussion and much emphasis must be directed
        toward  the  quality  assurance/quality  control  program.   As  has  been
        stated previously numerous times, by numerous sources, water quality
        monitoring programs and subsequently-based decisions are only as good as
        the quality (accurateness, precision) of the crude data. Suffice it to
        say here, that an active and effective quality assurance/control program
        is a major cornerstone of this State's monitoring program and is
        considered a prime contribution to the success of the program.

             In designing studies, SCOHEC incorporates as many facets of these
        monitoring  activities  as  is  necessary  to  allow  a whole  waterbody
        approach to managing water quality.  This approach is very efficient,
        realizing a very complete picture of the water quality in a given water-
        body with the minimum man-hours and duplication of effort. This is the
        result primarily of sound assessment design and effective organization
        and coordination of resources.

        The last major consideration that has been given to developing a
    successful monitoring program by South Carolina is the identification of the
    users of data or the sources of data requests. In South Carolina, this group
    is quite diverse ranging from individual citizens to public interest groups
    to various local/state/federal agencies. Data users are:
         O    Departmental program areas (e.g., domestic wastewater engineers)

           � Water quality trend/ambient condition analysts
           O Wasteload allocation analysts

           O Public/private environmental groups

           O Public at large

                                        -6-

           � Other local/state/federal agencies (regulatory & non-regulatory)

         � Departmental administrators via program area outputs

        While this large group utilizes the data for different reasons, the
    Department uses and applies the data to the intermediate objectives and goals
    as previously discussed. This is done to ascertain whether progress is being
    made toward successful achievement of these goals and to make correct and
    appropriate decisions regarding maintenance and enhancement of desirable
    environmental quality in the State.

         Implicit in the identification of users of the data, whether in-
    Department or out-of-Department, is the capacity to communicate the data to
    interested  parties  efficiently  and  accurately.   Technical  reports  are
    produced for every special study and copies are available to any interested
    organization  or persons.   A list of technical  reports  is available  upon
    request. Additionally, all trend monitoring and special studies data, with
    the exception of some biological data, are stored in the EPA STORET computer
    system, and facility inspection data are stored in the EPA Computerized
    Permit Compliance System.  Summaries of'trend monitoring and special studies
    data are available in several formats through the Water Quality Monitoring
    Section, including the annual Program Plan and this Monitoring Strategy.

         Presently underway is the integration of certain program and service
    areas within the Department via a computer network such that communication
    between and among such areas will be greatly expedited and enhanced.
    Concomitant  with  this  intra-Departmental  improvement  will  be  likewise
    enhancement of communication to interested parties outside the Department.
    Since  the  computer  'network  will  allow  more  data  to  be  handled  more
    efficiently at a quicker pace, less time and effort will have to be spent by
    employees in handling the data and more time and effort will be spent on
    extracting what the data means and communicating that message to users.

         In the following sections, each aspect of the SCDHEC monitoring program
    is presented  in detail.   Included are descriptions  of station  locations,
    sampling frequency, parameter coverage, and quality assurance quality control
    procedures.

                                        -7-

    III. FIXED MONITORING NETWORK

             The purpose of the fixed monitoring network is to provide a system
        of stations that are sampled in a way that produces well defined data
        reflecting physical, chemical and biological conditions of the streams
        and lakes in South Carolina.

             All sampling procedur'es and analyses are performed in accordance
        with the State Quality Assurance Management Office (SQAMO) and all
        procedures follow the Standard ODeratinq and Ouality Control Procedures
        for Ambient Water Quality and Wastewater Facility Monitorinai (SCDHEC)
        and Procedures Manual for Stream and Wastewater Facility Flow Measure-
        ment (SCOHEC).

        A.   Primary Stations

             Primary stations are established and sampled in a uniform and
             logical manner over an extended period of time to provide solid
             baseline data. By reviewing data and establishing trends in water
             quality, the primary network aids in identifying stream segments as
             effluent limited or water quality limited.  Intensive water quality
             surveys, enforcement proceedings or other actions may be based on
             this  trend  data.   Our present  primary  network consists  of  196
             stations sampled once per month, year round.

             Stations are grouped according to the regional office responsible
             for their collection. Stations per region are:

             Aiken          34                              Florence       31
             Charleston     42                              Greenville     35
             Columbia       29                              Lancaster      25

             A statewide map of primary stations appears on the following page.

             Primary stations and descriptions are listed by region in Appendix
             A.  Criteria for location and establishment of primary stations
             are:

                   1. Influent to segment (sub-basin)
                   2. Effluent to segment
                   3. Major streams at state lines
                   4. Confluence of major streams
                   5. Above a major industrial area
                   6. Below a major industrial area
                   7. Water quality limited area
                   8. Major lake
                   9. Above major municipal area
                  10. Below major municipal area
                  11. Mouth of major tributary
                  12. Major water use area
                  13. Above major land use area
                  14. Below major land use area
                  15. Above a water intake
                  16. Sites located in intensive or special water quality
                       surveys
                  17. Other

                                        -8-

         Appendix A presents the primary stations and the rationale by which they
         were established.  Twenty-six (26) of these primary stream stations have
         been designated for inclusion in the U.S. EPA National Basic Water
         Monitoring Program (BWMP).

         Parameter coverage and frequency of analysis for the primary stations
         are as follows. .STORET parameter codes are also given:

                          Physical Parameters Samoled Monthly

    Flow or Stage Measurement  00061 or 00065    Conductivity*,**,***            00402
    Temperature***               00010              Total Suspended Solids   **00530
    Turbidity                    00076              Salinity*,***                00480
    Color*                       00080              Transparency**,*             00078
                                                   Chlorides*                   00940

                     Microbioloqical Parameters SamDled Monthly

    Fecal Coliform              31616 or 31615
    Total Coliform*              31506 or 31505

                          Chemical Parameters SamDled Monthly

    Dissolved Oxygen***          00300              Total Phosphorus             00665
    pH                           00400              Alkalinity                   00410
    BOD                          00310 or 80082    Total Organic Carbon        **00680
    Ammonia                      00610
    Nitrate-Nitrite              00630
    Total Kjeldahl Nitrogen    00625

                         Chemical Parameters SamDled Ouarterlv

    Lead                        01051               Manganese                    01055
    Cadmium                      01027              Copper                       01042
    Chromium                     01034              Mercury                      71900
    Zinc                         01092              Phenols*                     32730
    Nickel                      01067               Total Organic Carbon         00680
    Iron                        01045

                       Chemical Parameters SamDled Annually *,**

    Pesticide Scan including, but not limited to, the following:

         DDT                  39300, 39305               Toxaphene              39400
         DDD                  39310, 39315               Lindane                39782
         DDE                  39320, 39327               Alpha BHC              39337
         Aldrin                       39330              Beta BHC               39338
         Endrin                      39390               Ethion                 39398
         Dieldrin                    39380               Heptachlor             39410
         PCB's                       39516               Heptachlor Epoxide    39420
         Parathion                   39540               Malathion              39530

                                           -9-

                          *  026
                                    4'- t  c-j>--            * C~~~W-023

                                     >. 0-021-~~99
        4~~~~~~~~~>~~~~  021V                     /        k'    )~4ytW.041                               C
                 ~~~~~~312$            *,o             K             "~~~~~~~~~~~~~~J flifiF~~~1311

                                         ad     01          I          %f" tP:r
         22,42~~~~~~~~~~~~~~~~~~~W0 ,                               'c
                                    021~~~~~~~~~~~  (             Lth�N,  ,4~~- PY't.SC; l7I '~)08

                     A"~~~~~ /                                                                     N
                  ~~t{<,ftY\  $~~!r~1~~~' ~~~SkY$                     2          7         9          N~'~-

                    9IV2                            4      �                         f,}

                                      ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~ s2i   K~ Eel)L P 1
                                                  *S~~~~~~~~2&.   -~~~~~~~~~~~

    Fixed Monitorig Network                                      K      ? ~yYV. O$' ~T,
                                                                                               roP.

                                                        V-~~~k

                                                                           2 ~~~~~~~~~~~~~~~~0

                                                     -32jr~                                                I'

    Chemical Parameters Samoled Annually (continued)

         Pesticide Scan

         Diazinon                    39570              Guthion         39580

         Phosdrin                    39610              Trithion        39786

         Acid Extractable Organics  45582               Hardness        00900

         Base-Neutral Extractable   45583
           Organi cs

         Volatile Organics           84085
             *Selected Stations Only.

            **Basic Water Monitoring Program Stations (transparency only where
              appl icable) .
           ***Profiled at one (1) meter intervals at lake and estuary stations
              collected by boat.
              Appendix B includes the primary stations and individual parameters
              for each.
         B.   Secondarv Stations

              Our present secondary network consists of 355 strategically located
              stations.  The network is regionally organized with the following
              assignments:

              Aiken           26                        Florence         74
              Charleston      43                        Greenville      100
              Columbia        33                        Lancaster        79

              Secondary  stations  and  descriptions  are  listed  by  region  in
              Appendix A.  A statewide map of secondary stations appears on the
              following page.

              Secondary station locations are based on the following criteria:

              a.   Known water quality problem areas; secondary stations act as a
                   check on primary stations where data historically show poor
                   quality. These stations are usually located in relation to
                   smaller discharges throughout the state.

              b.   Potential water quality problem areas; stations in these areas
                   are located in high complaint areas, agricultural and domestic
                   non-point source areas, and areas where data have revealed
                   poor conditions.

              C.   Areas with the same. selection criteria as applied to primary
                   stations. In these cases the same problems or potential for
                   problems exist, but with a lesser degree of importance. These
                   areas still require monitoring, but on a less frequent basis.

                                         -11-

        Appendix A presents the secondary stations and the rationale by which
        they were established.

        Secondary stations are routinely sampled six (6) times per year, once
        per month  May  through  October.   Secondary  station  sampling  may  be
        suspended during intensive or special stream surveys or due to other
        higher priority samplings.

        Parameter coverage and STORET parameter codes are:

                  Physical Parameters SamDled Monthly May-October

        Temperature**  00010                      Salinity*,**            00480
        Turbidity       00076                     Conductivity*,**         00402
        Color*         00080

                  Chemical Parameters SamDled Monthly May-October

        Dissolved Oxygen**  00300                 Nitrate-Nitrite         00630
        pH                   00400                Total Phosphorus        00665
        BOD                  00310                Phenols*                32730
        Total Kjeldahl       00625                Ammonia*                00610
          Nitrogen*

              Microbiolocical Parameters Samoled Monthly May-October

         Fecal Coliform Bacteria    31616 or 31615
        Total Coliform Bacteria*   31506 or 31505

                       Chemical Parameters Samoled Annually

        Heavy Metals* Pesticides*
        Hardness*         00900                   Chlorides*              00940

        *Selected stations only.

       **Profiled at one (1) meter intervals at lake stations collected by boat;
         profiled at top, mid, and bottom depths at estuary stations collect.by
          boat.

        Appendix B includes the secondary stations and individual parameters for
         each.

    C.   Sediment Stations

        There are 191 selected sediment stations within South Carolina. Sediment
         stations  are  sampled  for analysis  once  per year.   Primary  sediment
         stations are located at the influent or effluent of a subbasin and areas
         of  environmental  sinks.   Secondary  sediment  stations  selected  for
         analysis are based on district input stemming from their knowledge of
         local problem areas. Table 1 lists the sediment stations by district.

                                         -12-

                                  �'r  ."*U'           Y\

                                                    '4   ~         4)  9'cw,'e'                      .plu,      CD 24

                                             Q~~~   864                        - ~~~~tS-*-'*~'""''
             An:-'�/                                                                                       P0PI48..d   ;-                 03.3eO
    ''   \'Q(; ��                           SOJ�/j;�i   N                                            'j'
                        f~L                I                                                                    IV                          I60   .   '033
                          8~~~~~41.  ~~~~~~~~~~~                         >    .nnv,4  -~~~~~~~~~~~~~~~~~~~~~~~~~Q5J  '1� .Fd~~~~~~~~~~~~~~~~~~~~~~~~t (�  N  'P Ott~~~~~~~~~~~~~~~~~~F'', �\

                                                   J~'    T7-                                                               r a     ,

                                             .b &-     aak     K                              cosV           )"

                      t~~~�~~~� �; ~ ~   I~i                       * C T   I-  �~                ) . \  N�~ ~ l l I r 1 1   ~ .�l Ur � o r /

      Fixed�-~   MonSitrn  Networ           *01                                                   ,, 2% .. ,~�"  !~%   �,   -'-     ,j'��    ~

                                                                                 P11.               '"*                     :: ~   V
                                                                                     d   .   i ** '1

                                                 I".  "'(       Si,                                                 I�I� ,��.~~~~~~~~~>1. 0
                                                                          7-                    or.Il                                             10

                                                                                         44�

                                 i~~~~~~~~'r *.*'
                                                         i' ~~~~~~~~~~~~~~�   -�~~~~~~~~
                                                                                      s�.��i~~~� i;   :i I6~~~Y   I   'h. �P41)     �PI�LI lli�~ ~ ~ ~ ~

                        Sediment Parameters Samoled Annually

              Total Kjeldahl Nitrogen  00627            Chromium                01029
              Total Phosphorus          00668           Mercury                 71921
              Per Cent Volatile Solids 70322            Cadmium                 01028
              Oil and Grease            00557           Nickel                  01068
              Lead                      01052           Pesticide Scan including,
                                                        but not limited to:
              Zinc                      01093
              Copper                    01043           DDT             39301, 39306
              PCB's                     39519           DDD             39311, 39316
              Acid Extractable          45582           DDE             39321, 39328
               Organics*                                Aldrin                  39333
              Base-Neutral Extractable 45583            Endrin                  39393
              Organics*                                 Dieldrin                39383
              Volatile Organics*        84085           Methoxychlor            39481
                                                        Lindane                39783
                                                        Toxaphene              39403

              *Selected stations only, see Table 1 below.

                                         Table 1

                                    Sediment Stations
    Columbia

         (a)  Primary:        S-204    *B-054    *CW-206
              November        S-223    *B-236      CW-207
                              S-260                CW-208
                              S-273    *C-007      CW-209
                              S-274               *CW-222
                              S-279    *CSB-OO1L
                              S-280    *CSB-OO1R
                              S-290

         (b)  Secondary:                B-077      E-035
              September                 B-316      E-101

    Aiken

         (a)  Primary:       *E-008    *SV-118    S-123       CSTL-012  ST-025
              December        E-013     SV-250    S-131       CSTL-028
                              E-059    *SV-291
                              E-090     SV-294
                              E-091     SV-318
                              E-092    *SV-323
                              E-094

         (b)  Secondary:      E-007A    SV-072    S-050
              September       E-076     SV-073    S-093
                                        SV-096    S-233

                                           -14-

    Greenville

         (a)  Primary;       SV-098    S-007       B-008     BE-001
              October       *SV-121
                            *SV-122
                             SV-227   *S-018      B-026    *BL-001
                             SV-288    S-021      B-041
                                        S-073     B-148
                                        S-088     B-317
                                       *5125
                                        S-250
                                        5-296

         (b)  Secondary:     SV-015    8-192
              September     *SV-037    B-302
                             SV-107
                             SV-137
                             SV-282

    Lancaster

         (a)  Primary:        B-042     PD-004    CW-013    CW-152
              October         B-044     PD-006   *CW-016    CW-197
                            *B.046     PD-080    CW-016F   CW-198
                              8-048     PD-113    CW-041    CW-201
                              8-051     P0-327    CW-057    CW-226

         (b)  Secondary:    *B-057      P0-066    CW-018   *CW.225
              September   B -086        P0-152   *CW-023
                              8-100               CW-027
                             *8-119                CW-155
                             *B-330              *CW-224

    Charieston

         (a)  Primary:       CSTL-006  SV-191   *ST-001    MD-007       M0-119
              December       CSTL-062             ST-006    MD-026      M0-120
                              CSTL-063             ST-016    M0-043      MD-152
                              CSTL-079 *E-015                MD-045     MD-195
                             *CSTL-098 *E-100               *MD-048      MD-202
                              CSTL-107                       MD-052      MD-241
                             *CSTL-109                       MD-115
                                                            MD-118

         (b)  Secondary:     CSTL-010  ST-007    MD-004    MD-209
              September      CSTL-013             MD-006    MD-210
                              CSTL-085            MD-010    MD-116
                                                  MD-206

         (c)  Biological:   *MD-214   *MD-634
              March         *MD-215   *MD-635
                             *MD-216   *MD-636
                             *MD-538   *MD-639
                             *MD-632   *MD-640
                             *MD.633   *MD-655

                                          -15-

    Florence

         (a)  Primary:       *MD-080    PD-012    PD-043    PD-170        PD-325
             November        MD-124   *PD-027    PD-052    PD-189        PD-332
                             MD-127   *PD-028   *PD-061   *PD-202
                             MD-146   *PD-038    PD-069    PD-227
                             MD-162    PD-041    PD-091    PD-281

         (b)  Secondary:      MD-158    PD-030A   PD-256
              September                 PD-081    PD-321
                                       PD-097
                                       PD-159

         (c)  Biological:   *MD-212   *MD-637
             March          *MD-213   *MD-638

              *Stations sampled for sediment organics (see above).

         D.   Schedule for the Ambient Monitorinq Proqram for FY'88 by Laboratory
              District

              The following is the schedule for collection of samples for primary
              water  stations,   primary  sediment   stations,   secondary  water
              stations, and secondary sediment stations for each District
              Laboratory.   The  schedule  includes  the  number  of each  type  of
              sample to be collected, and it also includes the month(s) for
              collection. Please refer to Section A, B, and C and Appendix C for
              details relevant to specific parameters for each station.

              Lab: Aiken

                   Primary Surface Stations -- 34

                   -Quarterly for metals, TOC, and phenols* -- March, June,
                     September and December
                   -Annually for Pesticide - PCB's and other organics (selected
                     stations) -- April
                   -Annually for hardness (selected stations) -- to coincide with
                     one of the metals samples

                   Primary Sediment Stations -- 18
                   -Collected in December

                   Secondary Sediment Stations -- 8
                   -Collected in September

                   Secondary Surface Stations -- 30
                   -Collected from May through October

              Lab: Columbia

                   Primary Surface Stations -- 29
                   -Quarterly for metals, TOC, and phenols* -- February, May,
                     August, and November

    *Selected Stations

                                         -16-

                  -Annually for Pesticides -PCB's and other organics (selected
                    stations) -- March
                  -Annually for hardness (selected stations) --to coincide with
                    one of the metals samples

                  Primary Sediment Stations -- 18
                  -Collected in November

                  Secondary Sediment Stations -- 4
                  -Collected in September

                  Secondary Surface Stations -- 33
                  -Collected from May through October

             Lab: Florence

                  Primary Surface Stations -- 32
                  -Quarterly for metals, TOC, and phenols* -- February, May,
                    August, and November
                  -Annually for Pesticides - PCB's and other organics (selected
                    stations) -- April
                  -Annually for hardness (selected stations) --to coincide with
                    one of the metals samples

                  Primary Sediment Stations - - 22
                   -Collected in November

                  Secondary Sediment Stations - - 7
                   -Collected in September

                  Secondary Surface Stations -- 74
                   -Collected from May through October

              Lab: Greenville

                   Primary Surface Stations -- 31

                   -Quarterly for metals, TOC, and phenols* --January, April,
                    July, and October
                   -Annually for Pesticide -PCB's and other organics (selected
                     stations --May
                   -Annually for hardness (selected stations) --to coincide with
                    one of the metals samples

                   Primary Sediment Stations -- 20

                   -Collected in October

                   Secondary Sediment Stations --7

                   -Collected in September

                   Secondary Surface Stations --100

                   -Collected from May through October
    *Selected Stations

                                         -17-

             Lab: Lancaster

                  Primary Surface Stations -- 21

                  - Quarterly for metals, TOC, and phenols* -- March, June,
                     September, and December
                  - Annually for Pesticide - PCB's and other organics (selected
                     stations) -- March
                  - Annually for hardness (selected stations) -- to coincide
                     with one of the metals samples

                  Primary Sediment Stations -- 20

                  - Collected in October

                  Secondary Sediment Stations -- 13

                  - Collected in September

                  Secondary Surface Stations -- 77

                  - Collected from May through October

             Lab: Charleston

                  Primary Surface Stations -- 42

                  - Quarterly for metals, TOC, and phenols* -- January, April,
                     July, and October
                  - Annually for Pesticide - PCB's and other organics (selected
                     stations) -- May
                  - Annually for hardness  (selected stations) -- to coincide
                  with
                     one of the metals samples

                  Primary Sediment Stations -- 27

                  - Collected in December

                  Secondary Sediment Stations -- 11

                  - Collected in September

                  Secondary Surface Stations -- 42

                  - Collected from May through October

             Lab: Biological Services

                  Primary Sediment Stations -- 16

                  - Collected in March

    * Selected stations

    E.   Basic Water Monitorino Proaram (BWMP)

         Twenty-six of the S.C. Department of Health and Environmental
         Control primary trend monitoring stations have been designated as
         U.S. EPA National Basic Water Monitoring Program stations.  These
         stations are listed below:

         STATION NO.                    COUNTY               DISTRICT

            B-046                       Union                Catawba
            B-054                       Newberry             Central Midlands
            B-236                       Fairfield            Central Midlands
           BL-001                       Spartanburg          Appalachia II
            C-007                       Richland             Central Midlands
          CSB-001 L&R                   Richland             Central Midlands
         CSTL-109                       Hampton              Trident
         CSTL-098                       Beaufort             Trident
           CW-016                       Lancaster            Catawba
           CW-206                       Richland             Central Midlands
            E-008                       Orangeburg           Lower Savannah
            E-015                       Dorchester           Trident
            E-100                       Dorchester           Trident
           MD-048 *(MD-214)             Charleston           Trident
           MD-080 *(MD-213)             Georgetown           Pee Dee
          'PD-027                       Darlington           Pee Dee
           PD-028                       Darlington           Pee Dee
           PD-038                       Marion               Pee Dee
           PD-061                       Horry                Pee.Dee
           PD-202                       Sumter               Pee Dee
            S-125                       Laurens              Appalachia II
            S-018                       Greenville           Appalachia II
           ST-001                       Berkeley             Trident
           SV-118                       Allendale            Lower Savannah
           SV-323                       Aiken                Lower Savannah
           SV-291                       McCormick            Lower Savannah

         *Biological  Sampling cannot be conducted at these stations.   In
         parentheses  are the Trend  Biological  Monitoring  stations  where
         accompanying biological data are gathered (see Appendix C).

          Appendix A presents station descriptions.

                                     -19-

                 Parameter coverage and STORET parameter codes are:

                              Parameters SamDled Monthly

        Temperature          00010              Total phosphorus            00665
        Turbidity            00076              Ammonia                     00610
        Alkalinity           00410              Biological oxygen demand   00310
        Dissolved oxygen    00300               Total suspended solids      00530
        pH                   00400              TotaA organic carbon        00680
        Conductivity         00402              Flow                        00061
        Fecal coliform       31616 or 31615    SalinityC                    00480
        Total Kjeldahl       00625              TransparencyBIC             00078
          nitrogen                              Nitrate-Nitrite             00630

        A = Streams only
        B = Lakes and Impoundments only
        C = Estuaries only

                             Parameters Samoled Ouarterlv

                                     Heavy Metals

                              Parameters Samoled Annuallt

              Pesticides/PCB's
             Volatile Organics                       84085
              Base-Neutral Extractable Organics       45583
             Acid Extractable Organics               45582
              Trace organics and metals in sediment

              (See Section C, includes all Sediment Parameters Sampled Annually)

                              Parameters SamDled Annually

                   Representative fish/shellfish tissue analysis (.see following
                   Section and Appendix C)

    Parameter coverage at each station appears in Appendix B.

         F.   Bioloqical Monitorina

                   The biological monitoring network provides information which
              will allow for the detection and evaluation of changes in the
              biological  stability  of  aquatic  communities.   Data  collected
              through this program are also used to detect the presence and/or
              build-up of potentially hazardous substances in aquatic organisms.
              The various activities falling under the biological monitoring
              program are detailed below.

                                         -20-

      1. Fixed-Sta'tion Monitorinci - A program of long-term monitoring utilizing
        51 fixed biological monitoring stations distributed as follows-:

             26 EPA Basic Water Monitoring Program (BWMP) Stations

              9 Special Status Stations

             16 Estuarine Stations

        These stations are sampled at least annually for a variety of parameters
         (Table 2) to the extent that laboratory and manpower resources permit.
        Station location descriptions are presented in Appendix C while specific
        parameter coverage and sampling frequency information is listed in the
        appropriate following subsections.   Stations are selected according to
        the same criteria presented for the BWMP stations in Appendix A as well
        as according to these additional criteria:

             a.   At  locations  in  selected  major  water  bodies  potentially
                  subject to inputs of contaminants from areas of concentrated
                  urban, industrial, and/or agricultural use.

             b.   At locations in selected water bodies which are of critical
                  value for sensitive uses such as domestic water supply,-
                  recreation, propagation and maintenance of fish and wildlife.

             C.   At  locations  in selected  'areas  suited  to del iver  natural,
                  background water quality characteristics on a long-term basis.

             d.   At locations in selected areas where specific water quality
                  impairment has been documented with ameliorative procedures in
                  place to follow the response of the water system to those
                  procedures.

    2.   Toxic  Materials  Monitorinci  -  Uptake  and  concentration  by  aquatic
        organisms of toxic and potentially hazardous substances will be studied
        at trend  biological  monitoring  stations.   This  program will  also  be
        extended to areas of intensive surveys and/or special studies as
        dictated by the intent of the investigation.

    3.   Parameters  and Samolinci  Freauencv  - Parameter s sampled during  trend
        monitoring and intensive surveys are determined by the characteristics
        of the site  being sampled  or intent  of the  sampling  activity.   The
         parameters collected and the intended sampling frequency for each type
         of fixed-station biological monitoring activity is outlined below.
        Because of constraints on laboratory resources, prioritization of
         samples may preclude tissue analyses from' some of the annual trend
        network  collections.   The  51  stations  described  in Appendix  C  are
         sampled yearly. Parameters available for inclusion as well as frequency
         used in fixed-station biological monitoring are described in Table 2.

                                       Table 2

                    Fixed-Station Biological Monitoring Program
                Biological Community Coverage and Sampling Frequency

                 Station         Macro-       -
    Parameters   Status        invertebrate      Finfish    Crustacean   Shellfish

    Counts       BWMP                1             2
                 Special            1             2
                 Estuarine         3              2                           3

    Species      BWMP               1              2
     Ident.      Special            1              2
                 Estuarine         3              2                           3

    Toxic Sub-   BWMP                              2
    stances      Special                           2
                 Estuarine                        2             1             3

      1.  Each Station sampled once annually between June and August
      2. Each station sampled once annually between September and October
      3. Each station sampled once annually in March

                        a.   Macroinvertebrates - Quantitative collections will
                             be made  at  all  riverine  and  estuarine  stations
                             (Table  2).   Four  Hester-Dendy  samplers  will  be
                             exposed for Pour weeks at all  riverine  stations;
                             three 0.01 m  quadrats  will  be collected  at  all
                             estuarine stations.
                             Analyses to be conducted are:

                                  (i)  Identification to family, genus and/or
                                         species
                                 (ii) Counts
                                (iii) Size distributions of oysters at estuarine
                                         stations
                                 (iv) Community structure at estuarine stations

                        b.   Toxic Materials Monitoring Program - The species and
                             size requirements of individuals used in tissue
                             analyses along with the proposed number of tissue
                             analyses to be conducted are summarized in Tables 3
                             and 4.  A list of organic toxicants and inorganic
                             toxicants tested for in each type of animal, and the
                             sampling frequency are presented in Tables 5 and 6,
                             respectively. The sampling program for each type of
                             animal tissue is detailed in the following sub-
                             sections.

                                  (i) Finfish

                                  A.   One composite of five whole fish of the
                                       same species within a selected weight

                                         -22-

                                        class will be collected from each major
                                        trophic  level   (omnivores,   piscivores,
                                        insectivores) at each trend station (24
                                        BWMP   stations    and   special    status
                                        stations).

                                         Table 3

                    Fixed-Station Biological Monitoring Program Species
                         Requirements and Sample Size Restrictions
                                     for Tissue Analyses

       Tissue                                No. Individ.    Size/Weight
       Group                  Sample Type    in Sample        Restrictions   Preparation

    Finfish: omnivores         Composite          5              TBD*         Whole fish
             piscivores        Composite          5             TBD          Whole fish
             insectivores     Composite           5             TBD          Whole fish
             estuarine         Composite          5             TBD          Whole fish

    Crustaceans                Composite         30             >12.7 cm      Somatic
     (C. sapidus)                                               in width      muscle

    Shellfish                  Composite         30             >7.5 cm       Whole
     (C. virginica)                                             in height    Shucked

      * to be determined

                                          Table 4

                        Fixed-Station Biological Monitoring Program
                     Proposed Number of Tissue Analyses by Station Type

      Tissue                       Number of Samoles by Station TvDe                TOTAL
      Group               Riverine      Lacustrine     Estuarine      Off-Shore

     Finfish                75              21              4              1        101
     Crustaceans            --              --             16             --         16
     Shellfish              --              --             16             --         16

      TOTAL                 75              21             36              1        133

                                             -23-

                                       Table 5

                        Fixed-Station Biological Monitoring Program
                          Organic Chemical Parameter Coverage and
                      Proposed Sampling Frequency for Tissue Analysis

                                                         Tissue TyDe

    Chemical Group      Parameter              Finfish    Crustaceans    Shellfish

    Pesticides/PCBs   Aldrin (ug/kg)*              1           1              1
                      B-BHC (ug/kg)               1           1              1
                      Chlordane (ug/kg)           1            1             1
                      DDD (ug/kg)                 1           1              1
                      DDE (ug/kg)                 1 I 1
                      DDT (ug/kg)                 1            1             1
                      Dieldrin (ug/kg)            1           1              1
                      Endrin (ug/kg)              1           1              1
                      Heptachlor (ug/kg)          1           1              1
                      Heptachlor epoxide (ug/kg) 1            1              1
                      Hexachlorobenzene (ug/kg)  1            1              1
                      Lindane (ug/kg)             1           1              1
                      Methyoxychlor (ug/kg)       1           1              1
                      Toxaphene (ug/kg)           1            1             1
                      Diazinon (mg/kg)            1           1              1
                      Ethion (mg/kg)              1           1              1
                      Guthion (mg/kg)             1           1              1
                      Malathion (mg/kg)           1           1              1
                      Methyl parathion (mg/kg)   1            1              1
                      Parathion (mg/kg)           1           1              1
                      Ronnel (mg/kg)              1           1              1
                      a-BHC (mg/kg)               1           1              1
                      Mirex (mg/kg)               1           1              1
                      PCBs (mg/kg)                1           1              1

    Organic           Pesticides/PCBs              1           1              1
    Priority          Acid extractables            2           1              1
    Pollutants        Base-neutral extract-
                        ables                     2           1              1
                      Polynuclear aromatic
                        hydrocarbons              2           1              1

      1. analyses conducted annually
      2. analyses conducted biannually
      * ug/kg = parts per billion; mg/kg = parts per million, wet weight

                                           -24-

                                        Table 6

                       Fixed-Station Biological Monitoring Program
                        Inorganic Chemical Parameter Coverage and
                     Proposed Sampling Frequency for Tissue Analysis

                                                       Tissue Tvoe

    Chemical Group      Parameter               Finfish    Crustaceans    Shellfish

    Heavy Metals       Cadmium (mg/kg)*             1             1             1
                     Chromium (mg/kg)             1 I 1
                     Copper (mg/kg)       I                     1             1
                     Lead (mg/kg)                 1 I 1
                     Mercury (mg/kg)              I             1             1
                     Nickel (mg/kg)               I             1             1
                     Zinc (mg/kg)                 I             1             1

    Inorganic         Routine metals                1 I 1
    Priority          Beryllium (mg/kg)             2             1             1
    Pollutants        Silver (mg/kg)                2             1             1
                     Thallium (mg/kg)             2             1             1

      1. analyses conducted annually
      2. analyses conducted biannually
      * mg/kg = parts per million, wet weight

                                     Analyses will be conducted annually for
                                     heavy metals and pesticides/PCBs at all
                                      stations  and  biannually  for  priority
                                     pollutants. Such samples from Lake Marion
                                      (3 of the 9 special status stations) will
                                      be analyzed annually for all parameters.

                                 B.   One  composite  of  five  whole  flounder
                                     within a selected weight class will be
                                     collected from Charleston Harbor, Winyah
                                      Bay,  Port  Royal  Sound,  and  St.   Helena
                                      Sound. Analyses will be conducted annually
                                      for heavy metals and pesticides/PCBs and
                                      biannually for priority pollutants.

                                 C.   One composite of five whole pelagic fish
                                      of the same species within a selected
                                     weight  class  will  be  collected  from
                                      off-shore.  Analyses  will  be  conducted
                                      annually for heavy metals and pesticides/
                                      PCBs and biannually for priority pol-
                                      lutants.

                                        -25-

                            As appropriate, single or composite fillets of
                            large gamefish may be prepared for analyses
                            from any of these areas in addition to the
                            whole fish samples.

                 (ii) Shellfish

                       A.   One  composite  of  thirty  adult  (>7.5  cm  in
                            height) oysters (Crassostrea virginica) will be
                            collected from the mid-intertidal zone at 16
                            estuarine stations. Analyses will be conducted
                            annually for organic and inorganic priority
                            pollutants.

               (iii)   Crustaceans

                       A.   One composite  of  somatic muscle  tissue  from
                            thirty legally-harvestable (>12.7 cm in width)
                            blue  crabs   (Callinectes  sapidus)  will  be
                            collected at 16 estuarine stations. Analyses
                            will be conducted annually for organic and
                            inorganic priority pollutants.

                (iv)   Sediment

                       A.   One   sample  will   be  collected   from   the
                            approximate  top  3  cm  of  sediment  in  the
                            mid-intertidal  zone  at  16 estuarine  stations
                            where shellfish are collected. Analyses will be
                            conducted annually for organic and inorganic
                            priority pollutants.

    5.   Acute and Chronic Toxicity Assessment Proaram

             The Toxicity Assessment Program predicts the effects of
        wastewater discharges on aquatic life. Data collected through this
        program are also used to provide legally defensible data on damage
        in situations where compliance monitoring indicates violation of
        permits and/or water quality standards, and to provide information
        suitable for inclusion in the evaluation of permits issued under
        the NPDES discharge permit system. To accomplish these objectives
        the following test procedures may be utilized:

             (a)  Laboratory Bioassay - A static bioassay program which can
                  be utilized for both screening and definitive acute and
                  chronic toxicity testing.

             (b)  Mobile Bioassay - A mobile unit capable for use in both
                  dynamic and static bioassays. The major emphasis of the
                  unit will be on acute toxicity.

             (c)  Instream macroinvertebrate assessments.

                                   -26-

             Parameters and SamDlincj Freauencv

             Selection of wastes and dischargers utilized for toxicity testing
        will be closely coordinated with NPDES permitting program areas,
        compliance    monitoring    personnel,    enforcement    personnel    and
        district/laboratory personnel. Ten static chronic toxicity tests and 48
        static acute toxicity tests will be conducted this year.

    G.   Shellfish Monitorina

             Fixed-Monitorinq Network

                  The -state's coastal area is divided into 23 shellfish
             management  areas with  a total  of 361 monitoring  stations.   The
             purpose of this monitoring network is to provide data which
             accurately reflects the sanitary conditions of coastal shellfish
             and shellfish growing waters in South Carolina to insure that the
             health of shellfish consumers is protected.

                  The shellfish monitoring program provides the data base which
             is used in conducting a comprehensive evaluation of each shellfish
             growing  area.   These  evaluations,  or  sanitary  surveys,   are
             conducted every  three years with  annual  updates.   The data  are
             collected at strategically located sites and used to classify
             shellfish  waters  as to  harvesting  suitability.   The  monitoring
             network also serves to provide sanitary-related data from each
             shellfish  area  during  the  harvesting' season  to  ensure  th.at
             conditions which existed during the comprehensive evaluation still
             prevail;   that  the  harvest  classification  is  correct;   and,
             ultimately that shellfish are safe to be consumed by the public
             once harvested.  All shellfish waters receive one of the following
             harvest classifications:

                Approved:   Areas where  a sanitary  survey  indicates  that  the
                            water  is  not  contaminated  with  fecal  material,
                            pathogenic   microorganisms,    or   poisonous   and
                            deleterious substances in concentrations dangerous
                            to human health.  The fecal coliform MPN median in
                            approved waters does not exceed 14/100 ml and not
                            more than 10 percent of the samples exceed 43/100
                            ml.

          Conditionally      Areas generally of the same quality as approved
          Approved:          however, the quality may temporarily vary because of
                            sporadic impacts from non-point and point sources,
                            rainfall, or seasonal activities.  Shellfish may be
                            harvested for marketing under conditions specified
                            in a management plan.

               Restricted:  Areas where a sanitary survey indicates there is a
                            limited  degree  of  pollution  which  renders  the
                            shellfish   unsafe   for   direct   marketing.    The
                            shellfish  may  be  marketed   after  relaying  or
                            depuration.  The  median  fecal  coliform  levels  in
                            restricted waters are between 14/100 and 88/100 ml
                            with not more than 10 percent of the samples
                            exceeding 260/100 ml.

                                        -27-

               Prohibited:  Areas where a sanitary survey indicates excessive
                            concentrations of pollutants exist or where the
                            potential exists for excessive pollutant concen-
                            trations.   The median  fecal  coliform' MPN  exceeds
                            88/100 ml in the water or more than 10 percent of
                            the samples exceed 260/100 ml. Shellfish may not be
                            harvested from prohibited areas for human food use.
                            Closed  safety  zones  may  be  established  around
                            potential pollutant sources and are classified as
                            prohibited areas.

        All sampling procedures and laboratory analyses are conducted in
    accordance with the National Shellfish Sanitation Program (NSSP) 'guidelines.
    Areas closed to the harvesting of shellfish are posted with signs indicating
    the potential for serious illness from consuming shellfish harvested within
    these areas and outlining penalties for harvest violations.

        Sampling  stations  are  established  at  locations  representative  of
    variable  sanitary  water  quality  within  shellfish  areas.   Many  of  these
    locations are positioned at classification boundaries to confirm established
    harvesting classifications.  All 361 stations are sampled at least six times
    during the shellfish harvesting season, (S eptember 15 - May 15) (Table 7).
    Stations within waters that are classified conditionally approved are sampled
    monthly. There are also seven stations that are sampled six times during the
    season either on ebb or flood tide only.

        Complete descriptions of station locations are included in Appendix 0.

                                       Table 7

                    Fixed-Station Shellfish Monitoring Program
                  Physical and Bacteriological Parameter Coverage
                               and Sampling Frequency

    Parameter Group         Parameter               Water             Shellstock

        Physical           Tide Stage                 *                   NA
                           Water Temperature         *                    NA
                           Air Temperature           *                    NA
                           Wind Direction            *                    NA
                           Salinity                  *                    NA

        Bacteriological   Fecal Coliform              *                   **
                           Total Plate Count         NA                   **
                           E. coli                   **                   **
                           Sample Temperature        *                    **
                           Sample Type               NA                   **
                           Species                   NA                   **

      *Sampled at least six times during harvesting season.
     **Sampled as appropriate.

                                          -29-

    IV. INTE NSIVE SURVEYS AND SPECIAL WATER OUALITY STUDI'ES

        A.   Point Source Wasteload Allocations

             Intensive stream surveys are conducted for gathering field data for
             calibration or verification of water quality mathematical models
             and for the determination of the quality of the State's waters. It
             is the goal of the Department to calibrate models with measured
             field  data  when  issuing  point  source  wasteload  allocations
             requiring advanced treatment. Emphasis and priority will be placed
             on gathering field data for issuance of wasteload allocations for
             201 waste treatment  facility  projects.   Stream  surveys will  be
             designed and carried out as described in the Basic Water Monitoring
             Program.

             In addition to intensive stream surveys, time of travel studies to
             determine stream velocities for water quality model reaches will be
             conducted. These will be scheduled as needed and as resources allow
             for streams where data is lacking and complete surveys are not
             possible or feasible.

             Stream surveys are projected for a five-year period and each year
             revised as needed, prioritized, and then included in the State
             Program  Pl an.   Of these  projected  number of scheduled  facility
             surveys each year, the actual number performed for publicly owned
             facilities will be completed first with the remaining number of
             industrial and private facility surveys completed afterwards.  An
             effort will be made to complete all municipal surveys prior to
             permit issuance/reissuance.

             Intensive stream surveys will be performed generally during the
             warmer month~s  of May through  October.   Winter months  are  less
             desirable for intensive water quality surveys that are to be used
             for model calibration. This is based on the following factors:

              1.   Biochemical  reaction  rates  and  biological  populations  are
                  lowered by the colder temperatures.

             2.   Generally, the flow in the streams is higher than normal and
                  much less predictable.

             3.   Dissolved  oxygen  concentrations  are  higher  due  to  higher
                  saturation levels and lower temperatures.

             4.   For modelling  purposes,  it  is desirable  to conduct  field
                  studies which result in data closely aligned to the conditions
                  under which water quality predictions are made.  For example,
                  predictions are normally based on low stream flows (7Q10).

             5.   On those occasions where seasonal limits are at issue, studies
                  may be conducted during the winter months.

             Study plans for all intensive surveys are submitted to the State
             Quality Assurance Management Office (SQAMO) for approval prior to
             sampling.  All sampling and field analyses are performed according
             to Standard Operating~ and Quality Control Procedures for Ambient
             Water Quality and Wastewater Facility Monitoring (SCOHEC) and

                                        -30-

         Procedures  Manual   for  Stream  and  Wastewater  Faci lity  Flow
        Measurement (SCDHEC).

    B.   Soecial Water Ouality Studies

             Special water quality studies are conducted on an as needed
         basis to determine cause and effect relationships in water bodies
        where trend monitoring indicates a deterioration in environmental
         quality and to provide legally defensible data on damage in
         situations where compliance monitoring indicates violation of
         permits  and/or water  quality  standards.   Special  water  quality
         assessments are often requested for water bodies having high or
         potentially high public water us e values.

             Special  studies provide immediate and indepth investigations
         of specific environmental problems and involve practical research
        which leads to a better understanding of the water quality of the
         State of South Carolina.  Each study is followed by a report which
         analyzes the data obtained during the study.   These reports  are
         available to all interested parties.

             An investigation of specific environmental problems usually
         originates as an official request from other sections of EQC, such
         as Industrial Wastewater, Enforcement, the Modelling Section,
         District Services personnel, or Solid and Hazardous Waste. Studies
         may also be initiated in response to requests by private citizens
         or special interest groups.  Once an official request to carry out
         a specific  task  has  been  received,  the  special  studies  group
         designs, receives approval, and implements the study.  The results
         of such studies are reported primarily to the originator of the
         study request.

              In conducting practical research, the special studies group
         generally relies on its own staff, as well as the scientific staff
         of other sections of EQC.  The special studies staff designs and
         implements, or coordinates if other groups are involved, such
         studies and reports all findings to all interested parties.

              Study plans for any special studies are submitted to the State
         Quality Assurance Management Office (SQAMO) for approval prior to
         sampling. All sampling and field analyses are performed according to
         Standard Operating and Quality Control Procedures for Ambient Water
         Quality and Wastewater Facility Monitoring (SCDHEC) and Procedures
         Manual  for  Stream  and  Wastewater  Facility  Flow  Measurement
         (SCOHEC).

    C.   Lake Edgar A. Brown

              A special study to document the causative factors contributing
         to the eutrophic state of Lake Edgar A. Brown, a 100 acre system
         located within the town limits of Barnwell, South Carolina, was
         begun in May 1988.  The 18 month study is being jointly funded by
         EPA  and  SCDHEC  under  the  Clean  Lakes  Program.   Sampling  was
         conducted for one year, with semi-monthly collections during the
         growing  season  (April-October)  and monthly otherwise.   Following
         interpretation of th-e study results, a set of restoration alter-*

                                   -31-

             natives will be presented to those parties involved with lake
             stewardship.

                  A total of -three stations were sampled, two within the lake,
             and one on Turkey Creek. Turkey Creek does not presently flow into
             Lake Brown.   Flow was diverted in 1968 as part of an effort to
             control aquatic macrophytes.

             Parameters to be analyzed:

               Depth                        m
               Dissolved oxygen             mg/l              Water column profile
               Temperature                 �C                 Water column profile
               pH                           SU                Surface and bottom
               Specific conductance         umhos/cm          Surface and bottom
               Total ammonia                mg/l              Surface and bottom
               Nitrate-nitrite              mg/l              Surface and bottom
               Total Kjeldahl nitrogen      mg/l              Surface and bottom
               Total phosphorus             mg/l              Surface and bottom
               Total orthophosphorus        mg/l              Surface and bottom
               Dissolved orthophosphorus   mg/l               Surface and bottom
               Total alkalinity             mg/l              Surface and bottom
               Chlorophyll a                ug/l              Surface
               Secchi depth                 m
               Photic zone depth            m
                Extinction coefficent
                Phytoplankton enumeration   #/ml               Surface
                 and identification
                Fecal coliform               #/t00 ml          Surface
               Streamflow (Turkey Creek)   ft /sec

    D.   Clean Lakes Program

             South Carolina DHEC received a federal grant and conducted a lake
        classification  evaluation  during  1980-1981  entitled  "South  Carolina
        Clean  Lakes Classification  Survey,"  Technical  Report No.  019-82.   A
         final publication was submitted as part of the federal grant in 1982.
        This publication has been utilized by SCDHEC in making management
        decisions related to lakes in South Carolina, to provide information for
        305b reports, and to inform the public of the conditions in the lakes
         studied.

             SCDHEC has received a grant from EPA to update the Survey through a
         reassessment of all lakes during FY 1990, and to complete a report
        describing the trophic state of these lakes for inclusion in the 305b
         report.  The updated report will include comparisons of data collected
         from the larger lakes during FY 1980-81, FY 1985, and FY 1990, as well
         as the data from minor lakes collected during FY 1980-81 and FY 1990.
        The data will also be used to rank the lakes according to trophic
         condition.

              For ranking purposes, the seventeen (17) major public lakes of
         South Carolina will be considered in a separate grouping apart from the
         twenty-five (25) minor lakes addressed by this grant.  The seventeen
         (17) major lakes are listed below:

                                        -32-

        Lake William C. Bowen                   Lake Moultrie
        Clarks Hill Reservoir                   Lake Murray
        Fishing Creek Reservoir                 Parr Reservoir
        Lake Greenwood                          Lake Robinson
        Lake Hartwell                           Lake Richard B. Russell
        Lake Jocassee                           Lake Secession
        Lake Keowee                             Lake Wateree
        Lake Marion                             Lake Wylie
        Monticello Reservoir

    The remaining 25 public lakes are:

        Adams Mill Pond (Goodale St. Park)   Langley Pond (Horse Creek Pond)
        Ashwood Lake                           Lake Long
        Boyd Mill Pond                         Lake Oliphant
        Broadway Lake                          Prestwood Lake
        Lake Edgar A. Brown                    Reynolds Pond
        Lake Cherokee                          Rock and Cedar Creek Reservoir
        Chester State Park Lake                Saluda Lake
        Lake Conastee                          Lake Thicketty
        Lake Craig                             Vaucluse Pond
        Lake Cunningham                        Lake Wallace
        Eureka Lake                            Lake Warren
        Goose Creek Reservoir                  Lake Yonah
        Lake Johnson

         Parameter coverage will be similar for the sampling of both groups
    of public lakes.  Parameters to be measured and additional  information
    are given below:

           Parameter

           Dissolved oxygen                     Profile
           Temperature                          Profile
           Conductivity                         Surface and bottom
           pH                                   Surface
           Secchi Depth
           Photic Zone Depth
           Chlorophyll a                        Surface
           Algal Growth Potential               Headwaters and coves only
           Total Kjeldahl Nitrogen              Depth-integrated
           Ammonia                              Depth-integrated
           Nitrate-Nitrite                      Depth-integrated
           Total phosphorus                     Depth-integrated
           Orthophosphorus                      Depth-integrated
           Dissolved orthophosphorus            Depth-integrated

         Quarterly sampling will  be completed during FY 1990.  During  FY
    1990-91, collected data will be used to compute two or more trophic
    state indices.  These indices will be used to rank the lakes based on
    water quality and public use criteria.

                                     -33-

    V.   WASTEWATER DISCHARGE COMPLIANCE MONITORING

             All wastewater dischargers to the surface waters of the State of
        South Carolina must obtain a National Pollutant Discharge Elimination
        System (NPDES) Permit to discharge.   This applies to all  public and
        privately owned wastewater treatment facilities. The NPDES permit sets
        limits for physical and chemical characteristics of the facility
        effluent to protect the water quality of the receiving waterbody.  A
        number of publicly owned treatment works (POTWs) have requirements in
        their NPDES permits to implement an approved pretreatment program, as
        well.

             The purpose of the facility monitoring program is to insure that
        permitted effluent limitations are met and properly reported to the
        State, to insure proper operation and maintenance of wastewater
        treatment facilities, and to insure that the public's concerns and
        complaints concerning wastewater dischargers are answered effectively.
        This monitoring function encompasses the review of NPDES permit
        compliance schedules, review of NPDES self-monitoring data, .inspection
        and evaluation of wastewater treatment facilities, collection and
        analysis   of   samples   at   wastewater   treatment   facilities,   and
         investigation of complaints concerning wastewater treatment facilities
        or stream quality throughout the State.

             The information gathered by the facility monitoring program is used
        by the State and EPA to determine permit compliance and to support
        enforcement  actions.   Inspection  results  are  also  useful  in  grant
        reviews and permitting functions. Facility monitoring is often included
         in water quality assessments as well.

             Certain inspections are used to improve permittee performance
        through improved data quality and the provision of technical assistance.
        Of course, the facility monitoring program also serves to maintain a
        regulatory presence in the State.

             The following sections detail the various means at our disposal to
        accomplish these goals.

        A.   Comoliance Schedule Trackinci

                  Schedules of Compliance for permits and administrative orders
             are maintained in a data file designated as the Permit Compliance
             System or PCS.  This program was originally developed by EPA to
             track permit compliance and the State has assumed responsibility
             for maintaining and updating the file's data base. The Enforcement
             Section receives a' PCS Quick Look Report containing scheduled
             compliance dates  on a monthly basis.   These dates  are compared
             against actual compliance status. Achieved compliance is noted and
             noncompliance situations are suspended for further action by the
             enforcement staff; also, any amendments to compliance dates are
             input into the system.

                                       -34-

    B.   NPDES Self-Monitorinq

             All  NPDES  permittees  are  required  to  collect  and  analyze
        samples of their own effluent at regular intervals for specific
        permit  parameters.   Self-monitoring data is transmitted  to  the
         Enforcement Section by the permittee in the form of a Discharge
        Monitoring Report (DMR).

             Enforcement Monitoring Records are utilized to track NPDES
        self-monitoring information. For NPDES self-monitoring this system
         is utilized to assure timely submission by dischargers of DMRs and
        recording of reported values by effluent parameter for each NPDES
        permit. DMR files are reviewed on a monthly basis to determine
         appropriate enforcement action required for failing to submit dis-
         harge   monitoring   reports   and/or   for   significant   effluent
         violations.   In addition,  permittees normally  submit  reports  of
        noncompliance covering significant effluent violations as they
        occur. These non-compliance reports, submitted in advance of DMRs,
         provide DHEC the opportunity to determine if there may be effluent
         problems  requiring  immediate  investigations.   After being logged
         and reviewed, all DMR's are sent to the Enforcement Section to be
         placed in PCS and then in the NPDES file for the particular
         facility to provide a readily available source of effluent data.

    C.   Federal Comoliance Evaluation Insoections - (CEI)

             The Compliance Evaluation Inspection (CEI) is a nonsampling
         inspection designed to verify permittee compliance with applicable
         permit self-monitoring requirements and compliance schedules. This
         inspection is based on record reviews and visual observations and
         evaluations of the treatment facilities, effluents, receiving
        waters, etc. The CEI is used for both chemical and biological
         self-monitoring programs.

             During FY'89, CEIs will be performed on Publicly Owned Treat-
         ment Works (POTWs) only. Inspections of these municipal facilities
         are assigned the following priorities:

              1.   Completed PL 92-500 facilities (federally funded)

              2.   POTWs with Municipal Compliance Plan (MCP) or a Composite
                  Correction Plan (CCP)

              3.   Major municipals

             4.   Minor municipals

         The Insoection

             The inspection is comprised of an evaluation of the physical
         equipment, laboratory records, discharge monitoring reports, and
         the  operational  records  of the  facility.   The  results  of  the
         inspection are reported on the EPA Form 3560-3.  A two or three
         page narrative report summarizing the findings in each of 8 major
         areas evaluated

                                      -35-

    during the inspection is attached to the 3560-3 form. The 8 major
    areas evaluated are as follows:

         a.   Permit  Verification  - verification  of  name,  address,
             discharges), receiving waters, etc., contained in the
             permit.

         b.   Records and Reports - determination of compliance with
              recordkeeping and reporting requirements stipulated in
              the permit.

        C.   Facility  Site  Review  - examination  of  areas  on  the
              permittee's premises where pollutants are generated,
             pumped, conveyed, treated, stored or disposed.
        d.   Flow Measurement - installation, calibration and accuracy
             of flow measurement system is determined.

         e.   Compliance Schedules - where applicable.

         f.   Self-Monitoring  Program  - sampling  frequency,  type(s),
             parameters monitored, parameter limitations, samp]ling
             methodology are examined for compliance with permit.

        g.   Operation and Maintenance - a visual  inspection of unit
              processes is conducted.
         h.   Sludge Disposal - the permittee's sludge management and
             disposal methods are evaluated.

    Procedure

         The   accepted   procedure   for  conducting   the   Compliance
    Evaluation Inspection is as follows:

         a.   The facility evaluator notifies the permittee prior to
              the CHI by telephone.   The permittee  is instructed to
              have available all pertinent records for review.

         b.   The  evaluator  completely  fills  out  the  appropriate
              checklists for each major section evaluated during the
              inspection.

         C.   After completion and review of the inspection report, the
             completed form 3560-3, narrative report, and checklists
             are forwarded to the Facilities Compliance Section for
             review and distribution.

    Fol low-up

         Follow-up evaluations will be made on deficiencies noted in
    initial  Compliance  Evaluation  Inspections.   The follow-up  is as
    foll1ows:

         a.   A letter emphasizing the deficiencies noted will be sent

                              -36-

                  along with the initial report to the owner. This letter
                  will point out problems found during the inspection and
                  request corrections or plans for corrections. This letter
                  requires a response within thirty (30) days.  Responses
                  are forwarded to the District and to the Central files
                  when received and reviewed.

             b.   A memorandum accompanies a copy of the response in the
                  District requesting the initiation of a follow-up field
                  inspection.   The  actual  follow-up  evaluation  can  be
                  comprised of a routine state operation and maintenance
                  inspection with the emphasis placed on the status of
                  necessary corrective actions to problems noted in the
                  Compliance Evaluation Inspection report.

             C.   If corrective action on the initially noted deficiencies
                  has not been taken, the District should follow the
                  Enforcement Procedures for Federal Compliance Evaluation
                  Inspections until compliance is achieved.

             d.   In many cases long  range plans  to solve problems  are
                  accepted   is   reasonable   justification   of   certain
                  deficiencies. In some cases active 201 participation is
                  the most reasonable solution to present problems.

    D.   State Ooeration and Maintenance Insoections

             These evaluations are .designed to insure that wastewater
        treatment facilities are being properly maintained and operated in
        accordance with State and Federal regulations,'such as NPOES permit
        schedules and accepted maintenance procedures.

             The State Operation and Maintenance Program involves two types
        of inspections:  routine and follow-up inspections.  The State O&M
         inspections are the periodic inspections performed on each
        wastewater treatment facility in the State.  Follow-up inspections
         are the inspections in which the evaluator returns to the facility
        to determine if the deficiencies noted in a previous inspection or
         follow-up letter have been corrected.

             The State 0 & M inspections involve the actual visit to the
         treatment plant site and visual inspection of the facility. The
         inspector determines if the facility and the equipment involved are
         properly maintained  and operated.   Certain  limited  physical  and
         chemical tests are run on the effluent to help the evaluator
        determine the plant's efficiency and effectiveness of operation.

                                      -37-

        The following parameters are collected:

                       Effl uent

                       Temperature
                       pH
                       Dissolved oxygen
                       Chlorine residual

        The  inspection  program  is  not  a totally  regulatory  program.   The
    inspectors  provide  technical  assistance to operators  with  regard  to the
    proper operation  and maintenance of wastewater treatment facilities.   The
    inspection results are discussed with the operator, when possible, to let him
    know what corrective measures, if any, are needed.

         Procedure

             The following is the procedure followed for completing a routine
         facility evaluation:
          1.   Plan work schedule ahead of visits.

          2.  Review  file  (for  previous  evaluations,   inspections,   orders,
              Enforcement  action,  etc.)  and  make  notes  of  items  which  were
              unsatisfactory on previous visits and carry file or parts needed.

         3.   Review the permit completely.

          4.  Inform appropriate person (immediate supervisor) of your planned
              daily visits.

          5.  Make every effort possible to contact owner or operator of the
              facility to be evaluated to inform him of inspection plans. The
              owner or operator is expected to accompany the evaluator during the
              evaluation.

          6.  If you are unable to contact owner or operator, obtain access and
              permission to evaluate facility.

          7.  Make appropriate observations and field tests to determine which
              processes  are  satisfactory  or  unsatisfactory.    The  facility
              evaluator must make observations and tests as indicated on the
              evaluation forms. Effluent tests are mandatory.

          8.  If  the  facility  has  records  of  O&M,  check  records  and  make
              comments.

          9.  Reports must be completely filled out and signed by person making
              evaluation.    Make   appropriate   remarks   and   recommendations.
              Deficiencies  should  be listed  in remarks  section  of  inspection
              form.

         10.  Record name of person you contacted.  Have him-sign inspection form
             when possible.

                                         -38-

        11. Inform the owner or operator of findings and ask him to make any
             needed corrections.

        12.  Those  facilities  found  to  require  a  follow-up  visit  must  be
             scheduled and followed up at the specific time.  Plan for follow-up
             should be stated on inspection form.

        13. Dissolved oxygen, temperature and pH should be run on the stream
             above and below the facility discharge when observations indicate
             possible problem.

        14. If samples are collected for laboratory analysis, coordination
             should be made with laboratory and results should be included with
             evaluation report.

        15. If facility is not operated by a properly certified operator, this
             should be indicated on the evaluation report.  Appropriate action
             should be initiated by the District Director to insure action is
             taken to retain an operator of the appropriate grade.

             The inspector's reports are reviewed in the district before the
        copies  are distributed.   One copy of the  inspection  is sent to the
        facility owner, one copy to the operator, one copy is kept in the
        district office, and the original is sent to Central Office to be
        reviewed,  logged and sent to the Central  Files.   With every routine
        inspection, an update is made to the Carolina File Wastewater Inventory
        List. Inspection results are entered in PCS.

             Suspense files on problem facilities should be maintained in the
        District Office.   The facility evaluators should also keep a list of
        facilities which need to be sampled for possible enforcement action.
        Those lists should be forwarded to the regional monitoring supervisor
        periodically to be scheduled for sampling.

             Follow-up inspections are a result of inadequacies being found
        during a State O&M inspection.  If the follow-up inspections show that
        the inadequacies have not been corrected and the district staff has
        exhausted its resources in getting the facility in proper operational
        condition, then all necessary information concerning the facility can be
        addressed at a meeting at the District level. Enforcement action should
        follow the enforcement procedures for State O&M Inspections until
        compliance is achieved.

    E.   Comoliance Samolincq Insoections

             Compliance sampling inspections are performed to determine if
        wastewater treatment facilities are operating as permitted and designed,
        to collect data for comparison with self-monitoring data, and to support
        enforcement action.

        Sampling  of  facilities  are  assigned  the  following  priorities:

             1.   Federal Compliance Sampling Inspections.
             2.   Enforcement Section o~r EPA requests.
             3.   Engineering Division request.
             4.   District personnel request.
             S.   Routine sampling.

                                        -39-

    Federal Comoliance Samolina Insnections

        Federal Compliance Sampling Inspections are conducted on all major
    dischargers and specific minor dischargers on an annual basis. The
    Federal Compliance Sampling Inspection requires that an inspection of
    the facility be conducted by the EQC district facility evaluator. This
    inspection is to be made an one of the three (3) days required for
    effluent sampling.  The information gathered during this inspection is
    reported on the EPA Form 3560-3.  A list of the dischargers receiving
    Federal Compliance Sampling Inspections for each EQC district appears in
    Appendix E.

        A detailed inspection of the facility's records, regular operation
    and  maintenance,   flow  measurement  devices,   sampling  procedures,
    laboratory, and other permit conditions for compliance verification is
    conducted by the district facility evaluator.  If any deficiencies are
    found  which  can  be  corrected  with  little  or  no  expense  to  the
    responsible facility officials, a notice of deficiency is issued to the
    facility official.  This official  is allowed ten (10) working days to
    respond  to the deficiencies  noted.   If at the -end  of ten  days  no
    response has been acknowledged, the facility evaluator should so state
    in his report for possible enforcement action. Effluent sampling is
    included in the Federal Compliance Sampling Inspection. Procedures for
    sampling the effluent are the same as discussed below for routine State
    Compliance Sampling Inspections.

        After the sampling and inspection has been completed, the
    laboratory results are mailed to the Analytical Services Division.  The
    3560 form, checklists, 'and narrative report are mailed to the Facilities
    Compliance Section. All.data should be completed and mailed to Columbia
    within two weeks of completion of sampling.

    Reauested Samolina InsDections

        Upon receiving a request for compliance sampling, a review of
    historical data and the NPDES permit regulations for the facility is
    conducted to determine if previous sampling data will be sufficient. If
    additional sampling is needed, a request, including all parameters
    desired is sent to the District Office responsible for sampling that
    facility.   This  is coordinated  by personnel  in  the  Central  Office
    Facilities Compliance Section.  A written request for the sampling is
    then made to the District monitoring supervisor. Sampling and reporting
    procedures are the same as for routine State Compliance Sampling
    Inspections. (see below)

    Routine State Comoliance Samolinci Inspections

        Routine state compliance sampling inspections are set up by the
    District monitoring supervisor.  A schedule of facilities to be sampled
    is sent to the Facilities Compliance Section. It is a requirement that
    a monthly schedule of expected facility sampling be sent to the Central
    Office.

        All routine state compliance sampling inspections require two days
    of sample  collections.   The set-up  of flow recorders  and  automatic
    samplers is accomplished on an initial sampling day. The samples are

                                   -40-

        collected from the automatic sampler on two consecutive days of the
        sampling period  and  taken to the  District. laboratory  for  analyses.
        Samples are collected according to the NPDES permit requirements and
        SCDHEC's Standard O~eratina and Quality Control Procedures for Ambient
        Water Quality and Wastewater Facility Monitorinc (SCDHEC) and Procedures
        Manual for Stream and Wastewater Facility Flow Measurement (SCDHEC).

             After completion of the sample analyses the laboratory data sheets
        are sent to the Analytical Services Division which forwards them to the
        Facilities Compliance Section to be verified, reviewed and logged in.
        The data then goes to the Data Systems Management Section for processing
        and keypunching.
             After keypunching, the data is edited and a compliance monitoring
        report is generated. The data is compared with the NPDES permit limits
        to determine if any permit violations occurred. A formal report is then
        compiled by Facilities Compliance Section personnel and sent to the
        responsible facility official.  Copies are transmitted to the Central
        Office files, the District, and EPA (majors). A written response to the
        agency for any significant permit violation is usually requested.

             Follow-up inspections are conducted on deficiencies noted in the
        CSI as outlined under the CEI section.
    F.   Performance Audit Inspections
             The Performance Audit Inspection (PAI) is used to evaluate a
        permittee's self-monitoring program.  The purpose of the inspection is
        not only to determine the quality of self-monitoring but also to assess
        the  reliability  of  the  data  reported  by  the  permittee.   A  field
        evaluation is conducted which includes an evaluation of flow measure-
        ment,  sampling,  records,  and  operation  and maintenance.   Facilities
        Compliance Section personnel perform this part of the PAI. A laboratory
        evaluation  is also  conducted which  includes  a review  of analytical
        methods  and  procedures,  sample  handling  and  preservation,  quality
        assurance,  and  records.   The  EQC  Laboratory  Certification  Section
        performs this part of the PAI.
             The State routinely performs twelve (12) PAIs annually. Others may
        be performed as necessary.   EPA also conducts a number of PAls in the
        State each year.
    G.   Technical and/or Diaanostic Evaluations
             The technical  and/or diagnostic evaluation  focuses  primarily  on
        wastewater treatment facilities that are not in compliance with their
        permit requirements.   The purpose of the evaluation can be to either
        evaluate causes of non-compliance in support of enforcement actions or
        to  assist  those  facilities  without  self-diagnostic  capability.   The
        evaluation identifies major plant deficiencies in operation, design,
        and/or construction.  Other aspects of the permit  program such as the
        permittee's self-monitoring program can be included in the technical
        evaluation if deemed necessary.
             EQC conducts a minimum of twelve (12) technical and/or diagnostic
        evaluations annually.
                                        -41-

    H.   Pretreatment Proaram Audit and/or Insoection

             The pretreatment program audit and/or inspection is conducted
        annually on those publicly owned treatment works (POTWs) that are
        required by~ regulation to have an approved pretreatment program.   The
        purpose of the audit and/or inspection is to determine whether the
        program is being adequately implemented by the POTW.  The audit would
         include a review of the following items:

             1.   P01W treatment facility background information.

             2.   PONW pretreatment program background information.

             3.   Evaluation of PONW pretreatment program changes.

             4.   Legal authority evaluation.

             5.   Application of pretreatment standards.

             6.   Compliance Monitoring and Enforcement - POTW personnel.

             7.   Compliance Monitoring and Enforcement - industrial user file
                  review.

             S.   Data management and public participation.

             9.   Program resources review.

              EQC conducts either a pretreatment program audit or pretreatment
         compliance inspection at least annually on each PONW required to have a
         pretreatment program.

             The pretreatment program audits are conducted at each PONW facility
         whose  permit  expires  in  the  forthcoming  year.   The  pretreatment
         compliance inspections are performed on all other POIW's in the same
         year.

              Industrial user inspections and tours of the facilities are
         included in the audit procedures.. A report of the findings is forwarded
         to the P01W for corrective actions where appropriate.

             The pretreatment program audits and/or inspections are being
         conducted by personnel of the Facilities Compliance Section, Central
         Office.

                                        -42-

    VI. OUALITY ASSURANCE/OUALITY CONTROL PROCEDURES

             It is the policy of Environmental Quality Control (EQC) that neces-
        sary quality assurance (QA) activities be conducted within the State of
        South Carolina to demonstrate that all environmental data generated,
        processed, or used will be scientifically valid, defensible, and of
        known and acceptable precision and accuracy.  It is also the policy of
        EQC that all reported data will include documented precision and
        accuracy and be complete, representative, and comparable.  The quality
        of all data generated shall meet or exceed all EQC and EPA program
        requi rements.

             The Deputy Commissioner for Environmental Quality Control has the
        overall   responsibility   for  the  development,   implementation,   and
        continued operation of EQC's QA Program. To insure that EQC's QA policy
         is  uniformly  applied  to  the  generating  and  processing  of  all
        environmental data, a State Quality Assurance Management Office (SQAMO)
        has been established.

             This office is responsible for the Environmental Quality Control
        Assurance Program.  Environmentally-related measurement activities con-
        ducted by or for EQC shall be done only with the approval of the State
        Quality Assurance Management Office (SQAMO) after assuring that adequate
        quality assurance guidelines and procedures have been incorporated.
        This  includes  study-planning,  sample  collection,  preservation  and
         analysis, data handling, and use of physical, chemical, biological, and
        other data related to the effects, sources, transport and control of
        pollution, as well as personnel review and training.

           To accomplish these goals the Water Quality Monitoring Section and
         Facilities Compliance Section have developed and instituted SQAMO
         approved field study procedures and documentation, and data review in
         addition to participating in the laboratory certification program and
         routine EPA operating overview. Some specifics of these Sections'
        QA/QC activities include:

         1.   Submission of all study plans to SQAMO for review and approval
             prior to implementation.

         2.   Use of bound field logbooks by all monitoring and facility evalua-
             tion personnel.  In these logbooks are recorded all of the routine
             daily meter calibration results, remarks and notes relating to all
             activities, and values for all field measured parameters as well 'as
             time, date, station location, and collector identification informa-
             tion associated with all sampling activities.  This logbook format
             provides a legally admissible document for any court supervised
             compliance/enforcement proceedings.

        3.   Regular reviews  and updates  of SCDHEC's Standard Operating  and
             Quality Control Procedures for Ambient Water Quality and Wastewater
             Facility Monitoring (SOP), Procedures Manual for Stream and Waste-
             water Facility Flow Measurement, and Standard Operating and Quality
             Assurance  Procedures  for  Biological  Services.   These  documents
             describe in detail the field sampling procedures, meter calibration
             and maintenance procedures, sample chain-of-custody documentation,

                                       -43-

        sample preservation, holding times and recommended sample containers
        specifications, data sheet examples, and data submission requirements.

    4.   At least twice yearly all field personnel  are accompanied on sample
        collection activities by the quality assurance officer for evaluation of
        adherence to standard operating procedures (SOP) for QA/QC. These
        evaluations each year are for water quality monitoring SOP review and
        for facility compliance sampling SOP review.

    5.   Approximately  every  other  year  the  EPA  conducts  on-site  routine
        overviews of SCDHEC's QA/QC procedures.

    6.   Water Quality Monitoring Section personnel participate in the laboratory
        certification program by assisting in the laboratory reviews conducted
        every three years (see subsequent section for a discussion of this
        program).

    7.   Data checking and editing is performed on data by the quality assurance
        officer after data punching but before final submission to the EPA
        STORET system. The STORET system performs additional data checks, and
         any errors reported are rechecked by the QA officer.

                                        -44-

    VII. EMERGENCY RESPONSE

             The Emergency Response Section, now part of the Bureau of Solid and
         Hazardous Waste Management, was established to respond to and coordinate
        emergency activities for all Office of Environmental Quality Control
        emergencies. The Emergency Response Section has the responsibility for
        emergencies related to water, air, drinking water, solid waste, waste-
        water, etc.

        A.   Soill Resoonse Team

                  Data collected during a spill investigation is for the dual
              purposes of establishing the spiller, if unknown, and as a means of
             measuring the actual or potential environmental damage caused by
              the spill. In this manner, the Department meets its directives of
              Section 48-1-50, Subparagraph 21 of the South Carolina Code of Laws
             which directs the Department to "establish the cause, extent, and
              origin of damages from waste including damages to the fish, water-
              fowl, and other aquatic animals and public property which result
              from the discharge of waste to the waters of the State."

                  To encourage industry and transportation to minimize or elimi-
              nate spills, a State Contingency Plan for oil and hazardous
             materials  has  been  developed.   This  plan  was  approved  by  the
              Department of Health and Environmental Control Board.  Copies have
              been distributed to the following:

                            Fire Departments

                            Law Enforcement

                            Civil Defense Agencies

                            S.C. Highway Department

                            S.C. Highway Patrol

                             Industrial Section Sector

                            Oil Jobbers

                            Miscellaneous

                            Engineering Firms and
                            Interested Citizens
                            Other Governmental Agencies

                  This contingency plan is reviewed and updated every three (3)
             years,  or  more  frequently  if needed.   We  anticipate  that  the
              updated contingency plan will be reissued by late spring of 1990.

                  A twenty-four hour telephone number has been established to
              facilitate spill reporting.  The number~is 253-6488., Between 8:30
             A.M. and 5:00 P.M. this number is manned by personnel in Emergency

                                        -45-

        Response, after 5:00 P.M., an answering service intercepts all calls,
        then contacts the person who i s on callI to respond to the spill.I Many
        spills are reported through this number and greater emphasis will be
        placed on the reporting of all spills.

             A spill response team has been established in each of the State's
        twelve districts.   This has enhanced response time and provides  for
        better   local   coordination   through   on-scene   coordinators   (OSC).
        Additional  training  sessions  will  be  held  in  each  of  the  twelve
        districts during FY'89. Each district office has at least one copy of a
        procedures manual and two reference manuals involving spills of oil and
        hazardous material s.

             The Emergency Response Section utilizes a computer system known as
        OHMTADS (Oil and Hazardous Material Technical Assistance Data System).
        This system is designed as a source of information and technical
        assistance which can be utilized during a serious spill situation. The
         information obtained can be relayed from the Central Office to the OSC
         in the field.  A portable OHMTADS terminal telephone coupler apparatus
         i s availIabl e for use at the scene of a spill I. Access to Hazardline is
        also available as a source of additional information not available
        through OHMTADS.

             To encourage the development of a local contingency plan and mutual
        assistance groups, meetings have taken place with local governmental
         agencies  (such  as  civil  defense)  and  industries  to  develop  spill
        cooperatives and response assistance groups.

             To coordinate response activities with other governmental agencies
        we work very closely with the Environmental Protection Agency, the
        United States Coast Guard, South Carolina Department of Highway and
         Public Transportation, South Carolina Water Resources Commission, the
        Emergency Preparedness Division of the South Carolina Adjutant General's
        Office, and South Carolina Wildlife and Marine Resources in the
        reporting and cleaning up of spills.  This cooperation is necessary to
        provide for efficient, coordinated and effective action in minimizing
        damage from oil and hazardous substances.  In addition, information is
        coordinated through other Department of Health and Environmental Control
        bureaus such as air, wastewater, water hygiene and special environmental
        programs.   Spill  data  is also utilized by other Bureaus  within  the
        Department  for  enforcement   actions,   by  concerned   citizens   for
         information collection, and frequently reviewed by attorneys during case
        preparation.

    B.   Soill Prevention Control and Countermeasures (SPCC)

             To prevent the discharge of oil from non-transportation related
        onshore and offshore facilities into or upon the navigable waters of the
        United States we will randomly investigate facilities to determine if
        SPCC plans have been prepared and if key personnel are aware of and
        understand  the  plan.   These  investigations  will  be  conducted  both
        singularly and collectively with E.P.A. Region IV personnel on all
        non-transportation related onshore-and offshore facilities, which due to
        their location, could reasonably be expected to'discharge oil in harmful
        quantities, as defined in Part 110 of 40 CFR.

                                       -46-

             The regulation is very specific for the preparation and imple-
        mentation of Spill  Prevention  Control  and Countermeasure  Plans.   For
        existing facilities, either onshore or offshore, the preparation date
        was July 10, 1974, and the implementation date was January 11, 1975.
        Anyone who has more t~han one tank above the ground whose aggregate
        capacities are greater" than 1,320 gallons, or any single tank whose
        capacity is greater than 660 gallons, must have a SPCC plan fully
         implemented.   For  tanks  that  are  buried  and  whose  capacities  or
        aggregate capacities are greater than 42,000 gallons, the identical
        requirements exist. Tanks with lesser volumes, either above the ground
        or buried, are exempt from this requirement.  A fully implemented plan
         is one which sets forth in detail how a spill can be prevented, how a
        spill will be handled once it occurs, and the emergency procedures to be
        followed.   The  plan  -must  be  in  accordance  with  good  engineering
        practices and certified by a registered professional engineer. The plan
        must be kept at the facility to which it pertains if the facility is
        manned for eight (8) hours a day, or at the nearest field office if
        subject  facility  is not manned.   Plans must  be updated  every  three
        years. A certain amount of effort will be devoted to the reinspection of
        some facilities.

    C.   Fish Kill Prociram

             Fish kill data is collected for the purpose of assisting in the
        determination of the cause of the kill. Data collected is used to help
        establish   such   trends   as   mismanagement   of   pesticide/herbicide
        application, pollution sources (both point and non-point) and natural
        phenomenons resulting in environmental  stress.  The fish kill data is
        available for use by other bureau's in assessing any environmentally
        sensitive areas, by interested citizens, and fellow agencies such as the
        South Carolina Department of Wildlife and Marine Resources.

             Fish mortalities result from a variety of causes, some of natural
        origin  and  some  man-induced.   It  is  recognized  that  speed  is  all-
         important  in the  initial  phases  of  an  investigation.   Therefore,  a
        twenty-four hour telephone number has been established for the report of
        fish kills.  The number is 253-6488.  Between 8:30 a.m. and 5:00 p.m.
        this number is manned by personnel of the Emergency Response Section.
        After 5:00 p.m., the answering service intercepts all calls, and then
        contacts the person from the Emergency Response Section who is on call.

             All fish kills should be reported initially to the Emergency
        Response Section via the 24-hour telephone number.  The report should
        come to this number even if the district office is first notified of the
        kill. The Emergency Response Section will assist in co-ordinating and
        dispatching field investigators to the site of the fish kill.

             Once a kill is reported, a team of specially trained individuals is
        dispatched to the site. Since there is always the possibility of legal
        liability associated with a kill, a carefully developed field procedure
        is available for immediate activation.

                                        -47-

        When a kill report is received' maps of the area to be investigated are
        consulted to determine the best access points, and to locate known
        industrial, municipal, and other potential sources of pollution.

             A fish kill response team has been established in each of the
        State's twelv'e DHEC districts.  This has enhanced our response time and
        provided for better local co-ordination through district personnel.  We
        have assembled a standard fish kill kit.  Sixty complete fish kill kits
        have been distributed among the Central and twelve district offices.
        Each kit consists of the following:   ice chest,  specimen containers,
        bacteri olog ical,  biological,  and  chemical   samples  containers  and
        preservatives.   In conjunction with  the above,  an updated  procedure
        manual has been distributed to each District Office as well as the South
        Carolina Wildlife and Marine Resources.   Fish kill  training  seminars
        have been conducted to broaden the knowledge of the investigators and
        the scope of the investigations.

             Whenever public waters are involved, DHEC investigators should
        contact an official of the S.C. Wildlife and Marine Resources Division
        to co-ordinate fish kill investigations between the two departments. The
        fisheries'  biologist  should be contacted  if possible.   If he is not
        available, a member of the law enforcement division should be called.
        It should be noted that the Wildlife Division is restricted to
        freshwater fish kills, and the Marine Resources Division restricts
        itself to the investigation of fish kills  in saline waters.   Marine
        Resources Division is located in Charleston, South Carolina.

             The extent of investigation of a given fish kill lies in the extent
        of the kill, the numbers and kinds of fish involved, and the resources
        available for the investigation.   Following a decision to investigate,
        the investigation should continue until a cause is determined, or until
        all known potential causes have been eliminated as being implicated in
        the kill.

             Analytical Services Division laboratories analyze all of the
        samples collected on fish kill investigations except for biological
        samples. They are alerted and given an estimate of the number and kinds
        of samples, and date of arrival.

             If the cause of a kill can 'be determined to be man induced, a-
        report is submitted to the Division of Water Quality Assessment and
        Enforcement of the Department of Health and Environmental Control for
        enforcement action.  If the cause of a kill cannot be determined after
         investigation of all possible sources, then the Department of Health and
        Environmental Control will inform these possible sources that a kill has
        occurred and that the Department of Health and Environmental Control
        will ask them to investigate further and determine if a spill may have
        occurred accidentally which could have caused the kill.

    D.   Technical Assistance

             With the promulgation of the hazardous material regulations, there
         is a definite need for additional training.  Training is needed in the
        following areas: chemical identification, personnel protection during

                                        -48-

    spill  investigations,  spill  investigations,  reporting  techniques  and
    data collection.

        We are currently developing an in-house training course to
    encompass the areas of operation/maintenance of hazardous atmosphere
    monitoring   equipment,   response   safety,   and   containment/cleanup
    techniques. Each District response person will receive at a minimum one
    safety and response technique training course. Central Office personnel
    receive a respiratory safety training course annually.

        Training for the Emergency Response Program is developed from both
    in-house and EPA sponsored training courses.

                                   -49-

    VIII. COMPLAINT INVESTIGATIONS

        A.   Purgose

                  The main purpose for the investigation of complaints is to
             determine if a pollution or health hazard exists and- to correct
             problems found. Another reason is to serve the public and to make
             the public aware of action taken by this agency.

        -B. Strategyv

                  Because monitoring personnel are located in 12 District
             offices around the state, we are normally able to provide prompt
             response, follow-ups, and documentation of all complaints referred
             by  the  public  or  through  a member  of  the  legislature.  -This
             activity is scheduled in such a manner that provides minimal
             disruption of the normal work schedule.   State law provides that
             where a facility inspection is required, results of the inspection
             must be reduced to writing with a copy furnished to the complainant
             and the party being investigated.   Correction of the problem is
             made voluntarily in most cases, but necessary enforcement can be
             taken under the Pollution Control Act by the Enforcement and NPDES
             Administration Division.

        C.   ComDlaint Investiqation Policy

                  Whenever  possible,  complaints  should  be  filed  with  the
             district office having jurisdiction over the complainants location
             (see Table 9).

                  Telephone complaints received in the central office will be
             documented and referred to the appropriate District Director by
             telephone or radio.  Central Office personnel  will listen -to the
             complaint, obtain the complainant's name and phone number, and
             advise him that the proper person will contact him by phone as soon
             as possible.  It will then be the responsibility of the District
             Director to obtain the necessary information from the complainant
             and follow through with the investigation without delay.

                  Complaint letters received in the Central Office will be
             acknowledged by a letter from this office and referred to the
             District Director  for response.   District  Directors  are  advised
             that any and all assistance possible from this office will be
             furnished on request, but complaint investigation and proper
             documentation in our files is the specific responsibility of the
             District Director. We recognize the necessity for latitude and the
             exercise of professional judgement on the part of the District
             Director in complaint procedure and documentation. Again, with the
             express understanding that the handling of complaints is the
             responsibility of the District Director, the following is offered
             relative to proper documentation:

              1. A memorandum to the file, (handwritten if necessary) covering
                  complaint specifics and disposition, is considered to be the
                  absolute minimum (copy to wastewater files). The standard

                                       -50-

                                         Table 8

                        Office of Environmental Quality Control EQC District
                        Directory

    APPALACHIA I                              Environmental Quality Control Office
    (Anderson, Oconee Counties)              220 McGee Road
                                            Anderson, S.C.  29621              260-5569

    APPALACHIA II                             Environmental Quality Control Office
    (Greenville, Pickens Counties)           301 University Ridge, Suite 5800
                                            Greenville, S.C.  29601            242-9850

    APPALACHIA III                            Environmental Quality Control Office
    (Spartanburg, Cherokee, Union            151 E. Wood Street
      Counties)                              Spartanburg, S.C.  29303            596-3800

    CATAWBA                                  Environmental Quality Control Office
    (Lancaster, Chester, York Counties)    1001 W. Grace Street
                                            Lancaster, S.C.  29720             285-7461
                          Mailing Address:  PO Box 100, Fort Lawn, SC  29714

    CENTRAL MIDLANDS                         Environmental Quality Control Office
    (Richland, Lexington, Newberry,          Building No. 5, P.O. Box 156
      Fairfield Counties)                    State Park, S.C.  29147             737-7015

    LOW COUNTRY                              Environmental Quality Control Office
    (Beaufort, Jasper, Colleton,             149 Ribaut Square
      Hampton Counties)                      Beaufort, S.C.  29902               524-9760

    LOWER SAVANNAH                           Environmental Quality Control Office
    (Aiken, Orangeburg, Barnwell,            117 Marion Street, NE
      Bamberg, Allendale, Calhoun            Aiken, S.C.  29801                  648-9561
      Counties)

    PEE DEE                                  Environmental Quality Control Office
    (Florence, Dillon, Marion, Darling-    3204 Industry Boulevard--Route 11
      ton, Chesterfield, Marlboro Co.'s)   Florence, S.C.  29501                 662-3522

    TRIDENT                                  Environmental Quality Control Office
    (Charleston, Berkeley, Dorchester        1000 Air Park Road
      Counties)                              Charleston Heights, S.C.  29418  554-5533

    UPPER SAVANNAH                           Environmental Quality Control Office
    (Greenwood, Abbeville, Laurens,          P-129
      Saluda, Edgefield, McCormick Co's.) One Park Avenue
                                             Greenwood, S.C.  29646             223-0333

    WACCAMAW                                 Environmental Quality Control Office
    (Horry, Georgetown, Williamsburg         1705 Oak Street
      Counties)                              Myrtle Beach, S.C.  29577           448-1902

    WATEREE                                  Environmental Quality Control Office
    (Sumter, Kershaw, Lee,                   105 N. Magnolia Street
      Clarendon Counties)                    Sumter, S.C.  29151                '778-6548
                           Mailing Address: P.O. Box 1628                       778-1531

        complaint investigation form should' be used wherever practical since it
        will provide file documentation.

    2.   A facility owner has not been legally notified of an unsatisfactory
        situation unless he has been notified in writing.  If, in the ,judgement
        of the District Director, the matter investigated may result in
        administrative or court action by this agency, the owner is to be
        properly  notified with  a copy to our files.   In  instances where  a
        magistrate's warrant to enter. and inspect is issued, we have no choice
        but to reduce the results of such inspection to writing with a copy to
        the owner.

    3.   Many  complaints,  by  their  nature,  necessitate  a  letter  to  the
        complainant  covering  results  of  the  investigation  and  corrective
        measures taken.  It is understood that copies of such letters will be
        sent to wastewater files (or appropriate program file).

    4.   In order that copies of letters and other documentation may be properly
        filed, it is requested that they be forwarded to the attention of
         Enforcement Section, Bureau of Wastewater and Stream Quality Control.

    5.   Poor or  incomplete  documentation  will  very  effectively  prevent  the
        Department from taking proper enforcement action.

    6.   Use of the complaint investigation form is highly recommended.

                                        -52-

    IX. DRINKING WATER SUPPLIES MONITORING PROGRAM

              The monitoring program for drinking water supplies is divided into
         the following analytical groups:

              A.   Microbiological
              B.   Inorganic Chemicals
              C.   Organic Chemicals

         A.   MICROBIOLOGICAL                                      Projected Samples
                                                                      Per Year

              1.   Routine Sampling                                       13,000
                   a.   Repeat Samples                                     1,300

              2.   Town Surveys                                            3,400

              3.   Sanitary Surveys                                          500

              4.   Non-Routine Sampling                                    5,000

              5.   Private Well Samples                                    6,000

         B.   INORGANIC CHEMICAL

              1.   Routine Sampling (Public Complete Analysis Group)
                   a.   Surface Water                                         85
                   b.   Groundwater (Community)                              545
                   c.   Groundwater (non-transient non-community)            125
                   d.   Repeat Sampling                                       75

              2.   Routine Sampling (Nitrate Analysis)
                   a.   Groundwater (non-community)                          310
                   b.   Repeat Sampling                                       30

              3.   Controlled Fluoridation Program                         1,500
                      (Fluoride Analysis)
                   a.   Repeat Sampling                                      100

              4.   Corrosion Monitoring (Metals Analysis)                    400

              5.   Sanitary Survey (Public Complete Analysis Group)          200

              6.   Non-routine, Investigative Samples                      1,400

              7.   Private Well Sampling (Private Routine Analysis         3,754
                     Group)

         C.   ORGANIC CHEMICAL

              1.   Surface Water Supplies - Routine                           85
                   a.   Repeat Samples                                         8

              2.   Non-Routine Samples                                       550

              3.   Private Well Samples                                    1,580

                                          -53-

                                                           Projected Samples
                                                               Per Year

           4.   Sanitary Surveys. ISO

          S .   Trihalomethane Monitoring
                a.   Greater than 10,000 population                      140
                b.   Less than 10,000 population                          94

           6.   Volatile Organic Compound Monitoring                   3,094
                  (including 51 unregulated compounds)

    X. GROUND-WATER PROTECTION

           The Ground-Water Protection Division has the responsibility to
      develop a program to control and prevent the pollution of ground water
      in South Carolina.  Technical and policy making assistance is provided
      to the Bureau of Drinking Water Protection, Bureau of Water Pollution
      Control, other State and Federal agencies, and the general public.

      A.   Permit Issuance

                The responsibility for issuing permits for land disposal of
           wastes is assigned to the Bureau of Solid anid Hazardous Waste
           Management and the Bureau of Water Pollution Control.   However,
           prior to issuance of a permit, the Ground-Water Protection Division
           is called in to technically review the plans and specifications and
           make a site investigation relative to the potential effects on
           ground-water quality at the site.  An assessment of the geohydro-
           logical characteristics of the site is made by test drilling and
           recommendations are provided for issuance or denial of the permit,
           for conditions of the permit, and for ground-water quality
           monitoring.

                The objectives of the ground-water monitoring program are:

           a)   To obtain data for the purpose of determining baseline condi-
                tions of ground-water quality at the site.

           b)   To maintain  a monitoring  tracking  system to ensure  permit
                compliance.

           c)   To provide data for the early detection of ground-water pollu-
                tion or contamination, particularly in ground-water recharge
                areas and in areas of significant ground-water use.

           d)   To identify existing and/or potential ground-water pollution
                sources  and to maintain  surveillance  of these  sources,  in
                terms of their impact on ground-water quality.

           e)   To provide a statewide data base upon which management  and
                policy decisions can be made concerning the surface and
                subsurface disposal of wastes and the protection of. ground-
                water resources.

                                     -54-

    B.   Enforcement

             When a ground-water contamination problem is discovered,
        either from monitoring of a permitted site or from unregulated
        activities, the Division of Drinking Water Quality and Enforcement
        and/or the permitting program(s) pursue enforcement action.   The
        purpose is to stop further pollution of ground water and to assess
        the severity and extent of the problem. The responsibility for the
         investigation is usually placed on the owner of the facility but
        occasionally, either because the owner is uncooperative or unknown,
        the study is performed by the Ground-Water Protection Division.
        Recommendations are made to the appropriate enforcement section(s)
        throughout all phases of the enforcement action until a suitable
         solution to the problem is reached.

    C.   Water SuDolv

             The Water Supply Construction Division has the authority of
        permitting the construction or modification of public water supply
         systems  in the state.   Technical  assistance  is provided  to the
        Water Supply Construction Division by the Ground-Water Protection
        Division by reviewing public water-well specifications to ensure
         proper well-construction  standards  are being  met.   Ground-water
        conditions as indicated by the monitoring program are considered in
        the review of the specifications and the proposed well location.
        Technical assistance is -provided to individual well owners upon
         request.   The  Water  Supply  Construction  Division  private  well
        program. handles routine water-quality problems but when there are
        hydrogeological aspects, both related to quality and quantity, the
        Ground-Water Protection Division provides assistance to the well
        owner.

             Certification of well drillers through the Board of Certifi-
        cation of Environmental Systems Operators has been implemented. In
         addition, amendments to the State Safe Drinking Water Act
         authorizes regulation of the construction, maintenance, operation,
         and abandonment of wells by standards to be established by an
        Advisory Committee to the Board. The standards were implemented on
        June 28, 1985.

    D.   106 Program

             The Ground-Water Protection Division has been given the
         responsibility for development of the ground-water portions of the
         106 water-quality management  planning  effort.   Current  projects
         being developed under 106 are as follows:

         a)   Continual   evaluation   of   the   implemented   comprehensive
             ground-water protection strategy for South Carolina with
             attendant public participation and awareness programs;

         b)   Assessment of ground-water  recharge for aquifer  systems  in
             South Carolina;

         c)   Development   and   implementation   of  ground-water   quality
             standards systems for South Carolina.

                                   -55-

        d)   Development  of  an  ambient  ground-water  quality  monitoring
              network statewide.

         e)   Develop  and  maintain  a  ground  water  contamination  site
              inventory.

    E.   Underaround Injection Control Proqram

              The Ground-Water Protection Division activities required under
         primacy of the Underground Injection Control Program include:

         a)   Designation of underground sources of drinking water;

         b)   Development and maintenance of an inventory of injection wells;

         c)   Implementation  of permitting  for Class  II,  III,  and  IV A
              injection wells;

         d)   Surveillance and investigation of injection facilities;

         e)   Provision  for  training  activities  to  support  the  U.I.C.
              program;

         f)   Development and maintenance of data management system;

         g)   Provision for public participation and the dissemination of
              information regarding ground-water protection.

    F.   Underaround Storaqe Tank Proqram

              The Ground-Water Protection Division  is responsible for the
         implementation of the Underground Storage Tank Control Regulations.
         Regulated activities include:

         a)   Notification  of  existing  underground  storage  tanks  for
              development of a tank inventory;

         b)   Permitting of new underground storage tank systems;

         c)   Surveillance and investigation of all underground storage tank
              facilities;
         d)   Overseeing all  phases of leak assessments  and remediations
              from underground tanks.

         e)   Underground storage tank training opportunities;

         f)   Development and implementation of automated data management
              system;

         g)   Provision for public participation and dissemination of infor-
              mation concerning underground storage tanks.

         h)   Administering the Federal UST Trust Fund Cooperative Agreement
              to address leaking UST's with no responsible party.

             1)   Development  and  implementation  of programs' as mandated  by
                  State SUPERB Act.

    XI.  SOLID AND HAZARDOUS WASTE FACILITY MONITORING PROGRAM

             It  has  been , recognized  nationally  that  hazardous  waste  land
        disposal facilities are the known or potential sources of harmful
        contamination  to  the  nation's  ground-water  supplies.    Many  such
        facilities have been determined to have inadequate ground-water
        monitoring systems to detect  such contamination.   In South Carolina,
        there are thirty-two hazardous waste land disposal facilities regulated
        under the South Carolina Hazardous Waste Management Regulations. These
         facilities are required to monitor groundwater in the upper most aquifer
        antd if contamination is detected, to conduct further comprehensive
        assessments. Additionally, pursuant to the federal 1984 Hazardous and
        Solid Waste Amendments to the Resource Conservation and Recovery Act,
         solid waste management units located at these and an additional 50 or so
        facilities will be evaluated to determine if release of- hazardous
        constituents  have occurred.   Ultimately,  contamination from hazardous
         and solid waste management units must be remediated through corrective
         action programs.

             Consistent with Federal mandates, SCDHEC through its Bureau of
        Solid and Hazardous Waste Management conducts periodic inspections and
        evaluations of these groundwater monitoring systems. As a part of these
        oversight activities, ground-water samples are taken and analyzed. This
        ground-water information is utilized by Department staff in determining
        the adequacy of these monitoring  systems.   Furthermore,  such data  is
         invaluable in determining the reliability of results provided by the
        regulated community.

        -A. Solid Waste Facilities

             Ground-Water Monitorina

                  Ground-water monitoring wells are located after approval from
             the Hydrogeology Division.   An effort  is made to determine  the
             direction  of flow of the ground  water.   One  (1) well  is  then
             located hydraulically upgradient and at least two (2) wells are
             located hydraulically downgradient.  Circumstances at the site may
             dictate  additional  wells  (e.g.,  extremely  large  sites,  complex
             .geol ogy) .

                  To  establish   background  conditions,   wells  are  sampled
             quarterly  for  one  (1) year.   After  background  is  established,
             monitoring may be reduced to semi-annual and annual monitoring.
             Changes in water quality would serve as an indicator that ground
             water  may  be  impacted  by  the  waste  disposal  activities.   In
             addition to SCOHEC sampling, solid waste facilities submit all data
             that they collect.

             Analyses normally required of owners for sanitary landfill wells
             are:

                                        -57-

             To Establish Backaround Conditions.(quarterly for I year)

             pH                        Barium               Endrin
             Specific conductance      Cadmium              Lindane
             Total organic carbon      Chromium             Methoxychlor
             Chlorides                 Lead                 Toxaphene
             Fluoride                  Mercury              2,4-D
             Sulfates                  Selenium             2,4,5-TP Silvex
             Nitrates                  Silver               Water Level
             Arsenic

             After Backaround Conditions are Established

             Semi-Annuallv Annually

             pH                                   Chlorides
             Specific conductance                 Sulfates
             Total Organic Carbon                 Nitrates
             Water Level

             When laboratory results show significant values in excess of
        allowable drinking water standard criteria for water quality, a
        determination  will  be  made  on  the  necessity  of  a  leachate
        collection   and   treatment   system   to  prevent   ground   water
        contamination.   Other remedial  measures may be considered  (e.g.,
        clay or impervious cover to restrict the flow of surface water
        through the waste).

    B.   Hazardous Waste Land Disoosal Facilities

        Ground-Water Monitorinc

             EPA's Technical Enforcement Guidance Document is the primary
        guidance under which ground-water is monitored.   A ground-water
        monitoring system must be capable of immediately detecting a
        release of hazardous waste or constituents into the uppermost
         aquifer and hydraulically interconnected  aquifers.  At least one
         (1) well must be located hydraulically upgradient from the waste
        management area. At least three (3) wells must be located hydraul-
         ically downgradient at the limit of the waste management area.

             To establish background concentrations, wells are sampled
         quarterly  for  one  (1) year.   After  background  is  established,
        monitoring may be reduced to semi-annual and annual monitoring with
         the Department's concurrence. Changes in water quality would serve
         as an indicator that ground water may be impacted by the disposal
         activity. Data is required by regulation to be submitted to SCDHEC
         by facilities, and SCDHEC conducts periodic monitoring (Ref. SW-
         846).

             Analysis normally required for interim status hazardous waste
         land disposal facilities are:

                                   -58-

    To Establish Backaround Conditions (quarterly for 1 year)

    Arsenic              Silver               Chloride
    Barium               Endrin               Iron
    Cadmium              Lindane              Manganese
    Chromium             Methoxychlor         Phenols
    Fluoride             Toxaphene            Sodium
    Lead                 2,4-D                Sulfate
    Mercury              2,4,5-TP Silvex      pH
    Nitrate              Radium               Specific Conductance
    Selenium             Gross Alpha          Total Organic Carbon
                        Gross Beta           Total Organic Halogen
                        Turbidity            Water Level
                        Coliform Bacteria

    After Backaround Conditions are Established

    Semi-Annually                        Annually

    pH                                   Chloride
    Specific Conductance                 Iron
    Total Organic Carbon                 Manganese
    Total Organic Halogen                Phenols
    Water Level                          Sodium
                                        Sulfate

         If contamination is determined to exist, more comprehensive
    assessments and corrective actions may be required under the
    regulations.

                                 -59-

    XII. LABORATORY SUPPORT

        A. 'Laboratory Services

                  The Analytical Services Division provides laboratory services
             to the following programs: Water Pollution Control, Drinking Water
             Protection,    Ground-Water    Protection,    Recreatignal    Waters,
             Shellfish, Solid and Hazardous Waste Management, District Services,
             Biological  Monitoring,  and  Emergency  Response  Services.   The
             analytical services offered include bacteriological, chemical, and
             physical analyses. The types of samples analyzed include water,
             wastewater, leachate, soil, sediment, chemical wastes, fish, and
              shellfish.

                  The organizational structure encompasses five sections and
              five  regional  laboratories.   The  Central  Laboratory  Sections
              include Sample Management, Metals Analysis, Automated Analysis,
             Or-ganic  Analysis,  and  Environmental   Microbiology.    The  five
             regional laboratories are located in Aiken, North Charleston,
              Florence, Greenville, and Lancaster.

                  The Regional Laboratories initiate all stream and wastewater
              analysis and the Central Laboratories provide support analyses,
              i.e., metal, nutrient, toxic extraction procedures, and organic
              analyses.  Drinking Water is essentially a Central Laboratory pro-
             gram with support from the Regional Laboratories.
                  The  Division  Director  coordinates  the  internal   quality
              assurance program.

         B.   Analytical Services Qualitv Assurance Proqram

                  A quality assurance program is essential to produce valid data
              and to provide a means to systematically demonstrate its validity.
             The quality assurance program encompasses every aspect of the
              laboratory analysis from container preparation through the actual
             data release from the Analytical Services Division Laboratory to
              the Environmental Quality Control (EQC) Programs.

                  The Analytical  Services  Division  has developed  two quality
             control manuals which detail the day-to-day operation of the
             quality  assurance  program:   (1) Procedures  and  Quality  Control
             Manual  for Chemistry  Laboratories--Analytical  Services  Divisio ,n;
              and (2) Laboratory Procedures Manual for Environmental Micro-
              biology--Analytical  Services  Division.   The elements  of  quality
             control addressed in the manuals include organization and sample
             chain of custody; personnel training; quality control of laboratory
              services,    equipment,    reagents,    solvents,    and   glassware;
             methodology; and analytical performance control.

                  The  overall   laboratory  quality  assurance  program  which
              includes the previously discussed elements requires a minimum of
              15%  of  allocated  resources.   The  frequency  for  analysis  of
             replicates and spike recovery samples is noted in the manuals and
              is in compliance with U.S. EPA guidelines.  EPA reference samples
             are also analyzed as noted in the manuals. In addition, the

                                        -60-

        Analytical Services Division participates in the annual EPA Water
        Supply and Water Pollution Performance Audit Sample Programs. The
        Environmental Microbiology Laboratories perform replicate analyses,
        positive tast controls, media control tests, equipment control
        tests, etc., as required by EPA Laboratory Certification and
        Evaluation guidelines.

             The laboratory analyses are conducted according to the List of
        Approved Test Procedures in the Federal Register, Volume 49, No.
        209, October 26, 1984, and in the Federal Register, Volume 51, No.
        125, June  30,  1986.   The Analytical  Services  Division  quality
        control manuals include a section on methodology designed to reduce
        variations in applied techniques among the six laboratories where
        methods permit analyst interpretation, and thus provide a more
        uniform approach which will increase the reproducibility of results
        reported from the laboratory system.

             The proper containers must be selected for sampling as well as
        the  proper preservation  and  an adequate  volume  collected.   The
        reader should refer to the next section entitled "Sample Containers
        and Preservation."

             A detailed discussion of sample chain of custody and the
        management of data flow is included in the manuals.   The reader
         should refer to the flow chart, Table 10, entitled "Sample Chain of
        Custody and Data Flow."

    C.   Samole Containers and Preservation

             Control of the quality of laboratory analyses begins with the
         sample collection.   The validity of analytical  results  obtained
        depends upon a representative 'sample of the source from which it
        was collected.  The concentration of each constituent in a sampl e
        at the time of collection must be maintained until all analyses
         have been  completed.   Constituent concentrations  may be altered
         after collection through contamination of the container, reactions
        between sample components and the container walls, and through
         naturally  occurring  reactions  within  the  sample  itself.   This
         section contains the methodology employed by the Laboratories to
        control those factors which can affect sample'validity. The actual
         sample collection procedures are not included in this manual; the
        reader may wish to refer to the manual entitled Standard Ooeratincq
         and Oualitv Control Procedures for Ambient Stream and Wastewater
         Facility Monitorina (SCDHEC).

             Glass, polyethylene, and polypropylene bottles are used as
         sample containers. The sample container is cleaned and labeled for
        the parameter for which it is used.  The containers used for the
        various parameters have been chosen for their chemical resistance
        to  the  chemical   parameter   of  interest   and  the   required
        preservatives.-Random substitution of containers may not be made.

     SAMPLE COLLECTION SITE  _       _   REGIONAL LABORATORY SAMPLE CUSTODIANmples  REGIONAL LABORATORY ANALYSES
     (Samples with Field Sheet)                                                     Data

                            CENTL  LABORATORY SAMPLE  C  U     STODIN Samples
                   CENTRAL          LABORATORY                  SAMPLE CUSTODIAN  Data  METALS ANALYSIS SECTION
                                                                            AUTOANALYSIS SECTION
                                                                            ORGANIC CHEMISTRY SECTION
                                                                            MICROBIOLOGY SECTION

                                           ANALYTICAL SERVICES DIVISION OFFICE

                        F                                ~~~~~~~~~~~I                                '
     DRINKING WATER PilOTECTION.                SOLID & HAZARDOUS                     WATER POLLUTION CONTROL
                                                 WASTE MANAGEMENT

       I        o     I                                   I
     DRINKING
      WTRRCETOA                      GWATER ATRSELIH                          BIOLOGICAL       STREAM      FACILITIES
     PROGRAM           WATERS         PROTECTION                PROGRAM        SERVICES      MONITORING    MONITORING
                      .PROGRAM   '    PROGRAM                                  PROGRAM        PROGRAM       PROGRAM

    ANALYTICAL SERVICES DIVISION

    SAMPLE CHAIN OF CUSTODY AND DATA FLOW

                 TABLE 9

             Special cleaning procedures are employed for the various con-
        tai ners.   Each  parameter  or parameter  group  involves  different
        interfering compounds and contaminants which must be removed from
        the container walls.  Containers required for Parameters analyzed
        by the Organic and Inorganic Chemistry Laboratories are maintained
        by those laboratories.  Clean containers for organic and inorganic
        parameters are shipped to the Regional Laboratories by the Sample
        and Data Management Center in Columbia.   Containers required for
        parameters analyzed by the Regional Laboratories are maintained by
        those laboratories and cleaned according to special procedures.

             Based upon the available sample preservation research data and
        the  desire  to  parallel  United  States  Environmental  Protection
        Agency laboratory procedures, the Analytical Services Laboratories
        add preservatives to all drinking water, ground water, stream
        water, and wastewater program samples collected for chemical
        analyses upon receiving them into the laboratory with the following
        exceptions:

        (1)  If the samples cannot be transported to the laboratory before
             the end of the working day which is normally 5:00 p.m., the
             samples must be preserved in the field.

         (2)  All water samples for cyanide, phenol,  and sulfide analyses
             must be preserved at the site immediately after collection.

             The district offices are responsible for requesting the pre-
        servatives in order to maintain an ample quantity.  Each dispenser
        is labeled in bold letters to assist the collector to choose the
        proper  preservative  for  the  container;  i.e.,  METALS,  MERCURY,
        NUTRIENTS, TOC, etc.  Because the concentration levels cannot be
        maintained at the level collected indefinitely, maximum holding
        times have been set for each parameter. Analyses must be completed
        during the time limits set for valid results. Required containers,
        preservatives, and holding times for each parameter and procedures
        used for preserving cyanide, phenol, and sulfide samples at the
        collection site are listed in the Procedures and Quality Control
        Manual for. Chemistry Laboratories - Analytical Services Division,
        and Standard Operating and Quality Control Procedures for Ambient
        Water Quality and Wastewater Facility Monitoring - Stream and
        Facility Monitoring Section.  The regional  or central  laboratory
        chemists are responsible for providing containers, preservation
        materials, and preservation technique instructions to sample col-
        lectors for samples for cyanide, phenol, and sulfide analyses.

    D.   Laboratory Evaluation Procqram

             The laboratory certification program is authorized by Regu-
        lation 61-81 entitled "State Environmental Laboratory Certification
        Program" which became effective January 1, 1981.  The regulation
        applies to all laboratories which generate data for compliance with
        state environmental regulations.

             The two main components of the certification program are (1)
        an on-site evaluation of the laboratory in regard to facilities,
        equipment, methodology, records keeping, and quality control and

                                   -63-

    (2) the analysis of performance audit samples.  A detailed report
    of the evaluation revealing all deficiencies found is written and
    returned to the laboratory with -a' letter stating that all
    deficiencies are to be corrected and certification obtained within
    90 days.  If certification is not obtained at the end of 90,days,
    Environmental Quality Control will not accept data from that
    laboratory. Audit samples must be analyzed satisfactorily prior to
    certification.  These samples must be analyzed annually for each
    parameter for which certification is desired.  The unsatisfactory
    analysis of two consecutive audit samples for any parameter will
    result in decertification.

         Evaluation of wastewater laboratories are now being scheduled
    based on date of last inspection and alphabetically for those which
    have not received an initial evaluation.   These evaluations will
    include drinking water and wastewater laboratories with limited
    work in the disciplines of solid and hazardous waste, groundwater
    monitoring,  air,  and biological  assessments.   It should also be
    noted that some laboratories will require two or more people to
    perform the evaluation and many laboratories will require follow-up
    evaluations.   Complete  evaluations  are  planned  at  three  year
    intervals.   The   laboratory   certification   staff   assist   with
    performance  audit  evaluations.   Technical  review  of  laboratory
    design   and   equipment   specifications   is  conducted   for  the
    Construction Grants Program.

                               -64-

    XIII.  DATA HANDLING

             Data for samples that are analyzed in the District Laboratories are
        reported on the appropriate data sheets and released by the  sample
        custodian.   These  data  sheets  are  sent  to the  Analytical  Services
        Division in Columbia each Friday where they,  along with data sheets
        generated in the Central Laboratory, are sent to the appropriate program
         areas.  All stream and facility data is distributed by Section managers
        to the appropriate section member.

         A.  Ambient  Stream  Monitorina  - Most  ambient  stream  and  sediment
              samples are collected by District personnel.  The data is sent to
             the Water Quality Monitoring Section manager through the Analytical
             Services Division.   The data are reviewed by the Water Quality
             Monitoring Section and are sent to Data Systems Management for key-
              punching. The keypunched data are edited and then stored in EPA's
             computerized data base (STORET) of water quality data. Data sheets
              are kept on file in the Water Quality Monitoring Section.

          B.  SDecial Study Data - Generally special studies are initiated in the
              Central Office through requests from other Divisions or Districts.
              Samples are usually collected with the cooperation of the District
             within which the study area lies. Samples and data are handled as
              for ambient monitoring.

          C.  ComDliance SamDlinc  - Compliance  sampling data are sent to the
              Facilities  Compliance  Section  manager  through  the  Analytical
              Services  Division.   After  review  by the  Facilities  Compliance
              Section, the data is sent to Data Systems Management for key-
              punching. Keypunched data is edited and a compliance monitoring
              report is generated. A determination of compliance is made by the
              Facilities Compliance Section.   If the facility  is not  in com-
              pliance, a letter of noncompliance is sent to the owner. Copies of
              the data are sent to the District Lab and the Central files.
              Copies of the report are sent to the permittee, District, Central
              files,  and  EPA  (majors).   Inspections  are  tracked  by  EPA's
              computerized Permit Compliance System (PCS).

          D.  NPDES ComDliance and Self-Monitorinq- NPDES compliance reports and
              self-monitoring data are monitored for accuracy and a determination
              of compliance made by the Enforcement Section.   If the facility
              shows a trend of noncompliance, a Notice of Violation is sent to
              the owner.

          E.  Federal  ODeration  and Maintenance  InsDections  - The  inspection
              reports are completed by the Facility Evaluator and sent to the
              Facilities Compliance Section. After review and logging, copies are
              sent to the facility owner, the District, EPA Region IV, and the
              Facilities Compliance Section files.  A letter is also sent to the
              owner with a response requested if problems are noted. Inspections
              are tracked by EPA's computerized PCS.

         F.   State ODeration and Maintenance InsDections  - Routine State 0 & M
              inspections are completed by the Facility evaluator and reviewed by
              the District Director. Copies of the report are distributed to the
              facility owner, the facility operator, and the district files, with

                                        -65-

        the original being sent to the-Facilities Compliance Section.. The
        original  is later placed in the 'Central -files.   Informati on -from
        the inspection is updated in the computerized Carolina File.
         Inspections are tracked by the EPA's computerized PCS.

    G.   Fish Kill  - Samples are sent to the Analytical Services Division
        for analysis.  The data is sent to the Emergency Response Section
        and collated with the fish kill report.  A copy of the fish kill
         investigation report and data is sent to the owner (if the kill
        occurred in a private pond), the person who reported the kill, the
        District Director of the area where the kill occurred, South
        Carolina Wildlife and Marine Resources if they helped with
        investigation or expressed interest in the kill, the Enforcement
        Section of DHEC, and OHEC's central files.  A permanent numerical
        record is kept by the Emergency Response Section.

    H.   Oil and Hazardous Materials - Normally, samples are not collected
        on  spill  investigations.   However,  whenever  the  spiller  cannot
        readily be identified, the samples are collected and they follow
        the procedure as alluded to in the "fish kill" procedure.

         For hazardous materials investigations, samples are usually col-
        lected upstream and downstream of the spill site, along with
        samples of the spilled material.  These samples are then returned
        to  the  Sample  and  Data  Control  Center  of  Analytical  Services
        Division  and  logged  in for analysis.   Upon completion,  data  i s
        entered on the appropriate data sheet and forwarded to the
        Emergency Response Section to be collated with the spill report.
        Copies of the hazardous materials report and data are sent to the
        spiller if requested, the Environmental Protection Agency if
        appropriate, the Central file of the Department of Health and
         Environmental Control, and to the appropriate Enforcement Section
        of the South Carolina Department of Health -and Environmental
        Control.

        A  permanent   numerical   record   is  kept  in the Central  files
        area.

    I.   Biolociical Monitorinci- After samp les are collected, data sheets are
        kept on file in the Water Quality Monitoring Section until sample
        analysis is completed.  Upon completion of analysis, any physical
        or chemical  data are placed  in STORET.  Data  sheets  describing
        biological data are kept on file in the Water Quality Monitoring
        Section.

                                   -66-

    XIV. APPENDICES

          -67-

                             APPENDIX A

    SOUTH CAROLINA DEPARTMENT OF HEALTH AND ENVIRONMENTAL CONTROL

         PRIMARY AND SECONDARY STREAM STATION DESCRIPTIONS
                    LISTED BY LABORATORY DISTRICT

                                       APPENDIX A

             SOUTH CAROLINA DEPARTMENT OF HEALTH AND ENVIRONMENTAL CONTROL

          PRIMARY AND SECONDARY STREAM STATION DESCRIPTIONS LISTED BY REGION

                           STREAM STATIONS FOR AIKEN - PRIMARY
                                 LOWER SAVANNAH DISTRICT

    Station      DescriDtion                                             Criteria   Basin

    CSTL-003    SALKEHATCHIE RVR AT SC 278 2.5 MI
                S BARNWELL                                                 6         0924
    CSTL-012    COOSAWHATCHIE RVR AT S-03-22 1.5 MI SW ALLENDALE            1         0932
    CSTL-028   -SALKEHATCHIE RVR AT SC 64 2 MI W OF BARNWELL                1,5       0924
    E-008       N FORK EDISTO RVR AT S-38-39 WSW OF ROWESVILLE              2,16      0914
    E-013       EDISTO RVR AT US 78 W OF BRANCHVILLE                        1,2,4    0908
    E-051       PROVIDENCE SWP AT E FRONTAGE RD TO 1-95 7 MI
                NW OF HOLLY HILL                                           7,14      0912
    E-059       4 HOLE SWP AT S-38-50 5.2 MI SE OF CAMERON                  1,7       0912
    E-090       S FORK EDISTO RVR AT US 1 12 MI NE AIKEN                    1         0918
    E-091       N FORK EDISTO RVR AT SC 391 5.5 MI S BATESBURG              1         0916
    E-092       N FORK EDISTO RVR AT SC 3 5.5 MI NW NORTH                   1,2       0914
    E-094       SHAW CREEK AT S-02-26 4.2 MI NE AIKEN                       12,15    0918
    E-099       N FORK EDISTO RVR AT S-38-74 NW ORANGEBURG                  7,9       0914
    S-123       LITTLE SALUDA RVR AT S-41-39 5.2 MI NE SALUDA               7,10      0840
    S-131       LK GREENWOOD AT US 221 7.6 MI NNW 96                        8,15      0844
    S-186       SALUDA RVR AT SC 34 6.5 MI ESE OF 96                        1         0842
    S-295       SALUDA RIVER AT S.C. ROUTE 39                               10        0842
    ST-025      LK MARION AT MID BRDG ON 1-95 AT SANTEE                     8         0804
    SV-069      SAND RVR AT OLD US 1 1.2 MI SE WARRENVILLE                  10        1306
    SV-071      HORSE CK AT S-02-104 0.6 MI SW GRANITEVILLE                 6         1306
    SV-118      SAVANNAH RVR AT US 301 12.5 MI SW ALLENDALE                 2,3,16   1304
    SV-250      HORSE CK AT SC 125 1.5 MI SW CLEARWATER                     6         1306
    SV-251      SAVANNAH RVR AT US 1 1.5 MI SW N. AUGUSTA                   6,12      1306
    SV-252      SAVANNAH RVR AT SC 28 1.6 MI NNW OF BEACH ISLAND            1,3       1304
    SV-291      CLARKS HILL RESERVOIR AT US 378 7 MI SW MCCORMICK           8,16      1308
    SV-294      CLARKS HILL RESERVOIR AT DAM AT US 221 1.5 MI
                SW CLARKS HILL                                             1         1306
    SV-318      LONG CANE CK AT S-33-117 7.0 MI NW MCCORMICK                10,17    1308
    SV-323      SAVANNAH RVR AT LOCK AND DAM                                1,3,16   1304
    SV-324      TIMS BR AT SRP ROAD C                                       17        1304
    SV-325      UPPER THREE RUNS CK AT SRP ROAD A                           17        1304
    SV-326      FOUR MILE CK AT SRP ROAD A-7                                17        1304

    Station Selection Criteria

    1 = Influent to segment (sub-basin)          9 = Above major municipal area
    2 = Effluent to segment                     10 = Below major municipal area
    3 = Major streams at state lines            11 = Mouth of major tributary
    4 = Confluence of major streams             12 = Major water use area
    5 = Above a major industrial area           13 = Above major land use area
    6 = Below a major industrial area           14 = Below major land use area
    7 = Water Quality limited area              15 = Above a water intake
    8 = Major lake                              16 = Basic Water Monitoring Program
                                                17 = Other

                                           A-1

    STREAM STATIONS FOR AIKEN - PRIMARY
       Lower Savannah District (continued)

    Station     DescriDtion                                              Criteria   Basin

    SV-327      STEEL CK AT SRP ROAD A                                       17       1304
    SV-328       LOWER THREE RUNS CK AT S-06-20 7.5 MI SW BARNWELL           17       1304
    SV-329      HORSE CREEK AT ASCAUGA LAKE ROAD (S-02-33) IN
                GRANITEVILLE                                                5        1306
    SV-330      STEVENS CREEK AT S-33-21                                     10       1306

    Station Selection Criteria

    I = Influent to segment (sub-basin)          9 = Above major municipal area
    2 = Effluent to segment                      10 = Below major municipal area
    3 = Major streams at state lines             11 = Mouth of major tributary
    4 = Confluence of major streams              12 = Major water use area
    5 = Above a major industrial area           13 = Above major land use area
    6 = Below a major industrial area            14 = Below major land use area
    7 = Water Quality limited area               15 = Above a water intake
    8 = Major lake                               16 = Basic Water Monitoring Program
                                                17 = Other

                                          A-2

    Primary Stream Monitoring Stations                                                                      ~

                                                                                      dip~ ~ ~ ~ ~~~~~~~~~K

                          STREAM STATIONS FOR AIKEN - SECONDARY
                                  LOWER SAVANNAH DISTRICT

    Station      DescriDtion                                              Criteria   Basin

    CSTL-OO1B   TURKEY CK 1 MI BL MILLIKEN BARNWELL OUTFALL
                 AT CLINTON ST.                                              6         0924
    CSTL-005    LEMON CK ON S-05-77                                          7         0924
    CSTL-037    GRAPEVINE CK ON S-05-32 SW OF BAMBERG                        10        0924
    E-001       FIRST BR AT BRDG ADJACENT TO WTR PLT AT JOHNSON
                   AT S-19-41                                                9         0918
    E-002        S FORK EDISTO RVR AT S-19-57 BL JOHNSTON SWR OUTFALL    10            0918
    E-007        N FORK EDISTO RVR AT US 601 AT ORANGEBURG                   5         0914
    E-007A       N FORK EDISTO RVR AT POWER LINE CROSSING
                   2 MI BL E-007                                             6         0914
     E-007B      N FORK EDISTO RVR 4 MI BL E-007 AT A CABIN                   6         0914
     E-007C      N FORK EDISTO RVR AT POLICEMANS CAMP 6 MI BL E-007           10        0914
    E-012       SOUTH EDISTO RIVER AT SC 39 BRIDGE                           2,11      0918
    E-019       HOME BR AT S-38-68 1.2 MI SW OF HOLLY HILL                   7         0912
    E-022       GRAMLING CK AT CLVT ON SC 33 2 MI E OF ORANGEBURG            10        0912
     E-036       GOOD LAND CK AT SC 4 2.1 MI E OF SPRINGFIELD                 10        0918
     E-076       TRIB TO GRAMLING CK AT SC 33-BL UTICA TOOL CO                6         0912
    S-050        LITTLE SALUDA RVR AT US 378 E SALUDA                        6,10      0840
    S-092       CORONACA CK AT S-24-100 4 MI NW OF 96                        7         0842
    S-093       WILSON CK AT SC 702 5.2 MI ESE OF 96                         7         0842
    S-233        WILSON CK AT S-24-101                                       10        0842
    S-235       WILSON CK AT S-24-124                                        7         0842
    S-255        CLOUDS CK AT S-41-26 4 MI NW BATESBURG                      7         0840
    SV-068       BEAVERDAM CK AT S-19-35 3.8 MI NW OF EDGEFIELD              10        1306
    SV-072      HORSE CK AT S-02-145                                         4         1306
     SV-073       LITTLE HORSE CK AT SC 421 BL EFF OF CLEARWTR FIN            6         1306
     SV-096       EFF FROM HORSE CK POND AT DAM ON S-02-254                   5         1306
     SV-151      HARD LABOR CREEK AT S-24-164 BRIDGE                          10        1306
     SV-175       LOWER 3 RUNS CK AT SC 125 11 MI NW OF ALLENDALE             6         1304

     Station Selection Criteria

     1 = Influent to segment (sub-basin)           9 = Above major municipal area
     2 = Effluent to segment                      10 = Below major municipal area
     3 = Major streams at state lines             11 = Mouth of major tributary
     4 = Confluence of major streams              12 = Major water use area
     5 = Above a major industrial area            13 = Above major land use area
     6 = Below a major industrial area            14 = Below major land use area
     7 = Water Quality limited area               15 = Above a water intake
    8 = Major lake                               16 = Basic Water Monitoring Program
                                                 17 = Other

                                             A-4

                                                                                                               41 ~ ~ ~ ~

                                                                                                             40~~~~~~~~~~~~~~~~~~~~~~~~

                                                                                      CIO~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~I

    Scnar StemMntrigSain

                            STATIONS FOR CHARLESTON - PRIMARY
                                    TRIDENT DISTRICT

    Station     Descriotion                                             Criteria   Basin

    CSTL-006    SALKEHATCHIE RVR AT 601 9 MI NE HAMPTON                     1,2      0922
    CSTL-062    TAIL RACE CANAL AT US 52 & 17A BELOW LAKE MOULTRIE          1        0820
    CSTL-063    WASSAMASSAW SWP AT US 176                                   1        0818
    CSTL-079    DIVERSION CANAL AT SC 45 12.6 MI W OF ST STEPHENS           1,2      0822
    CSTL-098    COMBAHEE RVR AT US 17 10 MI ESE YEMASSEE                    1,2,16   0920
    CSTL-107    COOSAWHATCHIE RVR AT US 17 AT COOSAWHATCHIE                 2        0930
    CSTL-109    COOSAWHATCHIE RVR AT S-25-27 2.5 MI SW CUMMINGS             2,16     0932
    E-015       EDISTO RVR AT SC 61 AT GIYHANS FERRY ST PK                  1,16     0906
    E-100       4 HOLE SWP AT US 78 E OF DORCHESTER                         2,16     0912
    MD-007      POCOTALIGO RVR AT US 17 AT POCOTALIGO                       1        0926
    MD-020      MOUTH OF WAPPOO CK BTWN CHANNEL MARKERS 3 & 4               7        0814
    MD-026      STONO RVR AT SC 700                                         2        0814
    MD-034      RT BK OF ASHLEY RVR BTWN MOUTH OF WAPPOO CK & DILLS CK  7            0814
    MD-043      COOPER RVR AT CHANNEL MARKER 72 NEAR USN AMMO DEPOT         1        0810
    MD-044      COOPER RVR BL MOUTH OF GOOSE CK AT CHANNEL BUOY 60          6        0810
    MD-045      COOPER RVR AB MOUTH OF SHIPYD CK AT CHANNEL BUOY 49         2        0810
    MD-046      COOPER RVR UNDER GRACE MEMORIAL BRDG                        7        0814
    MD-047      TOWN CK (W SIDE OF DRUM ISL) UNDER GRACE MEMORIAL BRDG  7            0814
    MD-048      S CHANNEL CHAS HBR OFF FT JOHNSON QUAR STA BELL
                   BUOY 28                                                 7,16     0814
    MD-049      ASHLEY RVR AT MAGNOLIA GARDENS                              6,10     0818
    MD-052      ASHLEY RVR AT SALRR BRDG                                    2        0818
    MD-069      INTRACOASTAL WATERWAY AT SC 703 E MT PLEASANT              17        0806
    MD-070      ABANDONED BRDG OVER THE COVE END OF PITT ST
                   MT PLEASANT                                             7        0814
    MD-071      SHEM CK AT BRDG ON US 17                                    7        0814
    MD-113      GOOSE CK RES AT CHTN WTR INTAKE                             12       0810
    MD-114      GOOSE CK AT S-10-52 N CHTN                                  10       0810
    MD-115      WANDO RVR AT SC 41                                          1        0808
    MD-118      NEW RVR AT SC 170 9 MI W OF BLUFFTON                        2        0928
    MD-119      EDISTO RVR AT US 17 12.5 MI NW RAVENEL                      1,2      0906
    MD-120      DAWHOO RVR AT SC 174 9 MI N OF EDISTO BCH SP                1        0902
    MD-152      COOPER RVR AT S-08-503 6.2 MI ESE OF GOOSE CK               2        0820
    MD-165.     CHAS HBR AT FT JOHNSON PIER AT MARINE SCI LAB               7        0814
    MD-195      BOHICKETT CR AT SC 700 1 MI SW OF CEDAR SPRINGS             9,10     0902
    MD-198      WANDO RVR BTWN RATHALL & HOBCAW CKS                         2        0808

    Station Selection Criteria

    1 = Influent to segment (sub-basin)          9 = Above major municipal area
    2 = Effluent to segment                     10 = Below major municipal area
    3 = Major streams at state lines            11 = Mouth of major tributary
    4 = Canfluence of major streams             12 = Major water use area
    5 = Above a major industrial area           13 = Above major land use area
    6 = Below a major industrial area           14 = Below major land use area
    7 = Water Quality limited area              15 = Above a water intake
    8 = Major lake                              16 = Basic Water Monitoring Program
                                                17 = Other

                                           A-6

                            STATIONS FOR CHARLESTON - PRIMARY
                                    TRIDENT DISTRICT

    Station     DescriDtion                                              Criteria   Basin

    MD-202      STONO RVR AT S-10-20 2 MI UPSTRM OF CLEMSON EXP STA         1        0814
    MD-217      DURHAM CK AT S-08-9 BRIDGE                                  12,15    0820
    MD-240      FOSTER CREEK AT CHARLESTON CPW WATER INTAKE                 15       0820
    MD-241      MECHAW CK AT SC ROUTE 45                                    17       0802
    ST-001      SANTEE RVR AT SC 41/US 17A NE OF JAMESTOWN                  5,16     0802
    ST-006      S SANTEE RVR AT US 17                                       2        0802
    ST-016      SANTEE RVR AT US 52 6.5 MI NNW OF ST STEPHENS               1        0802
    SV-191      SAVANNAH RVR AT US 17 8.9 MI SSW OF HARDEEVILLE             2,3      1302

    Station Selection Criteria

    1 = Influent to segment (sub-basin)          9 = Above major municipal area
    2 = Effluent to segment                     10 = Below major municipal area
    3 = Major streams at state lines            11 = Mouth of major tributary
    4 = Confluence of major streams             12 = Major water use area
    5 = Above a major industrial area           13 = Above major land use area
    6 = Below a major industrial area           14 = Below major land use area
    7 = Water Quality limited area              15 = Above a water intake
    8 = Major lake                              16 = Basic Water Monitoring Program
                                                17 = Other

                                        A-7

              cj~~~~~~~~,

                                                             ~~~~~~~0~ ~ ~ ~ ~

                   rz~~~~~~~~~~~

                              )   ~~~~~~~~~~~~~~~~~~~~~~~~N, ,.r*

    Primary Stream Monitoring Stations
               Trident District

                       STREAM STATIONS FOR CHARLESTON - SECONDARY
                                    TRIDENT DISTRICT

    Station      DescriDtion                                              Criteria   Basin

    CSTL-007    COMBAHEE SWP BL YEMASSEE SEWAGE OUTFALL                      10        0922
    CSTL-010    SANDERS BR AT SC 278                                         9         0932
    CSTL-011    SANDERS BR AT S-25-50                                        10        0932
    CSTL-013    SAWMILL BR AT SC 165                                         9,10      0818
    CSTL-043    SAWMILL BR AT SC 78 E OF SUMMERVILLE                         9,10      0818
    CSTL-044    IRELAND CK AT S-29-116 5 1/2 MI N OF WALTERBORO              9         0906
    CSTL-068    ASHEPOO RVR AT SC 303 10 MI SSW OF WALTERBORO                17        0906
    CSTL-069    ASHEPOO RVR AT US 17 3.4 MI ESE OF GREEN POND                4         0906
    CSTL-075    BLACK CK AT CO RD 41 5 MI SW OF HAMPTON                      7         0932
    CSTL-085    PIER IN COOPER RVR AT END OF RICE MILL RD IN
                   PIMLICO                                                   10        0820
    CSTL-099    EAGLE CK AT SC 642 5 MI SSE OF SUMMERVILLE                   10        0818
    CSTL-102    ASHLEY RVR AT SC 165 4.8 MI SSW OF SUMMERVILLE               6,10      0818
    CSTL-108    SANDERS BRANCH AT SC RD 363                                  6         0932
    E-014        EDISTO RVR AT US 15 S OF ST GEORGE                          10        0908
    E-016        POLK SWP AT UNIMP RD S-18-180 2 MI S OF ST GEORGE           10        0908
    MD-001       BEAUFORT RVR AB BEAUFORT AT CHANNEL MARKER 231              6         0920
    MD-002       BEAUFORT RVR AT DRAWBRDG ON US 21                           6,10      0926
    MD-003       BEAUFORT RIR BL BEAUFORT AT CHANNEL MARKER 244              6,10      0926
    MD-004       BEAUFORT RVR AT JCT WITH BATTERY CK NR MARKER 42            6,10      0926
    MD-005       BEAUFORT RVR BL OUTFALL OF PARRIS ISL MB AT
                   BUOY 29                                                   17        0926
    MD-006       PORT ROYAL BTWN BUOY 25 & 24 W OF BAY PT ISLAND             2         0926
    MD-010      WHALE BR AT US 21                                            5         0920
    MD-013       MOUTH OF SKULL CK BTWN CHANNEL MARKERS 3 & 4
                   NEAR REDBO                                                17        0926
    MD-016       MOUTH OF MAY RVR 1.0 MI W OF CHANNEL MARKER 29              4         0926
    MD-025       ELLIOT CUT AT EDGE WTR DR (S-10-26 OFF HW 17)               11        0814
    MD-039       GOOSE CK AT S-08-136 BRIDGE                                 10        0810
    MD-116       BROAD RVR AT SC 170 7.5 MI SW OF BEAUFORT                   17        0926
    MD-117       CHECHESSEE RVR AT SC 170 10.5 MI SW OF BEAUFORT             17        0926
    MD-128       BEES CK AT SC 462 5.9 MI NE OF RIDGELAND                    17        0926
    MD-135      ASHLEY RVR AT SC 7 (N BRDG)                                  17        0818
    MD-172       BROAD RVR AT MOUTH OF ARCHER CK ON SW SIDE OF USMC          17        0926
    MD-175       CALIBOGUE SD AT MOUTH OF COOPER RVR NR RED BUOY 32          3,4       0926

    Station Selection Criteria

    1 = Influent to segment (sub-basin)           9 = Above major municipal area
    2 = Effluent to segment                      10 = Below major municipal area
    3 = Major streams at state lines             11 = Mouth of major tributary
    4 = Confluence of major streams              12 = Major water use area
    5 = Above a major industrial area            13 = Above major land use area
    6 = Below a major industrial area            14 = Below major land use area
    7 = Water Quality limited area               15 = Above a water intake
    8 = Major lake                               16 = Basic Water Monitoring Program
                                                17 = Other

                                            A-9

                      STREAM STATIONS FOR CHARLESTON - SECONDARY
                                    TRIDENT DISTRICT

    Station     Descriotion                                              Criteria   Basin

    MD-176      COLLETON RVR AT COLLETON NECK-AT JCT WITH
                  CHECHESSEE RV                                             17       0926
    MD-194      WHALE BR AT JCT WITH CAMPBELL'S CK-3/4 MI W OF
                  MD-010                                                    6        0920
    MD-206       STONO RIVER AT ABBAPOOLA CREEK                              12,14    0814
    MD-207       KIAWAH RIVER MOUTH AT STONO RIVER                           12,14    0814
    MD-208       STONO RIVER MOUTH AT BUOY 10 OFF SANDY PT                   12,14    0814
    MD-209       BOHICKET CK AT FICKLING CK                                  12,14    0902
    MD-210       BOHICKET CK MOUTH AT N EDISTO RVR                           12,14    0902
    MD-211      N EDISTO RVR MOUTH BTWN KIAWAH ISLAND & BOTANY
                  BAY ISL                                                   12,14    0902
    MD-242      ASHLEY RIVER, BETWEEN LEEDS AVENUE BOAT RAMP
                  AND MOUTH OF CHURCH CK.                                   10       0818
    ST-005      N SANTEE RVR AT US 17                                        2        0802
    ST-007      WALKER SW AT US 52 2.5 MI S ST STEPHENS                      17       0820

    Station Selction Criteria

    1 = Influent to segment (sub-basin)           9 = Above major municipal area
    2 = Effluent to segment                      10 = Below major municipal area
    3 = Major streams at state lines             11 = Mouth of major tributary
    4 = Confluence of major streams              12 = Major water use area
    5 = Above a major industrial area            13 = Above major land use area
    6 = Below a majQr industrial area            14 = Below major land use area
    7 = Water Quality limited area               15 = Above a water intake
    8 = Major lake                               16 = Basic Water Monitoring Program
                                                17 = Other

                                           A-10

                                                                     4,,~~~~~~~~~~~~~4

                                                                                                                                   to~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~E

                                                                                                                                                44~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~ 0

    Secondary Stream Monitoring Stations

                             Trident District

                         STREAM STATIONS FOR COLUMBIA - PRIMARY
                               CENTRALS MIDLANDS DISTRICT

    Station      DescriDtion                                              Criteria   Basin

    B-054        ENOREE RVR AT S-36-45 3.5 MI AB JCT WITH
                  BROAD RVR                                                 2,11,16  0860
    B-080        BROAD RIVER DIVERSION CANAL AT COLA WATER PLANT             1,2,15   0850
    B-236        BROAD RVR AT SC 213 2.5 MI SW OF JENKINSVILLE               1,16      0850
    B-280        SMITH BR AT N MAIN ST IN COLA                               7,10      0850
    B-327       MONTICELLO LK-LOWER IMPOUNDMENT BETWEEN LARGE
                   ISLANDS                                                   12       0852
    B-328       MONTICELLO LK-UPPER IMPOUNDMENT AT BUOY IN MIDDLE
                  OF LAKE                                                   12        0852
    C-001        GILLS CK AT BRDG ON US 76 (GARNERS FERRY ROAD)              7         0824
    C-007        CONGAREE RVR AT US 601                                  1,2,6,10,16  0824
    C-008        CONGAREE CK AT US 21 AT CAYCE WATER INTAKE                  12,15    0824
    C-017        GILLS CK AT SC 48 (BLUFF ROAD)                              6,10      0824
    C-068        FOREST LAKE AT DAM                                          15        0824
    CSB-OO1L    CONGAREE RVR AT BLOSSOM ST (SALUDA RIVER)                  1,4,10,16  0824
    CSB-OO1R    CONGAREE RVR AT BLOSSOM ST (BROAD RIVER)                   1,4,10,16  0824
    CW-206      WATEREE RVR AT US 76 & 378                                1,2,5,6,16  0826
    CW-207       LK WATEREE AT END OF S-20-291                                8        0830
    CW-208       LK WATEREE AT S-20-101 11 MI ENE WINNSBORO                   8        0830
    CW-209       LK WATEREE AT SMALL ISLAND 2.3 MI N OF DAM                   8        0830
    CW-222      WATEREE RIVER 1.6 MI US CONFLUENCE WITH CONGAREE             2,6       0826
    S-042        BUSH RIVER AT SC 560 S OF JOANNA                            6,10      0842
    S-204        LK MURRAY AT DAM AT SPILLWAY (MARKER 1)                     8         0838
    S-223       BLACKSGATE BR LK MURRAY AT SC 391                            1,8       0838
    S-260       KINLEY CK AT S-32-36 (ST. ANDREWS RD.) IN IRMO               10        0838
    S-270        SALUDA RVR AT 1-20                                          2         0838
    S-273        LK MURRAY AT MARKER 166                                     8         0838
    S-274        LK MURRAY AT MARKER 143                                     8         0838
    S-279        LK MURRAY AT MARKER 63                                      8         0838
    S-280        LK MURRAY AT MARKER 102                                     8         0838
    S-290        CAMPING CK S-36-202 BLW GA PACIFIC                          6         0838
    S-294       TWELVE MILE CREEK AT U.S. ROUTE 378                          17        0838

    Station Selection Criteria

    1 = Influent to segment (sub-basin)          9 = Above major municipal area
    2 = Effluent to segment                     10 = Below major municipal area
    3 = Major streams at state lines            11 = Mouth of major tributary
    4 = Confluence of major streams             12 = Major water use area
    5 = Above a major industrial area           13 = Above major land use area
    6 = Below a major industrial area           14 = Below major land use area
    7 = Water Quality limited area              15 = Above a water intake
    8 = Major lake                              16 = Basic Water Monitoring Program
                                               17 = Other

                                            A-12

                        STREAM STATIONS FOR COLUMBIA - SECONDARY
                                CENTRAL MIDLANDS DISTRICT

    Station      DescriDtion                                              Criteria   Basin

    B-047        BROAD RVR AT SC 34 14 MI NE OF NEWBERRY                     6         0852
    B-072        DUNCAN CK AT US 176 1.5 MI SE OF WHITMIRE                   6         0860
    B-077        WINNSBORO BR BELOW PLANT OUTFALL                            10        0850
    B-110        LK ELIZABETH AT SPILLWAY ON US 21                           7,8       0850
    B-123       WINNSBORO BR AT US 321-AB WINNSBORO MILLS OUTFALL            5         0850
    B-145        LITTLE RVR AT S-20-60 3.1 MI SW OF JENKINSVILLE             17        0850
    B-316        CRANE CK AT S-40-43 UNDER 1-20 - N COLA                     7         0850
    C-005        SIX MI CK ON US 21 S OF CAYCE                               10        0824
    C-021        MILL CK AT SC 262                                           9         0824
    C-022        MILL CK AT US 76 AT PINEWOOD LK 8 MI SE OF COLA             9         0824
    C-025        LK CAROLINE SPILLWAY AT PLATT SPRINGS RD                    10        0824
    C-048        WINDSOR LK SPILLWAY ON WINSDOR LK BLVD                      7         0824
    C-058        LK INSPIRATION - ST MATTHEWS (FRONT OF HEALTH DEPT)         9         0804
    C-061        SAVANNAH BR AT S-32-72 1.7 MI NNW OF S CONGAREE             9,17      0824
    C-063        HALFWAY SWP CK AT S-09-43 3 MI E OF ST MATTHEWS             10        0804
    C-066        RED BANK CK AT S-32-244                                     9         0824
    C-067        RED BANK CK AT SANDY SPRINGS RD BTWN S-32-104 &
                   SC 602                                                    10        0824
    C-069        CEDAR CREEK AT S-40-66                                      14        0824
    CW-040       LITTLE WATEREE CK AT S-20-41 5 MI E OF WINNSBORO            10        0830
    E-034        BULL SWP CK AT CLVT ON UNIMP RD 1.1 MI NW OF
                   SWANSEA                                                   9         0914
    E-035        BULL SWP CK AT US 321 0.9 MI S OF SWANSEA                   10        0914
    E-101        LIGHTWOOD KNOT CREEK OFF LEXINGTON CO. RD 77
                   AT CITY OF BATESBURG WATER INTAKE                         10,15    0916
    S-044        SCOTT CK AT SC 34 SW OF NEWBERRY                            9         0842
    S-099        LITTLE RVR AT S-36-22 8.3 MI NW SILVERSTREET                11        0842
    S-102        BUSH RVR AT S-36-41 8.5 MI S OF NEWBERRY                    11        0842
    S-149        SALUDA RVR AT MEPCO ELECT. PLANT WATER INTAKE
                   2.8 MI SSE IRMO                                           15        0838
    S-150        LORICK BR AT PT UPSTRM OF JCT WITH SALUDA RVR               10        0838
    S-151        LORICK BR AT S-32-107 2 MI SSE IRMO                         10        0838
    S-152        SALUDA RVR JUST BELOW LK MURRAY DAM                         8         0838
    S-211        HOLLANDS LANDING LK MURRAY OFF S-36-26 AT END
                   OF S-36-3                                                 8         0838
    S-212        MACEDONIA LANDING LK MURRAY AT END OF S-36-26
                    MACEDONIA                                                8         0838
    S-213       ADAMS CAMP BR ON CO RD S-36-15 OFF S-36-26                   8         0838
    S-287        RAWLS CREEK AT S-32-107                                     10,14    0838

    Station Selection Criteria

    1 = Influent to segment (sub-basin)           9 = Above major municipal area
    2 = Effluent to segment                      10 = Below major municipal area
    3 = Major streams at state lines             11 = Mouth of major tributary
    4   Confluence of major streams              12 = Major water use area
    5 = Above a major industrial area            13 = Above major land use area
    6 = Below a major industrial area            14 = Below major land use area
    7 = Water Quality limited area               15 = Above a water intake
    8 = Major lake                               16 = Basic Water Monitoring Program
                                                 17 = Other

                                            A-13

                                                               C lis
                                                                                                                            f-a
                                                                                                                                     9?           C,
                                                                            715                                                                                              ed a r
                                                                                              lackst

                                                                                                       d A R                                                      M

                                                                                                             Water,

                                                                                                           hite Lit

                                       1/7 34

                                      inar s I
                                                             176                                                                                     ro LA

                                                                                    B      nti                                 i    oro Mill 1
                                         a apa

                                                                                                                             eway
                                                              (21 on w
                                            Hel
            3                                                                    w               annons 269
                                                                    rna

                                                               76,
                                                               -                                                                                                                    T've

                                                       osperi y                             n                                                                         'w
                               S                                                            e IBEFw
                                                                                            R C                   0
                                                                                                                                       Figin
                                                          S     m  n
                                                             1) 21 K   11'

                                                                                                                                                              Yk

                                                                                                                St

                                                                                                                                             C,
                                                                                   S-2
                                                                                                                                                                        0

                                                                                    378                   est CQI
                                                                                                                   0

                                                                                                                                                N
                                                                                                  pr
                                                                                             ed Bank 76
                                                                                                                   a

                                                                                                          Pin

                                                                                                        C,
                                                       one a

                                                                                                                   26

                                                                          drna                                   6                                      7 222

                                                                                             lion
                                                                                                                                              ort M(tte
                                                                                                                                                                       Pi
                                                                                                                    I 21
                                                                                                       3                                                    0
                                                                                                                                          H

                                                                                                                                   StMatt
                                                                                                      17
                                                                                      r

                                                                                                          North
                                                                                                           E                         n               iso
                                                                                                     rG I3

                                                                                                                                   t
                                                                                                                                   21

                                                                                                                                          n e

    Primary Stream Monitoring Stations

          Central Midlands District

                                          C   I'l        C    ~_

                                                                    kst ~ ~ ~ ~   ~    ~    ~     ~    ~ ~ eg  Id a

    Secondary~~~~~~~~~~~~~~~~~~~~~~~~~~~ Stream Montoin  Stti1                                     IE N
                                                          own~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

                                                                                Water~~~~~~~~~~~~~~~~~~

                         STREAM STATIONS FOR FLORENCE - PRIMARY
                                    PEE DEE DISTRICT

    Station      Descriotion                                              Criteria   Basin

    MD-073      SAMPIT RVR OPP AMER CYANAMID CHEM CO                        6         0702
    MD-075      SAMPIT RVR BTWN MOUTHS OF PORTS CK & PENNY
                  ROYAL CK                                                 5         0702
    MD-077      SAMPIT RVR AT US 17                                         5,6       0702
    MD-080      WINYAH BAY AT JCT OF PEE DEE & WACCAMAW AT
                  MARKER 92                                                2,4,16   0702
    MD-124      WACCAMAW RVR AT SC 9 7.0 MI W OF CHERRY GROVE               1         0716
    MD-127       INTRACOASTAL WTRWAY AT SC 544 7.5 MI SW OF
                  MYRTLE BEACH                                             2,10      0715
    MD-146      WACCAMAW RVR & ICWW 1 MI BL JCT-AT BUCKSPORT
                   LANDING                                                  2,4       0716
    MD-149      WHITES CK 100 YDS UPSTRM OF JCT WITH SAMPIT RVR             10        0702
    MD-162       LITTLE RVR AT S END OF ISL DUE E OF TOWN (IN RVR)          1         0715
    PD-012      PEE DEE RVR AT US 1 NE CHERAW                               1         0726
    PD-021      BLACK CK AT S-16-18 1 MI NNE HARTSVILLE                     5         0725
    PD-023      BLACK CK AT S-16-13 5.5 MI NE HARTSVILLE                    6         0725
    PD-025      BLACK CK AT S-16-133 2.25 MI NE OF DARLINGTON               6         0725
    PD-027      BLACK CK AT S-16-35 5.5 MI SE DARLINGTON                    6,10,16  0725
    PD-028      PEE DEE RVR AT SC 34 11 MI NE DARLINGTON                    2,16      0726
    PD-038      LUMBER RVR AT US 76 AT NICHOLS                              2,16      0722
    PD-041      LYNCHES RVR AT US 52 NEAR EFFINGHAM                         1         0728
    PD-043      POCOTALIGO RVR AT S-14-50 9.5 MI NE MANNING                 2         0714
    PD-052      LITTLE PEE DEE AT S-34-60                                   2         0720
    PD-061      PEE DEE RVR AT US 701 2.75 MI NE YAUHANNAH                  1,16      0702
    PD-069      LITTLE PEE DEE RVR AT SC 57 11.5 MI NW DILLON               1         0720
    PD-076      GREAT PEE DEE RVR AT US 378                                 6,17      0724
    PD-091      POCOTALIGO RVR AT US 15 3.5 MI S SUMTER                     1,9       0714
    PD-170      BLACK RVR AT SC 51 11.6 MI NE OF ANDREWS                    1         0706
    PD-189      LITTLE PEE DEE RVR AT US 378 12 MI W CONWAY                 2         0718
    PD-202      POCOTALIGO RVR AT S-43-32 9 MI SSE OF SUMTER              6,7,10,16  0714
    PD-227      BLACK RVR AT S-45-35 8.6 MI NW OF KINGSTREE                 1,2       0712
    PD-281      LYNCHES RVR AT S-21-49 5 MI NW JOHNSONVILLE                 2,9       0728
    PD-325      BLACK RVR AT S-22-489 4 MI NE GEORGETOWN                    2         0706
    PD-332      SPARROW SWAMP AT S-21-55 NR JOHNSONS CROSSROADS             2,14      0730
    ST-024      LK MARION AT END OF S-14-64 AT CAMP BOB COOPER              8         0804

    Station Selection Criteria

    1 = Influent to segment (sub-basin)    9 = Above major municipal area
    2 = Effluent to segment                 10 = Below major municipal area
    3 = Major streams at state lines        11 = Mouth of major tributary
    4 = Confluence of major streams         12 = Major water use area
    5 = Above a major industrial area       13 = Above major land use area
    6 = Below a major industrial area       14 = Below major land use area
    7 = Water Quality limited area          15 = Above a water intake
    8 = Major lake                          16 = Basic Water Monitoring Program
                                            17 = Other

                                          A-16

    0       ~  ~   ~~~~~~~~~~~ ~~~~I

                   ,~~~~~~l

                      Primary Stream Monitoring Stations

                                 Pee Dee District

                        STREAM STATIONS FOR FLORENCE - SECONDARY
                                     PEE DEE DISTRICT

    Station      Descriotion                                               Criteria   Basin

    MD-074       SAMPIT RVR AT CHANNEL MARKER #30                             4         0702
    MD-076N      TURKEY CK S-22-42 SW OF GEORGETOWN                           6         0702
    MD-085       INTRACOASTAL WTRWAY AT PT 3 MI N OF BRDG ON
                   US 501                                                     10       0715
    MD-087       INTRACOASTAL WTRWAY JUST N OF BRDG ON US 501                 9,10      0715
    MD-088       INTRACOASTAL WTRWAY 1 MI S OF BRDG ON US 501                 9,10      0715
    MD-089       INTRACOASTAL WTRWY 2 MI S OF BRDG ON US 501                  9,10      0715
    MD-091       INTRACOASTAL WTRWY 4 MI N OF BRDG ON US 501                  9,10      0715
    MD-107       KINGSTON LK NR PUMP STA ON LAKESIDE DR CONWAY                10        0716
    MD-110       WACCAMAW RVR AT US 501 BY PASS AROUND CONWAY                 17        0716
    MD-111       WACCAMAW RVR AT COX'S FERRY ON CO RD 110                     10        0716
    MD-125       INTRACOASTAL WTRWY (LITTLE RVR) ON SC 9 (US 17)              9         0715
    MD-136       WACCAMAW RVR 1/4 MI UPSTRM OF JCT WITH INTRA-
                   COASTAL WTRWY                                              4        0716
    MD-137       WACCAMAW RVR NR MOUTH OF BULL CK AT CHANNEL
                   MARKER 50                                                  9        0702
    MD-138       WACCAMAW RVR AT CHANNEL MARKER 57                            10        0702
    MD-158       CRABTREE CK AT LONG ST BL OUTFALL OF CONWAY #1
                    POND                                                     10        0716
    PD-014       CROOKED CR AT S-35-43                                        10        0726
    PD-015       PEE DEE RYR AT US 15                                         6        0726
    PD-016       PANTHER CK AT S-35-27                                        10       0720
    PD-017A      MCCLAUREN'S MILL POND SC 381                                 10       0720
    PD-029E      LITTLE PEE DEE RVR AT S-17-23                                5        0720
    PD-030      MAPLE SWP AT SC 57                                            10       0720
    PD-030A      LITTLE PEE DEE RVR BELOW JCT WITH MAPLE SWP                  10       0720
    PD-031       BUCK SWP AT S-17-33                                          10       0720
    PD-035       JEFFERIES CK AT SC 327 AT CLAUSSEN                           10       0724
    PD-036       CATFISH CK AT US 76                                          9        0724
    PD-037       BROWN SWP AT S-34-31                                         10       0718
    PD-039       GREEN SWP AT S-43-33                                         9        0714
    PD-042       LITTLE PEE DEE RIVER AT US 501                               10       0718
    PD-044       BLACK RVR AT US 52 AT KINGSTREE                              5,9       0710
    PD-045       BLACK RVR AT SC 377 AT BRYAN'S CROSS ROADS                   6        0710
    PD-055       LITTLE PEE DEE RVR AT SC 9                                   5,6      0720
    PD-072       SPARROW SWP AT S-16-697 2.5 MI E OF LAMAR                    10       0730
    PD-081       PRESTWOOD LK AT US 15                                        8        0725
    PD-085       LYNCHES LK AT US 378                                         9        0728

    Station Selection Criteria

    1 = Influent to segment (sub-basin)           9 = Above major municipal area
    2 = Effluent to segment                      10 = Below major municipal area
    3 = Major streams at state lines             11 = Mouth of major tributary
    4 = Confluence of major streams              12 = Major water use area
    5 = Above a major industrial area            13 = Above major land use area
    6 = Below a major industrial area            14 = Below major land use area
    7 = Water Quality limited area               15 = Above a water intake
    8 = Major lake                               16 = Basic Water Monitoring Program
                                                 17 = Other

                                            A-18

                        STREAM STATIONS FOR FLORENCE - SECONDARY
                                     PEE DEE DISTRICT

    Station      DescriDtion                                              Criteria   Basin

    PD-086A      LYNCHES LK ON SC 341                                        10        0728
    PD-087       LYNCHES LK AT SC 341 2.6 MI W OF JOHNSONVILLE               9         0728
    PD-097      CATFISH CANAL AT S-34-38 IN MARION                           7         0724
    PD-098      TURKEY CK AT LIBERTY ST IN SUMTER ABOVE
                    SANTEE PRI                                               5,9       0714
    PD-103       HIGH HILL CK AT US 52 ON CO LINE                            9         0725
    PD-106       LYNCHES RVR ON 1-20 4 OR 5 MI BELOW
                   BISHOPVILLE SEPTIC                                        10        0730
    PD-107       CROOKED CK AT SC 9 IN BENNETTSVILLE                         9         0726
    PD-112       COUSAR BR 1/4 MI BELOW BISHOPVILLE FINISHING CO             6         0730
    PD-115       POCOTALIGO RVR AT 3RD BRDG N OF MANNING ON US 301           7         0714
    PD-116       BLACK RVR AT S-14-40 E OF MANNING                           17        0712
    PD-137       SNAKE BR AT WOODMILL ST-HARTSVILLE                          6         0725
    PD-141      60" TILE DISCHARGING TO DITCH ACROSS RD AT
                   DARLINGTON STP                                            10        0725
    PD-143      KINGSTREE SWP CANAL AT S-45-44 2.1 MI NNE
                   KINGSTREE                                                 6         0710
    PD-159       BLACK CK AT S-16-23 4.7 MI NW OF HARTSVILLE         -       6         0725
    PD-168       BIG SWP AT S-21-360 1.1 MI W OF PAMPLICO                    9         0728
    PD-169       BIG SWP AT US 378 & SC 51 0.9 MI W OF SALEM                 7         0728
    PD-172       BLACK MINGO CK AT SC 41 14 MI NE OF ANDREWS                 2,14      0708
    PD-176       LAKE SWP AT S-26-99 5.9 MI NW OF AYNOR                      17        0718
    PD-177      CHINNERS MILL BR AT S-26-24 1.9 MI SSE AYNOR                 10        0718
    PD-186       BLACK RVR AT US 76 1.5 MI NE OF MAYESVILLE                   9        0712
    PD-187       SMITH SWP AT US 501 1.9 MI SSE OF MARION                    10        0724
    PD-190      MAIDEN DOWN SWP AT SC 41 3.5 MI N OF MULLINS                 6,10      0720
    PD-201       ROCKY BLUFF SWP AT S-43-41 8.1 MI E OF SUMTER               10        0712
    PD-203       PUDDING SWP AT SC 527 8.1 MI NW OF KINGSTREE                10,11    0712
    PD-229      NEWMAN SWP AT S-16-449 0.9 MI NE OF LAMAR                    9         0730
    PD-230      MIDDLE SWP AT SC 51 3.5 MI SSE OF FLORENCE                   10        0724
    PD-231      JEFFRIES CK AT UN# RD 3.3 MI ESE OF CLAUSSEN                 17        0724
    PD-236       PEE DEE RVR 2.5 MI DWNSTREM FROM MOUTH OF
                   JEFFRIES CK                                               6,10      0724
    PD-239      NASTY BR AT S-43-251 7.5 MI SW OF SUMTER                     6         0714
    PD-255      JEFFRIES CK AT SC 340 6.8 MI SSW OF DARLINGTON               5         0724
    PD-256      JEFFRIES CK AT S-21-112 4.8 MI W OF FLORENCE                 6         0724
    PD-258      SNAKE BR AT RR AVE IN HARTSVILLE                             6         0725
    PD-268      SONOVESTA CLUB HARTSVILLE OFF DOCK OF PRESTWOOD LK           8         0725
    PD-306       PANTHER CK AT US 15 OUTSIDE MCCOLL                          9         0720
    PD-310       BEAVERDAM CK AT S-17-30 8 MI E OF DILLON                    17        0722
    PD-319       LYNCHES RIVER AT SC 403                                     17        0730
    PD-320      SMITH SWP AT S-34-19 1 MI E OF MARION                        9         0724
    PD-321      CATFISH CANAL AT MARION BYPASS 2 MI SW OF MARION             10        0724
    PD-330       BLACK CK AT HWY 15 BYPASS                                   10        0725
    ST-018      TAWCAW CK AT S-14-127 3.2 MI S OF SUMMERTON                  10        0804

                                             A-19

                                       A                 '''   'b ~~~~~~~~~j

    -~~~~~~~~~~~~~~~~~                I -

                                                                                 Secondary Stream Monitoring Stations

                                                                                                 Pee Dee District

                        STREAM STATIONS FOR GREENVILLE - PRIMARY
                                 APPALACHIA II DISTRICT

    Station     Descriotion                                              Criteria   Basin

    B-008       TYGER RVR AT S-42-50 E. WOODRUFF                            2,4       0866
    B-021        FAIRFOREST CK AT SC 56                                      1,6,10   0864
    B-026       N PACOLET RVR AT S-42-956 6.5 MI E LANDRUM                  1         0868
    B-041       ENOREE RVR AT SC 49 SE OF WOODRUFF                          2         0862
    B-148       MIDDLE TYGER RVR AT SC 14 2 MI SSW GOWANSVILLE              1         0866
    B-317       S TYGER RVR AT SC 253 BL TIGERVILLE                         1         0866
    B-321       TRIB TO FAIRFOREST CK 200 FT BL S-42-65                     6         0864
    BE-O001     TRIB TO ENOREE AT UNNUM RD W US 25 N TRAVELERS REST         1         0862
    BL-001      LAWSONS FORK CK AT S-42-108                                 6,10      0868
    S-007       SALUDA RVR AT SC 81 SW OF GREENVILLE                        1         0847
    S-013       REEDY RVR AT S-23-30 3.9 MI SE GREENVILLE                   6,7,10   0846
    S-018       REEDY RVR AT S-23-448 1.75 MI SE CONESTEE                   6,7,10   0846
    S-021       REEDY RVR AT S-23-06 E WARE SHOALS                          2         0846
    S-034       LITTLE RVR AT US 76 BUS IN LAURENS ABOVE STP                6,9       0842
    S-073       REEDY RVR AT UN# RD OFF US 276 .75 MI E
                    TRAVELERS REST                                          1         0846
    S-088       N SALUDA RVR AT S-23-42 5.2 MI NNW TIGERVILLE               1,12      0848
    S-125       SALUDA RVR AT US 25 BYPASS 1.5 MI ESE WARE SHOALS           2,16      0844
    S-138       REEDY RVR AT FOOTHILLS RD OFF US 25 1.9 MI
                    SW TRVLS REST                                           6         0846
    S-250       SALUDA RVR AT FARRS BRDG ON SC 183 7 MI NE EASLEY           2         0848
    S-291       TABLE ROCK RESERVOIR AT WATER INTAKE                        15        0848
    S-292       NORTH SALUDA RESERVOIR AT WATER INTAKE                      15        0848
    S-296       LAKE RABON 300 FT US OF DAM                                 8         0844
    SV-031      ROCKY RVR AT S-04-263 2.7 MI SE ANDERSON AT STP             10        0131
    SV-098       LAKE RICHARD B. RUSSELL AT SC 72 3.1 MI SW
                   CALHOUN FALLS                                            8,15      1308
    SV-100      SAVANNAH RVR AT SC 181 6.5 MI SW STARR                      1,3       1310
    SV-121      LK SECESSION AT HWY 184                                     8         1310
    SV-122      DAM AT LK SECESSION                                         8         1310
    SV-227      N FORK CHATTOOGA RVR AT SC 28 3.5 MI NW MT REST             1,3       1312
    SV-230      BIG EASTATOE CREEK AT S-39-143                              17        1314
    SV-249      SENECA RVR AT SC 183 3.8 MI WSW SIX MILE                    8         1312
    SV-288      HARTWELL RESERVOIR AT SC 24 9.7 MI WNW OF ANDERSON          8         1312
    SV-311      LK KEOWEE AT SC 188 - CANE CK ARM 3.5 MI NW SENECA          8         1314
    SV-312      LK KEOWEE AT SC 188 - CROOKED CK ARM 4.5 MI N SENECA    8             1314
    SV-313      LK JOCASSEE AT LANDING AT S-37-25 5.0 MI NE SALEM           8         1312
    SV-322      HARTWELL RES AT S-37-54 (CONEROSS CK ARM)                   8,10      1312

    Station Selection Criteria

    1 = Influent to segment (sub-basin)          9 = Above major municipal area
    2 = Effluent to segment                     10 = Below major municipal area
    3 = Major streams at state lines            11 = Mouth of major tributary
    4 = Confluence of major streams             12 = Major water use area
    5 = Above a major industrial area           13 = Above major land use area
    6 = Below a major industrial area           14 = Below major land use area
    7 = Water Quality limited area              15 = Above a water intake
    8 = Major lake                              16 = Basic Water Monitoring Program
                                                17 = Other

                                            A-21

                       STREAM STATIONS FOR GREENVILLE - SECONDARY
                                 APPALACHIA II DISTRICT

    Station      DescriDtion                                              Criteria   Basin

    B-005        SOUTH TYGER RVR AT S-42-63                                  10        0866
    B-012        MIDDLE TYGER RVR AT S-42-63                                 6         0866
    B-019        JIMMIES CK AT S-42-201 2 MI E OF WOODRUFF                   10        0866
    B-020        FAIRFOREST CK AT US 221 S OF SPARTANBURG                    6         0864
    B-028        PACOLET RVR AT S-42-55 BL JCT OF N & S PACOLET R            4         0868
    B-035        BIG DURBIN CK ON S-42-160 3 MI E OF SIMPSONVILLE            10        0862
    B-037        ENOREE RVR AT S-42-118 SW OF WOODRUFF                       7         0862
    B-038       MILL CK AT S-42-118 1 1/4 MI SW WOODRUFF                     10        0862
    B-097        DURBIN CREEK AT SC 418                                      10        0862
    B-099A       ON # 1 INLET LK LANIER IN GREENVILLE CO                     8         0868
    B-099B      AT DAM LK LANIER IN GREENVILLE CO                            8         0868
    B-103        SPIVEY CK AT S-42-208 2.5 MI SSE OF LANDRUM                 10        0868
    B-113        RT BK OF DAM AT BOWEN LK ON RD S-42-213 NE
                    OF INMAN                                                 8         0868
    B-149        S TYGER RVR AT SC 14 2.9 MI NNW OF GREER                    8,12      0866
    B-162       TYGER RVR AT US 221 7.6 MI NNE OF WOODRUFF                   4         0866
    B-163A       PACOLET RVR AT BRDG ON S-42-757 2.9 MI NW
                    OF COWPENS                                               6,10      0868
    B-164        FAIRFOREST CK AT S-42-651 3.5 MI SSE OF
                    SPARTANBURG                                              6,10      0864
    B-186        MOUNTAIN CK AT S-23-335                                     6         0862
    B-191        POTTER BR ON RD 30 BL OUTFALL FROM HOUSING
                    PROJ COWPENS                                             10       0868
    B-192        PRINCESS CREEK AT COUNTY ROAD 540                           6         0862
    B-219        N TYGER RVR AT US 29 7.2 MI W OF SPARTANBURG                5         0866
    B-221        LAWSONS FK CK AT S-42-40 BL INMAN MILL EFF                  6         0868
    8-231        BEARDS CK AT US 276 3.7 MI NNE OF CLINTON                   6,10      0860
    B-235        KELSEY CK AT S-42-321                                       6         0864
    8-241        GILDERS CK AT S-23-142 2.75 MI ENE OF MAULDIN               10        0862
    B-242       TRIB TO FAIRFOREST CK 50 FT AB S-42-65 4 MI
                    NW OF SPARTANBURG                                        6         0862
    B-259        LITTLE BUCK CK AT UN# CO RD 2.3 MI SW OF CHESNEE            6,10      0868
    B-263       S TYGER RVR AT SC 290 3.7 MI E OF GREER                      10        0866
    B-277        LAWSONS FORK CK AT S-42-218 2.7 MI SSE OF INMAN             5,10      0868
    B-278        LAWSONS FORK CK AT UN# RD BL MILLIKEN CHEM                  6         0868

    Station Selection Criteria

    1 = Influent to segment (sub-basin)           9 = Above major municipal area
    2 = Effluent to segment                      10 = Below major municipal area
    3 = Major streams at state lines             11 = Mouth of major tributary
    4 = Confluence of major streams              12 = Major water use area
    5 = Above a major industrial area            13 = Above major land use area
    6 = Below a major industrial area            14 = Below major land use area
    7 = Water Quality limited area               15 = Above a water intake
    8 = Major lake                               16 = Basic Water Monitoring Program
                                                 17 = Other

                                            A-22

                                                                                            it Res

                                                                                                                    OW4,
                                                                      ass ramlin

                                                                                                                         0     Sprin

                                                         k 13                                      t-",                                                    Mi
                                                                                   r Fe
                                                                                  co
                                                                  y                                                                                                                                      �rse
                                              LAKE fton
                                        oc           JOGA                 n                                                                                                                                              RTA
                                                                                                                                          01
                                                                                                                                             Colet
                                                                                       am
                                                                            Sh Par a

                                                     n
                                in R oil x
                                                                                                                r   Spri- S
                                                                                                                                  Pauline

                                                                                               'Five zer nn
                                                         ile 007 oil

                                         n                     C
                             Wa r

                                                   RI
              L

                                                                                                Fou               S
               II fik
                                                                                               co mmurl                                                         r
                                                           n                                                          00

                                                                                                 k Sho In
                                                                 Labe G                                                                                           gsrrior
                                                            a Franc
                                           r Sandy Ln
                                 Oa arks

                                                                                                                                         reek

                                                           DER

                                                                                                               -a en

                                                                                                                  I y a Is

                                       RESERVOI

                                                                                                       A2
                                                                                                   r                                   rlo(
                                                        A
                                                                           21,
                                                                                               C.

                                                                             YA.

                                                                                                                        3YR

                                                               M

    Primary Stream Monitoring Stations Lo een                                                                                                                                                                                                   r

           Appalachia 11 District S

                                                                                                         22

                                                                           houn

                                                                                                      r ay

                                                                                M Car el

                                                                               A N

                                               X",                                         B-
                                                                   Co ills
                                                                           0
                                                   Falls
                                                               7'                               OW4
                                                                        cam n

                                                                                   Sprin

                                   k Bottom L   n a Fe

                            AKE y Lit,
                           JOCA Vale
                      cc it u 9                                                          S - 0 0
                                                  G   E
                 0                                                                                  tf a
                                                       Ha a
                                                Sh

                                                    S                                                                         uc
                                                                   p I M
                                                                             rin                    tation Jo
                                           Aria Pauline

                              r   E   x a I
                              DA Ti  F I nn
        0 4
                               C
               far 4
              w                                                           N Id M fill f

    L
                                                                UV
     b Lake F-ount n Du Wn
                    d                                                                                                    v                         nts
                                                              CD rommuni
              in S 35 Cro

                                                                                d
                         V-0 14 Lab ork Shoo
                1.                                                                                                                            Gr
                 -3 ena (a
                                      dy S
                 us S!                                                                                                                                        its

                                                                                            Creek

                                                        89

                                                                                  ydia    S no

                      RESER I
                                        Af
                                                             needs
                                         la S-09
                                                                               riot MO

                                                                                 EK

                                       Itlrnes
                                        ,on !B

                                                               ob
                                          I
                                                        e

    Secondary Stream Monitoring Stations tail
                                                                     s H
                                                 or
           Appalachia II District
                                                                    dj

                                                oun a IS
                                                 -0 2-
                                                                   r ley

                       STREAM STATIONS FOR GREENVILLE - SECONDARY
                                 APPALACHIA II DISTRICT

    Station      Descriotion                                              Criteria   Basin

    B-301        PAGE CK AT S-42-1258 1.7 MI SE LANDRUM                      10        0868
    B-302       HEADWTR OF BOWEN LK AT S-42-866 1 MI SE
                  CAMPOBELLO                                                6,8       0868
    B-315       TRIB TO N TYGER RVR AT UN# RD BL JACKSON #2 EFF              6         0866
    BE-007       ROCKY CK AT BRDG IN BATESVILLE 1 MI AB JCT
                  WITH ENOREE                                               6,10      0862
    BE-009       BRUSHY CK AT S-23-164                                       10,11    0862
    BE-015       ENOREE RVR AT CO RD 164                                     6,10      0862
    BE-018       ENOREE RVR AT SC 75                                         6,10      0862
    BE-020       HORSE PEN CK AT BRDG 1/4 MI AB JCT WITH
                   ENOREE RVR ON RD 143                                      10        0862
    BE-024      ENOREE RVR AT US 221                                         10        0862
    BE-035      BRUSHY CKAT HOWELL RD (UN#) APPROX 5
                  MI NE OF GREENVILLE                                       7         0862
    BE-039       BEAVERDAM CK AT RD 1967                                     10        0862
    BE-040      GILDER CK AT SC 14-AB GILDER CK PT                           6,10      0862
    BL-005       LAWSONS FORK CK AT S-42-79 AT VALLEY FALLS                  6         0868
    BP-001       PACOLET RVR AB DAM AT PACOLET MILLS                         6,10      0868
    S-004       N SALUDA RVR AT BRDG AB JCT WITH SALUDA RVR
                   E OF SC 186                                               14       0847
    S-005        BR OF GEORGES CK AT S-39-192, 2.6 MI NE EASLEY              10        0847
    S-010        BROAD MOUTH CK AT US 76                                     10        0847
    S-022        REEDY FORK OF LK GREENWOOD AT S-30-29                       8         0844
    S-035        LITTLE RVR AT S-30-37 SE OF LAURENS                         6,10      0842
    S-063       GEORGES CK AT US 123A - EASLEY                               6,10      0847
    S-067        BRUSHY CK ON GREEN ST EXT BL DUNEAN MILL
                   ON SC 20                                                  6         0846
    S-072        REEDY RVR ON HWY 418 AT FORK SHOALS                         7         0846
    S-084        BRUSHY CK AT S-04-52 8.3 MI N WILLIAMSTON                   10        0847
    S-087       SOUTH SALUDA RIVER AT CO RD 101                              14,17    0848
    S-091        ROCK CK AT S-23-453 3.5 MI SW OF SIMPSONVILLE               10        0846
    S-096        RABON CK AT S-30-54 8.8 MI NW CROSS HILL                    14,17    0844
    S-097       CANE CK AT SC 72 3.1 MI SW CROSS HILL                        8,14      0844
    S-119       SALUDA RVR AT S-04-178 3.2 MI SE WILLIAMSTON                 10        0847
    S-135       NORTH CK AT JCT WITH US 76 2.8 MI W OF CLINTON               7         0842
    S-161       TRIB TO SALUDA RVR ON DURHAM ST BL CAROLINA PLATING          6         0847
    S-168        LAUREL CK AT US 276 BELOW FIBER IND                         6         0846
    S-171       GROVE CK AT UN# RD BELOW J P STEVENS ESTES PLANT             6         0847
    S-178        HUFF CK AT SC 418 1.6 MI NW FORK SHOALS                     6         0846
    S-231        SPAIN CK AT SC 288 BELOW GAYLEY MILLS                       6         0848
    S-252       MIDDLE SALUDA RVR AT SC 288 2.3 MI WSW SLATER                11,14    0848
    S-264        LANGSTON CK AT SC 253                                       6         0846
    S-267       TRIB TO SALUDA RVR 350 FT BL W PELZER STP
                   ON S-23-53                                                10        0847
    S-289        BROAD MOUTH CK AT S-04-267 - BL BELTONS
                MARSHALL PLANT                                              10        0847
    SV-004      CONEROSS CK AT SC 59                                         10        1312

                                            A-25

                       STREAM STATIONS FOR GREENVILLE - SECONDARY
                                  APPALACHIA II DISTRICT

    Station      Descriotion                                               Criteria   Basin

    SV-015       TWELVE MI CK AT S-39-51 N OF NORRIS                          15        1312
    SV-017       18 MI CK AT UNNUMBERED CO RD 2.25 MI SSW OF EASLEY           10        1312
    SV-037       BETSY CK AT S-04-259 BL FIBERGLAS OUTFALL                    6         1310
    SV-041       ROCKY RVR AT S-04-152 BL ROCKY RVR STP                       10        1310
    SV-043       CHEROKEE CK AT S-04-318 4 MI S OF BELTON                     10        1310
    SV-052       SAWNEY CK AT CO RD 1.5 MI SE OF CALHOUN FALLS                10        1308
    SV-053B      BLUE HILL CK ON S MAIN ST ABBEVILLE                          6         1308
    SV-106       MARTIN CK AT S-37-65 N OF CLEMSON                            8,10      1312
    SV-107       TWELVE MI CK AT SC 133                                       6,8       1312
    SV-111       THREE & TWENTY CREEK AT CO RD 280                            6         1312
    SV-135       18 MI CK AT S-39-93 SW OF CENTRAL                            6,10      1312
    SV-136       FIRST CK AFTER LEAVING CENTRAL AT CLVT ON
                   MAW BRDG RD                                                10        1312
    SV-137       12 MI CK AT S-39-337                                         6         1312
    SV-139       CUPBOARD CK AB BREAZEALE ST PLANT & BL BLAIR HILL
                    AT S-04-733                                               6         1310
    SV-140       CUPBOARD CK AT S-04-209 BL EFF FROM BELTON
                    2 PLANT                                                   6,10     1310
    SV-141       BROADWAY CK AT US 76 BTWN ANDERSON & BELTON                  14        1310
    SV-181       6 & 20 CK AT S-41-29 8.2 MI SE OF PENDLETON                  14        1312
    SV-200       TUGALOO RVR AT US 123 7.0 MI SW OF WESTMINSTER               3,8       1312
    SV-203       LITTLE RVR AT S-37-24 7.1 MI NE OF WALHALLA                  17        1314
    SV-206       N FORK 12 MI CK AT US 178 2.9 MI N OF PICKENS                9         1312
    SV-236       H'WELL RESERVOIR AT S-37-184 6.5 MI SSE OF SENECA            8         1312
    SV-239       GOLDEN CK AT S-37-222 1.2 MI NW OF LIBERTY                   10        1312
    SV-241       WOODSIDE BR AT US 123 1.5 MI E OF LIBERTY                    10        1312
    SV-245       18 MI CK AT S-39-27 3.3 MI S OF LIBERTY                      6,10      1312
    SV-282       12 MI CK AT S-39-273 2.8 MI SSW OF PICKENS                   6,10      1312
    SV-301       NORRIS CK AT S-37-435 1 MI S OF WESTMINSTER                  10        1312
    SV-303       LK KEOWEE AT HEADWTR AT END OF S-37-202
                    1.5 MI SE OF W UNION                                     10        1314
    SV-308       E FK OF CHATTOOGA RVR AT SC 107 2 MI S OF ST LINE            3         1312
    SV-316       BIG GENEROSTEE CK AT CO RD 104                               10        1310

    Station Selection Criteria

    1 = Influent to segment (sub-basin)            9 = Above major municipal area
    2 = Effluent to segment                       10 = Below major municipal area
    3 = Major streams at state lines              11 = Mouth of major tributary
    4 = Confluence of major streams               12 = Major water use area
    5 = Above a major industrial area             13 = Above major land use area
    6 = Below a major industrial area             14 = Below major land use area
    7 = Water Quality limited area                15 = Above a water intake
    8 = Major lake                                16 = Basic Water Monitoring Program
                                                 17= Other

                                            A-26

                        STREAM STATIONS FOR LANCASTER - PRIMARY
                                    CATAWBA DISTRICT

    Station     Descriotion                                              Criteria   Basin

    B-042       BROAD RVR AT SC 18 4 MI NE GAFFNEY                          1         0856
    B-044       BROAD RVR AT SC 211 12 MI SE OF GAFFNEY                     2         0856
    B-046       BROAD RVR AT SC 72/215/121 3 MI E OF CARLISLE               2,16      0854
    B-048       PACOLET RVR AT SC 105 6 MI AB JCT WITH BROAD RVR            2,11      0868
    B-051       TYGER RVR AT SC 72 5.5 MI SW OF CARLISLE                    2         0864
    CW-002      ROCKY CK AT S-12-335 3.5 MI E OF CHESTER                    6,10      0832
    CW-008      FISHING CK AT SC 223 NE RICHBURG                            7         0832
    CW-013      SUGAR CK AT SC 160 E OF FORT MILL                           7         0836
    CW-016      CATAWBA RVR AT SC 9 AT FT LAWN                              2,16      0834
    CW-016F     FISHING CK RES 2 MI BL CANE CREEK                           5,8       0832
    CW-023      CROWDERS CK AT S-46-564 NE CLOVER                           7         0836
    CW-029       FISHING CK AT SC 49 NE YORK                                1,5,6    0832
    CW-041      CATAWBA RVR AT SC 5 AB BOWATER                              1,2,5    0836
    CW-057      FISHING CK RES 75 FT AB DAM NR GREAT FALLS                  5,8       0832
    CW-152      CROWDERS CK AT US 321 0.5 MI N OF NC ST LINE                6         0836
    CW-176      SIX MILE CREEK AT S-29-54                                   17        0836
    CW-197      LAKE WYLIE AB MILL CK ARM AT END OF S-46-557                1,8       0836
    CW-198      LAKE WYLIE AT CROWDERS CK ARM                               8         0836
    CW-201      LY WYLIE N LAKEWOODS S/D AT EBENEZER ACCESS                 8         0836
    CW-226      MCALPINE CREEK AT US 521, NC                                10        0836
    PD4004      BLACK CK AT S-13-43 1 MI NE NICEY GROVE                     1         0725
    PD-006      LITTLE LYNCHES RVR AT US 601 2 MI NE KERSHAW                1         0732
    PD-080      LYNCHES RVR AT S-28-15 4.5 MI SE BETHUNE                    1,4       0730
    PD-113      LYNCHES RVR AT SC 9 W OF PAGELAND                           1         0734
    PD-327      LK ROBINSON AT S-13-346 5 MI E MCBEE                        7         0725

    Station Selection Criteria

    1 = Influent to segment (sub-basin)          9 = Above major municipal area
    2 = Effluent to segment                     10 = Below major municipal area
    3 = Major streams at state lines            11 = Mouth of major tributary
    4 = Confluence of major streams             12 = Major water use area
    5 = Above a major industrial area           13 = Above major land use area
    6 = Below a major industrial area           14 = Below major land use area
    7 = Water Quality limited area              15 = Above a water intake
    8 = Major lake                               16 = Basic Water Monitoring Program
                                                17 = Other

                                            A-27

             Soul ~~~ Z  at       In~~~sire -  ~~                     002\ ~   WYLIE

      Wars\                                 iorroeVr             rz     ')ep

                   Ion  acolet Mu    B-0 4 \\O~~~~~~~~~on

                                                      ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~77

                                                                                                                                                                            ?Ii)  I4~~~~~  ~ >  - ~ Wh,te5    '

                       A~      ~~~                                      ~~~~~~~~~~~~~~~~~~~~~~~~ CrRn

    4,~~~~~~~~~~~~~oac    il

                                                                      tl ~ ~ ~ ~  ~     ~     ~     ~     ~     ~     ~     ~    ~    Warow/l

                       STREAM STATIONS FOR LANCASTER - SECONDARY
                                     CATAWBA DISTRICT

    Station    Description                                                Criteria    Basin

    B-056        CHEROKEE CK AT US 29 3 MI E OF GAFFNEY                       10        0856
    B-057        BUFFALO CK AT SC 5 1 MI W OF BLACKSBURG                      5         0856
    B-059        IRENE (BEAVERDAM) CK AT S-21-307 2.5 MI W
                   OF GAFFNEY                                                 10       0856
    B-062        THICKETTY CK AT SC 211 2 MI AB JCT WITH BROAD RVR            10,11    0856
    B-064        MENG CK AT SC 49 2.5 MI E OF UNION                           10        0854
    B-067A       TOSCH'S CK AT US 176 2 MI SW OF UNION                        10        0864
    B-067B       TOSCH CK AT RD TO SEWAGE PT OFF HWY S-42-92
                    SW OF UNION                                              9         0864
    B-074        DRY FORK CK AT S-12-304 2 MI SW OF CHESTER                   10        0854
    B-075        SANDY RVR AT SC 215 2.5 MI AB JCT WITH BROAD RVR             17        0854
    B-086        ROSS BR TO TURKEY CK AT SC 49 SW OF YORK                     10        0854
    B-088        CANOE CK AT S-11-245 1/2 MI W OF BLACKSBURG                  10        0856
    B-095        THICKETTY CREEK AT S-11-165                                  6         0856
    B-100        FURNACE CK AT S-11-50 6 MI E OF GAFFNEY                      10        0856
    B-119        BUFFALO CREEK AT S-11-213, 2.2 MI NNW OF
                    BLACKSBURG                                               15        0856
    B-128        LIMESTONE MILL CK AT RD CONNECTING US 29 & SC 1              10        0856
    B-133        THICKETTY CK AT SC 18 8.3 MI S OF GAFFNEY                    10        0856
    B-159        BULLOCKS CK AT SC 97 4.8 MI S OF HICKORY GROVE               17        0856
    B-199        MITCHEL CK AT CO RD 233 2.3 MI SSW OF JONESVILLE             10        0864
    B-211        PEOPLES CK AT UNIMPROVED RD 2.3 MI E OF GAFFNEY              9         0856
    B-243        TRIB TO BROWNS CK AT CLVT ON CO RD 384 3 MI E
                    OF UNION                                                  17       0856
    B-286        TINKER CK AT RD TO STP 1.3 MI SSE OF UNION                   9         0864
    B-287        TINKER CK AT UN# CO RD 1.7 MI SSE OF UNION                   10        0864
    B-323        DOOLITTLE CK AT S-11-100 1.25 MI SE OF BLACKSBURG            10        0856
    B-325        CK INTO CRAWFORD LK ON UN# RD NEAR SC 161 &
                    705-KINGS MT                                             9         0856
    B-326        LONG BR CK ON SC 216 BL KINGS MTN PK REC AREA                10        0856
    B-330        GUYON MOORE CREEK AT S-46-223                                6        0856
    BF-007       FAIRFOREST CK ON CO RD 12 SW OF JONESVILLE                   6         0864
    BF-008       FAIRFOREST CK AT CO RD 16 SW OF UNION                        6,10      0864
    CW-006       WILDCAT CK AT S-46-650                                       10        0832
    CW-009       STEEL CK AT S-46-22 N OF FORT MILL                           7         0836
    CW-011       STEEL CK AT S-46-270                                         10        0836

    Station Selection Criteria

    1 = Influent to segment (sub-basin)           9 = Above major municipal area
    2 = Effluent to segment                      10 = Below major municipal area
    3 = Major streams at state lines             11 = Mouth of major tributary
    4 = Confluence of major streams              12 = Major water use area
    5 = Above a major industrial area            13 = Above major land use area
    6 = Below a major industrial area            14 = Below major land use area
    7 = Water Quality limited area               15 = Above a water intake
    8 = Major lake                               16 = Basic Water Monitoring Program
                                                 17 = Other

                                            A-29

                       STREAM STATIONS FOR LANCASTER - SECONDARY
                                     CATAWBA DISTRICT

    Station    Descriotion                                               Criteria    Basin

    CW-017       CANE CK AT S-29-50                                          6,7       0834
    CW-019       WATEREE RVR AT US 1                                          10       0828
    CW-027       LK WYLIE AT SC 49 AND SC 274                                8         0836
    CW-036       SUGAR CREEK AT S-46-36                                      6,10      0836
    CW-047       GILLS CK AT US 521 NNW OF LANCASTER                         7         0834
    CW-064       MCALPINE CK AT S-29-64                                      10        0836
    CW-080       25 MI CK AT S-28-05 3.7 MI W OF CAMDEN                      10        0828
    CW-083       12 MI CK AT S-29-55 0.3 MI NW OF VAN WYCK                   6         0836
    CW-088       GRASSY RUN BR AT SC 72 1.6 MI NE CHESTER                    9         0832
    CW-096       WILDCAT CK AT S-46-998 9 MI ENE OF MCCONNELLS               10        0832
    CW-105       BROWN CK AT UNIMP RD 1.2 MI N OF CLOVER BL PLT              10        0836
    CW-131       BEAR CK AT S-29-292 1.6 MI W OF LANCASTER                   7         0834
    CW-134       CALABASH BR AT S-46-414 2.5 MI SE OF CLOVER                 10        0836
    CW-151       BEAR CK AT S-29-362 3.5 MI SE OF LANCASTER                  5         0834
    CW-153       BEAVER DAM CK AT S-46-152 8 MI E OF CLOVER                  6         0836
    CW-154       KELLY CK AT S-28-367 2.9 MI SE OF ELGIN                     5         0826
    CW-155       SPEARS CK AT SC 12 3.6 MI SE OF ELGIN                       6         0826
    CW-171      ALLISON CK AT US 321 3.1 MI S OF CLOVER                      6,10      0836
    CW-174       CATAWBA RVR AT UNIMP RD AB JCT WITH ROCKY CK                6         0832
    CW-175       ROCKY CK AT S-12-141 SE OF GREAT FALLS                      12        0832
    CW-185       CANE CK AT SC 200 5 MI NNE OF LANCASTER                     7         0834
    CW-192       CROWDERS CK AT S-46-79 4.5 MI NW OF CLOVER                  7         0836
    CW-200       LK WYLIE AT SC 274 9 MI NE OF YORK                          8         0836
    CW-212      TOOLS FORK CK AT S-46-195 7 MI NW OF ROCK HILL               7         0832
    CW-213       BIG PINE TREE CK AT 1-20                                    6         0828
    CW-214       WATEREE RVR AT 1-20                                         6         0828
    CW-221       UNNAMED TRIB TO CATAWBA RVR AT HWY 161
                   0.4 MI W OF 1-77                                          10        0836
    CW-223       LITTLE PINE TREE CREEK AT S-28-132                          15        0828
    CW-224       FISHING CREEK AT S-46-163                                   6         0832
    CW-225       FISHING CREEK AT S-46-503                                   5         0832
    CW-227       NEELY'S CREEK AT 2-46-997                                   10        0832
    PD-005      TODD'S BR AT S-29-564 1.5 MI NE OF KERSHAW                   6         0732
    PD-009       LYNCHES RVR AT US 1                                         6         0734
    PD-066      LYNCHES RVR AT S-28-42                                       17        0734
    PD-067       FORK CK AT SC 151                                           6         0734
    PD-068       FORK CK AT UN# RD 1.5 MI SW JEFFERSON                       6         0734
    PD-152      THOMPSON CK AT US 1 2.2 MI SW OF CHERAW                      6         0726
    PD-179      N BR WILDCAT CK AT S-29-39 1 MI S OF TRADESVILLE             7         0734
    PD-180       S BR WILDCAT CK AT S-29-39 2 MI S OF TRADESYILLE            7         0734
    PD-215       LITTLE FORK CK AT S-13-265 1.5 MI SW JEFFERSON              10        0734
    PD-246      THOMPSON CK AT S-13-243 0.8 MI NE OF CHESTERFIELD            17        0726
    PD-247      THOMPSON CK AT SC 9 1.5 MI ESE OF CHESTERFIELD               10        0726
    PD-250      TRIB TO BIG BLACK CK AT S-13-54 SE PAGELAND                  10        0725
    PD-333      HILLS CREEK AT S-13-105                                      6         0734
    PD-334      MINE BRANCH AT S-29-188                                      6         0732
    PD-335       LITTLE LYNCHES CREEK AT S-29-95                             10        0732
    PD-328      TRIB TO HANGING ROCK CK OFF S-29-84 1.6 MI
                   S OF KERSHAW                                              10        0732
    PD-329      TRIB TO HANGING ROCK CK AT S-29-13 ABOVE
                   KERSHAW PT                                                9         0732

                                             A-30

                     APPENDIX B

    PRIMARY AND-SECONDARY STATIONS LISTED BY REGION

        SHOWING INDIVIDUAL PARAMETER COVERAGE

                                                                             Sample Stations: Aiken

      Station  ITemp I      DO IpH ISattlCondtI TSS ITurblColorITransIALkLIHardI BOO5 N NH3 1 NO2 ITKN I TP ITOC I CL I Phen IMetalslPest I Other I Total I FecalIFlow ISed I Sed I
       No.  NH4 I   I    1    1                 I    I      I     I   I    I                                                      JPCBs IOrg*  I Coli    CoLi              I IOrg*l

                -   M   M       IM         I I        I     I     I     I    I      I     I     I    I    I    I    I      I                               M
     CSTL-003 MI  lM  Ii                  1.          I     I     I          I      M  I      I                           I. I              A           I I    I           IM  I

     CSTL-005          I        M  I M  M             I           I I  I M      I        I    I                I I                I I           I I         I       I     I M

     CSTL-012 I       I        II M              I          I        I M                I      I     I      I     I      I     Ia  I    IM

     CSTL-028  M    M                            1          I     I M    A      M MMI                               I I M    M    0                     I       I     I      A

     CSTL-037        I    I               I      II         I     I I I            I     I           1    I M       I                           I I            I    I M

     CSTL-O0I1MIM                I        I      IM      I        I    I    1141            M                              I      I    I                                          I

        E-002         l         I                I  I              I I                                I  I  IM   I      I                                     I I    I

        E-0121   7A4141                    I     14         I A                        I     I      I M  MM  M                                          1         M AI

        E-007BI       l         IM   I                      I     I       II I  I                                          I I    I M           I I M          I I    I           I

        E-007C I      l                    I    I I         I     IM                I     M                                       IM  I  I              I      I     I I    I
      CST-037111414   I                         114 I             I I       114          14         114 I    I  I  I    I                  I            1141 I    I              I

            I         liiiI     I                II         I      II            I               1 1         1 I  I  I  I                           I  I              I     I     I

        E-008   IMIMIM                    I             I mI  1         I IM I        I 141    MI         M  I   I        I  A  I A  I         I       I        I                I

        E-012  I          i    I                    I       I      I I                            I  I    IM     I M                                            I    I           I

        E-013    M        I        I M     I                        M I            I I         I    I I        I I M  I M  I M    I                                  A I     A
                                                        Tefnp = temperature                 Salt  =salinity             Trans = transparency           Sed= sediment (routine)
    M  monthly, 0 = quarterly, A  annually            DO   = dissolved oxygen             Condt  conductivity         ANk  = alkalinity              Sed Org  sediment organics
                                                        TSS   = total suspended solids      Hard  hardness              TP   = total phosphorus        Metals  heavy metals
    *Base-Neutral and Acid Extractable, and           Phen  = phenols                     Turb  turbidity             TOC = total organic carbon     Fecal CoUi = fecal cotiform
       Volatile organics                   Pest =  pesticides and PCes Other =-other organics IH3 II4 I  ammonia                                     Total Coll =  total coIiform
                                                        Flow  = flow or stage weas.         Cl   = ch lorides      N     02 N03  = nitrate-nitrite     BCD 5 = 5-day biochemical
                                                        TKN   = total Kjetdhat nitrogen    pH    = pH                                                           oxygen demand

                                                                                               B-1

                                                                        Sanple Stations: Aiken

      Station  ITemp I DO I pH ISaltICondti TSS ITurbIColorITransjALktIHardj B905 1 NH3 1 NO2 ITKN I IP ITOC I CL I Phen IMetalstPest I Other  ITotal I FecallFlow I Sed  ISed I
       No.                                                                        INH4INO3I I           I    I    I       I     IPCBs I Org*  I Coli  I Coli       I      I Ir9*I

        E-019             I      I        I I      I             I I    I    I      I         I M     i      I    I             I     I       I       I      I

        E-022    M                              II         I     I I I                       I I  1                   I      I        I  I        I       I         I

        E-036 1M1141141             I     I    I  t        I     I   I    I  M          1          IMI        I    I             I     I      I       I      I

        E-051 M                                 II I        MI           I        I     I      1 1 1 1  I                       1,1 I           I    I         IA    I         I

        E-059 2      14M            I        I 1           I          I      1          1          1141  I        I       I      I    I       I       IA    I       I    I A

        E-076    M i i           i              II         I     IM             I              l              I      I        I     I          I       I      I    A      I

        E-090    M    M    M 1M                                     MI    I   M         1          1141       I                  I M                   114         I     I A

        E-091  I       I                 I    I    I      I        IMI              I                      I M                             I A      I I MI         I    I      I

        E-092    M            1      I          II I                II I          I        I   1 1 1 1  I M                        I          I M            I     I  I   A

        E-094    M        1M        I             M                 MIAI    MIMIMIQ                                I           1       I       I       IM IMMIAI                I

        E-099    M 1          1                 1          I      II I            I      1.11111                          I A   I    I         1M1            I     I     I M

        S-050        I   I                I    I      I             II I          I     I      1 1 1 1  I             I    I       I       I     I      IM         I       I A

        S-092       I    I     I                I    II                I     I    I    I                 I    I    I  I  I   I          I      I      I      I           . m

        S-093         l                   I     I I        I         I       I        I        III1*I                I        I    I     I             I I      I     A A

        S-123  M            4M                                      M IAIMIMINIMIMIl                                        a  IA M                    IN M  INM  A
                                                      Temp = temperature                  Salt  = salinity           Trans = transparency           Sed sediment (routine)
    M   monthly, 0 = quarterly, A  annual ly         DO   = dissolved oxygen             Condt = conductivity        Atk  = alkalinity              Sed Org  sediment organics
                                                      TSS   = total suspended solids      Hard  = hardness           TP   = total phosphorus        Metals  heavy metals
    *Base-Neutral and Acid Extractable, and          Phen = phenots                      Turb = turbidity            TOC = total organic carbon     Fecal Coti = fecal cotiform
       Volatile Organics                             Pest =  pesticides and PCBs         Other =  other organics I13 NH 4      ammonia             Total Coli =  total cI  ifoI I
                                                      Flow  = flow or stage meas.         Ct   = chlorides           N02 N03  = nitrate-nitrite     BOD5 = 5-day biochemical
                                                      TKN   = total Kjetdhat nitrogen    pH    = pH                                                         oxygen demand

                                                                                          8-2

                                                                         Sample Stations: Aiken

      Station  jTemp I DO I pH ISaltICondtI TSS ITurbICoLorITransIAlkLIHardI BOD    NH  I NH31 NKJ  I TP ITOC I Cl IPhen IMetalslPest IOther I Total IFecaLiFlow I Sed I Sed I
       No.                                                                             NH4  1 i3  NI                                 I I    II I PCBsIOrg*  I Coli  I Coli   I IOr

        S-131  1 M  I M      M I                             I       I     I   M     I M     I                   I I          I I M  I                      I I           I     I A

        S-186                        I   I   14    I   IMIAI  MIMIM   M    1                                           I                                        MMA

        S-233          111      I                 II I               I           I                                      I           I      I I         AM          I      I     A

        S-235         fI                   I      I     I           I I     I                      I      I                                 I I  I                  I I    I  M

        S-255     M1141141           I I          114        I      I    IAI   MI           1141         M        I

        l-295                              I      I          I      III I                   I     I  . I         I I     A          I      I I M  I M                          I M

       ST-025  1M   14M              I I          1       I         IM   I M  I  M                 I                   I I           I I            I I         M         I A

       Sv-068  I       lii                 I      II         I      IMI              I      I                                               I I    Im

       SV-2695    MM1                I     I      1          I      I    I    1     1       IMI        IM        I    I       I MI          I       I A         M         I     I      I

       lV-071                              I      I          I      III              I I           1                          I       I     I I M                   I I         I      I

       SV-0729M114M1    I                                               IAIMIMIMIMIMIQI   I    101    I                                             I    I MI    I   I   I

       sv-073                I                    II    I             II I           I      I      1            I        I       I       I       I      I      IA         I        IM  A

       SV-096                        I     I      1 1        I        I        I           1          1          I    I          I      I      I       I A   141         I      I     I

       SV-118     M M    I     Ii          I      II         I MI              I  I M1 1 1 1 M                                        I     I I         A  I M  M                A

       SV-151 M                                                                               I      I      I      I         I     I     I    I
                                                       Temp =-temperature                   Salt slinity                 Trans = transparency            SedI  sediment (routine)
    M  monthly, Q = quarterly, A  annually             DO    = dissolved oxygen              Condt = conductivity        Alk   = alkalinity               Sed Org  sediment organics
                                                       TSS   = total suspended solids       Hard  = hardness            TP    = total phosphorus         Metals  heavy metals
    *Base-NeutraL and Acid Extractable, and            Phen  = phenots                       Turb  = turbidity           TOC = total organic carbon       Fecal Coll = fecal coliform

       Volatile organics                               Pest =  pesticides and PCBs           Other = other organics      NH3 NH 4 =ammonia                Total Coli = total cotiform
                                                       Flow =  flow or stage meas.          CL  =  chlorides    NO02 N03 = nitrate-nitrite               BOD5 = 5-day biochemnical
                                                       TKNI   = total Kjetdhat nitrogen     pH    = pH                                                           oxygen demand

                                                                                            B-3

                                                                 Sample Stations:  Aiken

                I      lI I  I I           I     I    IIi  I II         I     I    I    I    I    I                 I1 1   I      I      I       I       I      I     I     I     I
      Station  ITemp I DO I pH ISaltCondtl TSS lTurbIColorITransIALkllHardl 80o5   NH3 I NO2 ITKN I TP ITOC  I Cl I Phen IMetalslPest   Other   Total I FecatllFlow   Sed   Sed I
       No.           I    I                   I    I I                              I    I                    I    I I            IPCs I  org*  Colij  Colil                I Or I

      SV-175      I   MI             I    I I M       I I         I    I        M  I     I    M  I     M   I   I    I      I      I     I       I           M   I     I     I     I

      SV-250   I M     IM                                           I I  I   I  IAI  I   I M                               I  A         I                         M I   A I    A

      SV-251   I M  I             I       I      1    I     I     I M  I A I  MI M  I M                        I M          M I QI                                                I

           IV-25        I    I    I               I         I     I M                       I         A I                                 I    IM   I    II                       I

      SV-291   I MI         MI I M I   I  I      I M I  M                 A I   M  I M  I M  IM  I M I  I    I                0   I A  I        I        I     IM  I        I     I

      SV-29    I M  I M I M I  IM I                               I M     A I  I M  I  I M  I     I     I    II  I  I                       A   I        I  I M  I A  I A

      SV-2318   I M  I M I M I  I                                 I M     A I  M  I M  I  I M          M I  I    I         I I    I A M M M M M  AI  I   I  MIMI            I     I
               I     I    I   i     I     I     I    I     I      I    I    I      I     I     I    I A                   I       I     I       I       I      I     I     I     IA
      SV-329  111414    1141141141� M  M    I   IMIAI MIMIMIMIMIMI   I   I     I A I  AlI    I M IMAA

      SV-31                                         I M  I                                       M I  M I                      O I   M  M  A    I  M            I M I    AI    I A  I

      SV-326    1141141 1           I MI  IMMI              I     IMIAI    M          MI                                  1                I  MIMIA                            AI
               I      -I   I    I      I  I     I                                                          l                MI  I  I  I  I  I  IA
      SV-318   I MIMIM(   I         I      I        M I        I  I IA I   MIM             M    M    M    O I              I   QIA              I I MIMIAI II

      SV-32    I M  I M I M                        I        I                                                                     I I       A I  IM  A      M I    M    I  A A I  A  I
           SV32  IM M M              111414                 I      1M A          MI      I    IM     M     M        I      I   OIA           A       l l l ll  I   HIMIAIAI
      SV-324lI I  I M I M I   I M  I             I M I      |       M  IA       M  I M  I                                                       I        I         M  I     I     I
           sV32  IM M M              114         1141       I      IM A          MIMIMIMIMIQI                       I      I    Q   AI    Al             I   MIMI           I     I

      SV-32       M  I    I   M   I  I     I     I   M I    I     I    I    I       I     I                                       I        I             I      I  M
           SV32    111414           114          114        I      IM A          MI     I     IM     M    O         I      I   QIA           A      l l ll  I   MIM         I     I

      SV-330   I M  I M I         I                M I'           I M     A I                                                               A I  I           M I   M  I      I              I

                                                      Temrp = temperature           S      alt  = salinity            Trans = transparency            Sed  sediment (routine)
    M = monthly, Q   quarterly, A  annually           DO    = dissolved oxygen            Condt = conductivity        AML   = alkalinity              Sed Org  sediment organics
                                                      TSS   =total suspended solids Hard  = hardness                  TP    = total phosphorus        Metals   heavy metals
    *Base-Netral and Acid Extractable, and           Phen  = phenos                       Turb  = turbidity           TOC =  total organic carbon     Fecal Coli m fecal coliform
           SV37 I MI MIMI   I M  I               I MI       I     IMI  AI    MI MI M    IM I MIQ   I                       I  QI AI  A I                 I  MI MI           I     I

       Vo lati le Organics                            Pest    pesticides and PCBs          ther  other organics  3  = a               ia              Total  oll Total Co ifor
           SV38 I M lIMI MI IMI                  I I   II   I     | IIAI    MI MI M lIM I MIQI    I                        I  QI         I  A I          I  MI MI           I     I
          SV32    IM M M            114         114        I      IM A          MI     I     IM     M     Q        I      I   OIA           A      l l ll  I   MIM         I     I
          SV39 I   M I   M I M   I  I     I     I M   I    I     I M  I     I  M   I   M I   M I M  I M I Q       I I     I I            I      I           M I   M~   I   I     I

          SV-30      M IMI MI             I      I MI       I     IMI  AI    MI MI M    iM I MIaI    I                     I  aI         I       I       I  MI MI           I     I

                                                      Temp  =temperature                  Salt  = salinity            Trans = transparency            Sed = sediment (routine)
    M4 = monthly, Q = quarterly, A = annually        DO    = dissoLved oxygen             Condt = conductivity        Alk   = alkalinity              Sed Org =sediment organics
                                                      TSS   = total suspended solids      Hard  = hardness            TP    = total phosphorus        MetaLs = heavy metals
    *Base-.Neutral and Acid ExtractabLe, and         Phen  = phenols                      Turb  =turbidity            TOC =total organic carbon       Fecal Coli =fecal coliform
       Volatile Organics                             Pest  = pesticides and PCBs          Other = other organics      NH3 NH4  ammonia                Total Coli = Total Coliform
                                                      Flow  = flow or stage meas.         Cl    = chlorides           NO2 NO3 = nitrate-nitrite       BOD5 = 5-day biochemicaL
                                                      TKN   = total Kjeldhal nitrogen     pH    = pH                                                          oxygen demand

                                                                                           8-4

                                                               Sanple Stations: Charleston

      Station  ITemp I DO I pH ISaltICondtI TSS ITurbIColorITransIAlklIHardI BOO5 I NH3 I NO2 ITKN I TP ITOC I CL I Phen IMetalsiPest I Other I Total I FecaliFlow I Sed  ISed I
       No.                 IIIINH4IN03I                                                               I    I    I    I      I       IPCBs I Orge  IColiiColi I          Io      rge

     CSTL-006     M       I     I    I     I     I    I      I I*       I    I M          I       A   I M       I M         I      I      I       I       I      I      I     I     I

     CSTL-007                              I I N  I    II II                  I  I                        1 I  I M  I  I                                  I I    I            I I

     CSTL-010  I              1        I         I*I         I     I I I            I     I      I    I    I    I    i      I       I     I       I       I MI          I aA

     CSTL-011 141141141                          I 1              I M         I M         1           1141            I     I      I              I         1           I I     Ia

     CSTL-013        I        i i                                     I I           I M              I     I                I       I A  M                I      I A          I A

     CSTL-0431141 11I                         I14            I     I    lI N    I         1 1         1141      I    1          Al        I       I       1               A M

     CSTL-044                I                   I           I      III     I         I           1                         I I    I  I  I     I      I             I               I

     CSTL-062    1 MI       MI       I1                      I     I    i        4        1         A                               I     I       I       1        M  a A

     CSTL-063                              I     II          I     II I             I     I       1 1 1 1 1                  I      I     I       I       I m        I    A   a

     CSTL-068    3Mi       Mi        I     I       1         I     I      AI                         I                               I  I                 I       I       A         I

     CSTL-069         lI Ii                I     IMI         I     I                I     I               1                  I I    I             I I  I    I                 I I

     CSTL-075         1   I11 MI                 I   I       I     III              I      I      I 1          I                   I     I       I        I      I     I     I     I
     CSTL-044114114M1                1     1     1141        I     I    1 IA n   I        114           M114                                      I        14

     CSTL-079  I M     I      Ii                 I I    I       I    I I    I       I      I M1               1        I            I     I       I        I      I     I I  I
     CSTL-08511114 M                       I   114 M               INAI               M IMNNMIQ                      A          o                         IN  INAI

                                                       Temp =  temperature                  Salt   salinity             Trans = transparency            Sed sediment (routine)
    CS= monthly, 0   = quarterly, A a 3 Mually        DO    = dissolved oxygen             Condt   conductivity        Ak   = alkalinity               Sed Org   sediment organics
                                                       TSS   = total suspended solids Hard    hardness                  T     = total phosphorus        Metals 1heavy metals
    *Base-Neutral and Acid Extractable, and           Phen  = phenots                      Turb    turbidity           TOC = total organic carbon       Fecal Co1i = fecaI  co1iform
       Volati le Organics                             Pest  = pesticides and MCs       o    ther = other organics      NH3 NH 4 =ammonia               Total Coti = total coliform
                                                       Flow =  flow or stage meas.          Ct   = chlorides       NO2 N03 = nitrate-nitrite            BOD5 m 5-day biochemical
                                                       TKMS  = total Kjeldhal nitrogen      pH    M pH                                                          oxygen demand

                                                                                             B-5

                                                                Sanple Stations: Charleston

      Station  ITemp  I DO I pH ISaltICondtI TSS ITurbIColorITransIALkljHardI 6005 RH3   NO2 ITKN I TP ITOC I CL I Phen IMetalslPest  IOther  ITotal I FecaLiFLow I Sed ISed I
       No.                                                                          INH4IN3           I    I    I                   IPCBs IOrg*  I Coti IcOI            I     IOrg~I

     CSTL-098                           IM   M  MIM  M   Ml MI             I I                  I      M      I M           I       I M           I       I       I MI MI A

     CSTL-099             i                I     I I         I        I        I        I        1 1 1 1 I               I    I       I       I      I      I      I               I

     CSTL-102         1111  I                    II          I        I        I        I        1                          I       I I  I     I      I      I      I               I

     CSTL-107 MO       IM      I MI        I     I           I     IM    A      M M   I   IMI    M        I    I    I               I     I       I  M I          I     I  I   A

     CSTL-108   M            I             I     IM        I                 IM I         I       I             I I          I I  I  I  IN I             I      I      I

     CSTL-09 I        11                   I    II                       I    .           I       1 1 1 1 1    I               I      IMM         I        I MI AM    AI

        E-014  8I  MIN M I           I I         IMI         I I       I     I M I       I       I    I         I M     I    I          I                  I I  I  I    I

        E-015         li      Ii              I      1          IMIII               I     I           1                      I      I MI M        I        I MI         I     I A

        E-016OIMIMIMI  IMIMIMI   I   IMIAIM                                                    MIMIMI   I   I   IAI  A                                     IM                  IA

        E-100         l                    I       I         I     I      I         I     I M  M  1 M  A M                          I MI          I   I       IA   I M     A

       MD-o1 IM IM I                 I     II IMI            I     I    I    I M          I I         IMI       I    I       I      I     I       I        I      I     I     I     I

       mD-00 I        111                  I     I2I         I     I I I            I     I       1 1 1 1 1                  I      I     I       I        I      I M         I     I

       Ml-003                              I     I I         I     I I I            I      I           l    i      I         I      I     I        I       I      I     I     I     I

       E-O16IMIMIMI                  I     IIM               I          ID   I N       I    M         IM        I                   I     I        I       I    A I      M  A

                                                        Temrp =temperature                   Salt = salinity            Trans = transparency             Sed sediment (routine)
    M  monthly, 0   quarterly, A = annually        DO        = dissolved oxygen            Condt = conductivi ty       AMk  = alkalinity                Sed Org  sediment organics
                                                       TSS   = total suspended solids       Hard = hardness             TP    = total phosphorus        Metals  heavy metals
    *Base-Neutral and Acid Extractable, and         Phen = phenots                         Turb = turbidity            TOC = total organic carbon       Fecal Coli = fecal cotiform
       Volati le organics                             Pest  m pesticides and PCBs          Other = other organics      NH3 NH4 = ammon ia               Total Coti = total cotiform
                                                        Flow  =flow or stage meas.           Cl   =chlorides            N02 N03 = nitrate-nitrite        BOD  = 5-day biochmical
                                                       TKN   = total Kjetdhat nitrogen      pH    = pH                                                          oxygen demand

                                                                                             B-6

                                                             Samrple Stations: Charleston

      Station  ITenp I DO I pH ISaltlCondtl TSS ITurbIColorITransIALklIHardI BOO5   NH3   NO2 ITKN I TP ITOC I CL I Phen IMetaisiPest  IOther   I Total I FecalIFlow I Sed I Sed
       No.                                       I                                 NHI3I,    I   I I              I I           JPCBs IOrg*  I CoLi ICotiI            I IOr9*j

       MD-00 5   I   I    I    I    I     I     I    I     I     I    I    I      I     I     I    I    I    I              I         I       I          MI                    I

       MD-006         I       I II M                                          I M  M  I I                   I M                     I      I I           I I  I    I     I A

       MD-007     M IMI MIMI                    IMI                I m         I 1      1           1        I      I        A I              I  MI MI             I    I A

       MD-010     Mi                                                  I M         I I              I m         I M  I    I  I    I A   I                                 I
       MD-013IM IM M M M                          M        I     I   I    111           14Mli                I M         I M          I       I  H   IN    I       IA

                                    MD-016  M    M  ~~~~~~~~~~~~~~~                 ~     ~~~~~~~~~~~~~~~~~~~I M
       MD-0201M I              I M I                       I II           I M   M          I  1 1          1        I        I   M        I       I          I M

       mD-027  I M  I M      I M   I  I  I    I M          I    I    I MI     M              I I 1  I  I M      I     I      I        I I         1          I     I     I     I

       mo-026    m I   I  i     i        I m   IIm        I     I   ImI          I    I               1                 I      I     I       I       I      I     I     I a

       MD-034   M I        M     I        I    I    I      I        I    I I            I       I     I M    I A    I           I     I M         I          I M
       MD-O13( MIMIMI14 MI14                    114        I     I MI    114            M 1        11 I           IIIP   I      I     I       I  M  I MI           I  I        I

       MD-039   I    I    I    I    I     IIM   I      I    M    I    I    I      I     I     I    I    I    I   I       I      I     I       I       I      I    I      I     I

       MD-043    M I  11M1                I    IMI         I     I   I    I M                I        I     I A                 I I   I       I       I      IM  A
       ID-0201141141411411I   114 IM     IIAIM   I    nMIHIMIII  I                                                        101             I    I 114   I   I                   I

       MD-044    M     M     M    M       M       m                 M    A     M     M    M      M    M    0                 Q aI     i                  M

       MD-045     M  M         M I  MI  I  M    I    I     I     I   I     I               I     M I  I  I   I    I      I   a        I I             I      I     I    -      I

                                                     Temp 1teMperature                   Salt =salinity             Trans = transparency           Sed sediment (routine)
    M = monthly, 0   quarterly, A = annually     DO    dissolved oxygen                  Condt = conductivity       Alk   = alkalinity             Sed Org  sediment organics
                                                     TSS  total suspended solids         Hard = hardness            TP    = total phosphorus       Metals  heavy metals
    *Base-N(eutral and Acid Extractable, and         Phen   phenots                      Turb = turbidity           TOC = total organic carbon     Fecal CoUi = fecal cotiform
       Volatile Organics                             Pest  pesticides and PC~s           Other = other organics     NH3 NH 4 = ammnia              Total Coti = total coliform
                                                     Flow    flow or stage meas. CI             =chlorides NO2 N03 =          nitrate-nitrite      BOB I  = 5Iday biochemical
                                                     TKN  total Kjeldhat nitrogen    pH   = pH                                                             oxygen demand

                                                                                          B-7

                                                              Sample Stations: Charleston

      Station  ITemp  IDO I pH ISaLtICondtI TSS ITurbIColorjTransIALktIHardI B005 1 NH3 1NO2 ITKN I IP ITOC I Ct I Phen I1etalsIPest  IOther I Total  IFecalfFlow I Sad I Sad I
       No.                                                                            NH4INO3I        I    I I       I.  I          JPCBsIOrg*  ICoLi  ICoLi            I     IOrq

       MD-046     M             I    I                                  I I M  M  I   A     I M   M     I I M      I   I           I I    I       I       I                   I

       MD-047    I   l        I I          I      I         I      II I             I      I M  M      l M                          I     I       I       I M           I M         I

       -048       M I        MI I    M    M      I'  H         M     MI   A IM         M     I    MIMIOINI                   1 1 M   I MI Q                                I AI

       MD-049     M     M    M    M  M           I m                M      A     M     M     M      M I M    Q     M                                             M  m

       O-052      M    M  I    M   I I        I M I       I ImI I M                              IIA  I           1                 I     I       I       I       I A  I        I

       MD-069 47IN    M      M         M         1M            I M        AIM          M    MIM M I                  I     . 0            I           MI  I I  I  I    I

       MD-070     M IM       M    M    M         IM                IM   I      IM  IM  I M          MIM     l        I M            I 0 1    1               14

       MD0-071    M     I      I    I      I     I                  M                              I A           I M       I M  M  IM    M    I  I  I

       D- 113     M    M     M 1   M 1   M     M 1M A                               M      I M   MIA   I  MIMI       I       1 a   IAI    AI                              A A M

       -114  1 M I        M          I      M   I M  I M           I  I  I       IM             I A                 I M      I                    I I  I     I      I      I M

       MD-115     M    M     MI                             I    M            M     IA M                    I M                     I     I       I       I       I     I     I     I

       M       -116      i                I     II         I      I llM  M         1       M M1                         I          I          1 I            A   I      M     A

       MD-117  I  liiI                     I   II           I   III                            I   I Miii    I.,                    I   I    I    I                                 I

       W~-118   MI    M              Im            II              Ill           I M       I      1 1 1 1 1                            I       I I  I     I       I     I     I     I

                                                      Temp  = temperature                  Salt  =salinity             Trans = transparency            Sed= sediment (routine)
    M  Wmonthly,  = quarterly                        A = annually  DO    = dissolved oxygen  Condt = conductivity      A     = alkalinity              Sed Org   sediment organics
                                                      TSS   = total suspended solids       Hard  = hardness            TP    = total phosphorus        Metals  heavy metals
    *Base-NeutraL and Acid Extractable, and           Phen  = phenols                       Turb  = turbidity          TOC = total organic carbon      Fecal Coli = fecal. coliform
       Vale tilLe Organics                            Pest =  pesticides and PC~s          Other = other organics    NH3 NH4 = ammonia                 Total Coli = total coliform
                                                      Flow I  flow  or stage meas.         Ct    =chlorides NO  N03  nitrate-nitrite RO I5 =51day biohe   m      I        Ical
                                                      TKN   = total Kjeldhal nitrogen  pH    = pH                                                              oxygen demand

                                                                                            B-8

                                                               Sample Stations: Charleston

      Station  ITemp I DO I pH ISaLtICondtI TSS ITurbjCoLorITransjAlklIHardj BOD5 I NH3 I NO2 ITKN I TP ITOC  ICl I Phen IMetalslPest  IOther  ITotal I FecalIFLow ISed  ISed I
       No.                                                                           N H4   I  N?3 I    I   I    I    I    I      IPCBsIOrg* IColi IColiI            I     IOrq~j

       MD-119     MIM  I          I            I      1 I           I IM  IIM   IM  IM                   I     I    I M           I     I   I       I  Q       I     I  I   A

       MD-120     M     M   I     M    I         I    I M         I    I   I       I     I   A    I  M                  I     I      I I M      I       I      I     I      I     I

       MD-128l111111111l                          14        I     IMIAI             I         M    IMIQI            I           1       I                 4    I I I M

       MD-135    I    M  I  N  I    M   I  I     I    I       I     I       I      I     I     I    I M     I    I         I I   I              I I  I     I      I M

       MD-152   M1141141141141 M           M       M                   I        4        1          1141  I    I           I      I     I       I       11A  I             I AI

       MD-     165  MIM   MII                               1 MI I                    I  1            li i i               I      I     I       I       I M          I      I     I

       14D- 1352           MM1                   14         I     I    I    I      I       1         1I    I               I      I     I       I       I      I     IM  M

       MD-175  I     I.1          1        I    I    I      I MII             I        I  M      1      I m             I    I       I       I      I      I M                    I

       MD-176            4111144                                  IMIAIM                   MI         MIQI          I      I M          I       I M41                 IAIM  M

       MD-194     M    M     M    M   M           mM                           M            M          MI      I I         I                        m      M

       MD-195    M    M      M    MIM            IM                  M   A   M        M     M'  M   M    0    M                                     M      M       m     A

       MD-198  )HM        M       MI        I IMI           IM         I I      I        I                   1        I        A  I     I       I       I      I      I     I     I

       MD-202    M  I M  I    II       MI        IM              I II I                          I M          I A                I I    I       I       IM            I     I     I

       mD-206     m          I  I   I  I   I   IM I   I     I     I    I    I      I        MI  I   I    I     I    I      I      I     I           M   I      I      I     I     I

                                                       TeDp =te1 mperature                 Salt =salinity              Trans = transparency           Sed sediment (routine)
    M = monthly, 0   quarterly, A = annually  = dissolved oxygen                          Condt = conductivity       ALk     =     alkalinity        Sed Org   sediment organics
                                                       TSS   = total suspended solids      Hard �=hardness             TP    = total phosphorus       Metals  heavy metals
    *Base-Nleutrat and Acid Extractable, and         Phen  = phenols                      Turb  turbidity            TOC = total organic carbon      Fecal Coti = fecal cotiform
       Volati le organics                            Pest  = pesticides and PCBs      o    ther  other organics    NH3 NH 4 =amomonia                Total Coll = total cotiform
                                                       Flow =  flow or stage meas.         Ct       chlorides          NP2 W03 = nitrate-nitrite     BOD 5  =5-day biochem~ical
                                                       TKNr   = total Kjetdhat nitrogen    pH   pH                                                            oxygen demand

                                                                                             B-9

                                                            Sample Stations: Charteston

                     I. I I   I    I     I     I    I     I    I                                                       I      I     I       I       I      I    I     I     I
      Station  ITemp IDO I pH ISaltICondtI TSS lTurblColorITransIAlklHardl BOD5   N H3 I NO2 ITKN I TP ITOC I Cl I Phen IMetalsiPest I Other ITotal I FecallFLou ISed I Sed I
       No.  N        u1                                                                I NO                                   I I   I    I    I   I  PCBs I Org* I Coli   Coli  I   0rg*

           D-  I     I    I    I   I     I     I    I     I     I    I    I      I     I     I    I    I    I    I      I     I     I                           I I  I
      MD-20  MI            MIH   M  I    I M                   I    I    I M          I MI   I M           I   I       I      I    I       I  M I         I     I    I    I

       MD-209    I M  IM   I M I MI      I     I M  I   I    I   I    IM   I    I             M   IM        I   I       I      I    I       I  M   I M   I       I    I    I

       MD-20 I M  I M    M I  I M              I M  I    I    I   I    I M                M         H I    I   I        I      I                            M           II

       MD-211      IMI     IMI I                IM        I     I         I      I    IM            MI      I   I       I      I     I      I   M     MI         I    I    I
           MD-217 I  I    I   I M  I     I     I    II    I     I    I    I      I     I          I i  I MI QI          I      I    I       I       I      I     I     I     I
       MD-210  I M    IM    I M I M I  I    II                  I   I I   I IM   I   I I   I                            I  A  I     I       I  M  I M      I     II A        I
               I    li       i           I    II     I            I    I         I    I       1  1  11                  I     I    I        I       I      I    I    I    I

       MD-21   IM I  M    IM   I M  I            MI M  I II    I   I    I M  I M  I M                  I M   I   I   I  I      I    I       I  M  I        I     I A         I

           ST- I    I  I    I              I  I           I    I I               I      I              I         IA1    I     I    I        I       I      I    I    I    I

       ST-005   M   M     M H M                 I�                M AM          M            M       m                                          M    mI    IH
       STMD-2007   IM  I M    M I I I          I M  I    I    I    I A IM   I             M         M I    I             I           I  I MI                     I           I
                   l ii                  I    II          I      II              I    I      *I   l l l l II            I     I     I       I       I' ll        I    I    I

       ST-20     I M  I M   IM I               I          I    I M      A I  M   IM    M I      M I M I  I              I      I    I       I  M I    I    I    I
               I     1       1       I         II  Ili I        I                             l      l I    I  I    I  I  I  I 1    1    1I

       SVMD-241  I M  I M   IM I M IMI    I               I    I M    A I M         M  I M    M I  I O  I   I           I  I A              I  I M   I    I    I A

                                                    Temp =temperature                  Salt  = salinity           Trans = transparency           Sed  sediment (routine)
    M  monthly, 0 = quarterly, A = annually         Do   = dissolved oxygen             Condt = conductivity       AMk  = alkalinity             Sed Org  sediment organics
                                                    TSS  = total suspended solids      Hard  = hardness           TP   = total phosphorus        Metals   heavy metals

      Volatile Organics                            Pest   pesticides  PCBs              ther = other organics      H3 I    II  I    Imonia      Total CoI I I   I   = total coliform I
       STD-001   I MI M IM IMIMI  MI MI                   I    I MI AI M   I MI MI  MI MI  MI MI                        I  OI AI  A I   MIM  I                   I     I AI

                        Flo  =flo or stage meas.                                       C     = chlorides          N2  = nitrate-nitrite          B      5-day bio  hei        i
                       I  I   ITK I    I    I    I    I    I    I Kjedha  nitrogen     p      H = pH                                                     oxygen demandI   I  I    I  I  I  I  I    I    I
       ST-006    IMIMIMIMIM I                  I M I      I    I MI AI M   I MIM I    IMMI  QI   I                      I  QI        |  I       I  M   IM     M  I AI    I
           ST07I M 1 MIM 1         I     II1      I    IIIA  I    II                   I        I    I  1 1I1Q  I  AI                I      I       I      I    I AI    I

               I     li   i   i                I    III I    II                  I     I   I     1 1 1 1 1              I      I    I   .I          I      I    I    I    I
       ST-016 7IM IM IM I    I            I    I MI       I MI MI A IM    I MI MI  MI MIQI    I 10                         QAI    I         I       INM I  I    AlI    I
               I    l ii                 I    II          I      II              I    I       1 1         1             I      I    1.              I      I    I    I    I
           SV11I M lIM I MI I            I    I MI        I    IMI  AI   M I MI M 1 1MIM1 1QIM1                         I  QI AI            I       I M IMIA I    I
                                                    Teap =temperature                  Salt  = salinity           Trans = transparency           Sed = sediment (routine)
    M  monthly, 0 = quarterly, A =annuaLly          DO   =dissolved oxygen              Condt = conductivity       Alk   = alkalinity            Sed Org = sediment organics
                                                    TSS  = total suspended solids      Hard  = hardness           TP    = total phosphorus       Metals = heavy metals
    *Base-NeuJtral and Acid Extractable, and        Phen  = phenols                     Turb  = turbidity          TOC =total organic carbon     Fecal Coli = fecal coliform
       Volatile Organics                            Pest  = pesticides and PCBs         Other = other organics     NH3 NH4 = amuonia        .    Total Coli = total coliform
                                                    Flow = flou or stage meas.         Cl    =chlorides           NO2 NO3 = nitrate-nitrite      BOO5 = 5-day biochemical
                                                    TKN   = total Kjeldhal nitrogen    pH    = pH                                                        oxygen demand

                                                               Sample Stations: Colunbia

      Station  ITemp I DO I pH ISaLtICondtI TSS ITurbICoLorITransIALkLIHardI 8005 1 NH3    NO2 ITKN I TP ITOC I Cl IPhen IMetalsiPest I Other  ITotal IFecaltFLow I Sed I Sed I
       No.              I                                                           NH4i1NO3I       II        I I             I  JPCBsIOrg* IColi IColiI             I I    rOr

      B-047                  I    I     I I     I     I       I     I I  I  I         I     N       I       I m         I     I      I       I             M I

      I-054       M    IM    M A  I                                                                    II I   M I II  I  I  I A I   A    I I   I  I               M I   '  A  I   I

      8-047    2 1         1        I     I        4        I          I    I      I     1          14         I    I      I      I     I       I       I      I M

      B-07        M i        I i MI              I  I       I     III              I     I         A.I M                          I     I       I       I m    I     I      I     I

      8-080  11M 4I  I4                                                                                                           I   I    I    I  M   IMIAIM  IMIMIMIM   I QI  I  a  M

      -110         I     1IM  I              I          I             I    I mI  I      I       I    I                   II   I       I       I       I      I     I M          I

      8-123    IMIMINI            I        I  I141          I     I    I    I       M  I           I141 M      I    I      I      I     I       I         1          I      I     II

      6-145    I       m                   I N I    I       I     III  I   I       I                  li         i  I        I      I     I       I     I         I     I         I

      8-236    11M  I I             M I    I  I M       I   I     II I              I  I A  I M           I   I    I      I  A  I         I       I  AIN         I    A  I AI

      3-280       M  I M1                     I    II       I     I       I m                        I I    I M            I I    I     I       I       I M     I     I     I     I

      B-327   m  I M         M I          I    I I          I       I I M             I A        I M               I M     I I            I I       I M        I I    I     I     I

      B-328     11414         I  1  M             I I 14   I                 I            I I  1   I                   I    I I  I     I       I       1         I         I     I

      c-001       M  I    I    I    I         I  I    I     I     I       I M              I     I I  I    A             I I  I  I  I   I       I       I       I     I     I     I

      C-005          I    IM   I       I         I    IM    I I     I       I      I        M        I    I    I    I      I      I     I       I       I       I     I     I     I
                                                      Teffp =temperature                  Salt  = salinity            Trans = transparency           Sed= sediment (routine)
    M = monthly, 0 = quarterly, A  annually           DO    = dissolved oxygen            Condt v conductivity        Alk   = alkalinity             Sed Org  sediment organics
                                                      TSS   = total suspended solids      Hard  = hardness            TP  =   total phosphorus       Metals  heavy metals
    *Base-Neutrat and Acid Extractable, and           Phen  = phenols                     Turb  = turbidity           TOC = total organic carbon     Fecal Coti = fecal colifform
       VolatilLe organics                            Pest =  pesticides and PCBs          Other = other organics    NH 3  NH4 = ammoni a             Total Coli = Total Coliform
                                                      Flo8-1flow or stage meas. C1  =            chlorides N 1   N13 =          nitrate-nitrite      BODI  =-day biochemicaI
                                                      TKN   = total Kjeldhal nitrogen     pH    m pH                                  25                      oxygen demand

                                                                                           B-11

                                                                  Sample Stations: Columbia

      Station  ITenp I DO I pH ISaLtICondtI TSS ITurbICotorITransIAtklHardj 9005 1 NH3   No2 ITKN I TP I TOCI Cl I Phen IMetalslPest  IOther I Total IFecaLIFtw I Sed  ISed I
       No.  N        NI         I    I     I     II                        I I I    IPCBs IN                            I                           CoI  I  EHI  I         ' IIOrg*I

      -007        M  I          I          I     I M  A    M                           M     M      M    MI I    I    I   I  I     I              I       I  A      M  1.A   A

      c-00     I     I          I             I           I             I    I.     I      I     I 8I      I    I    I              I     I       I       I       I     A M         I

      C-017         MINI                         M          M I           A IM    MIIMIMIMI   I                                 I        I  A             IN   IIa M         I

      C-021           li      ii  I              II         I        III            I      I       11         1           I  I        I     I       I     I         I         I     I

      C-022       MfI MI                         I     I      I      I         M       M     MMIMINIOI               I       10A    I             I       I I   I                   I

      C-025    1 m I  I    III  I                IM I       I      I          I          I        1 1 1 1               I      I     M  I      I      I      I      I               I

      C-048    I    N  I  N           I N           I        I     I I  M        I     I    I I  I    N  I  I    M  I        I  0      I      I   I          N

      C-058       M  ILI I I               I     II         I      I I I            I      I      1 1 1 1 1                  I      I     I       I        I      I     I           I

      C-061    I IM    I NI   I               I   M      I      I    I    I N I MMI                     I     I      I       I      I     I       I        IN

      C-063    I      I      I            II          I              I          I         I      1 1 1 1 1                  I      I     I       I        I      I     I     I

      C-066    ININ                  I I         InI        I      I    I    I      I        M          MI      I    I       I      I     I       I        I      I M

      C-067       M lI        Ii                                              I I        I I       I           I I                          I M  m  I                         I

      C-068       N I       M        I           IN          I     I    I MIN              INI           IN     I    I  A           I     I MI             I      I     I     I     I

      C-069           I      I            I     II         I         I        I         I        1 1 1 1 I              I    I       I       I      I      I      I               I

                                                        Temp = temperature                   Salt  = salinity            Trans = transparency            Sed sediment (routine)
    M = monthly, Q   quarterly, A  annually       no        = dissolved oxygen              Condt = conductivi ty      Atk   = alkalinity               Sed Org  sediment organics
                                                        TSS   = total suspended solids       Hard = hardness             TP    = total phosphorus        Metals  heavy metals
    *Base-Neutral and Acid Extractable, and           Phen = phenots                        Turb  = turbidity          TOC m total organic carbon       Fecal Coll = fecal cotiform
       Volati le Organics                             Pest =  pesticides and PCBs          Other = other organics    11H3 NH 4 =ammonia                Total Coli = Total Coliform
                                                        Flow  = flow or stage meas.          Cl   = chloride&            N02 N03 = nitrate-nitrite SODS  = 5-day biochemnical
                                                        TKN   = total Kjeldhal nitrogen      pH    = pH                                                          oxygen demand

                                                                                               B-12

                                                               Sample Stations: Colurrbia

      Station  ITemp IDO I pH fSalttcondtl TSS ITurblCotorlTranslAlkljHardl  OD5   NH3 1NO2 JTKN I TP ITOC I  l I Phen IMetalsIPest  IOther I Total j FecaLIjlow ISed  I Sed I
       No.                                         I I     I               I         H4INO3        I   I    I   I        I      IPCBs  IOrg*   I Coli  IColi             I IOrg*j

     CSB-00L     M IM  I I M                 I I    I    I       I                                    I M       I      I M      I I    I   I                          A I  A I    I  IA  A

     CSR-00IR    M  IM 1         I M      I     I M       I       M      A I  M      M    M I   M I    M           I            I A           I    A I       I M         IA  I

      CW-040      M       1M  M     I       MIMI           I     IMIAIM                   M M          IMI        I      I                               MI I    A   1  M

      Cl-206                              1'1        I     I     I      I M    A    M  M    M   1      1       1  I       M           I       i       I A          I     I A

      CW-207   I     I    I    I      I         I M        I     I             I I      I I   I         I    I    I             I     I       I       I      I     I   A   A

      CW-200   I8MIMI         I           I I   1          I        I lAI         I    I           1141 IM               I      I         I       I   IN]          I M     a

      CW-209  I M I          l            I     IM    M  M    MI                        I   A1                     Im           I     I  a        a          I     I A         I

      CW-1220    1     4      1     11M     M              I M      M   AIM          M I IIM   M       IMI           M       M alA        Al          I       I      AI   I A

       E-034    MI   l     i              I    I I         I        I        I        I                1                 1. I  I       I      I     I      I      I

       E-035    MI   1111                 I     1.1           I  III                         I A                      I         I    I        I       I      I     I     I    I

       E-101  M       M I I    I   I      I      MI  I     I     IAI              I     I     I   I I              I I       A  I     I       I       I      I     '  I        I
      CW-209   114114 II II    114 1                         IMIMIAIM    IMI MIMIMIQI                             I        I Q    I       I.      I  114           (A          I

       S-042  I M                               IM                         I M  I  I    I    I III  I    I 1             I      I     I I             I      I I  I  I

       E-099    INIM       MI       I     I      1         I     I    I    IM   I    11                      I    I      I      I     I       I       1            I

       S-10 2    M I  I   I    I    I        I  I    I     I     I    I    I    m       I     I    I    I    I    I      I      I     I       I       I      I     I     I     I
                                                      Terrp mtemperature                  Salt  = salinity           Trans m transparency           Sed sediment (routine)
    M  monthly, 0 = quarterly, A  annually           DO   = dissolved oxygen             Condt = conductivity       Atk  = alkalinity              Sed Org  sediment organics
                                                     TSS   =total suspended solids Hard = hardness                  TP    = total phosphorus       Metals   heavy metals
    *Base-Neutrat and Acid Extractable, and          Phen = phenots                      Turb = turbidity           TOC = total organic carbon     Fecal Coti = fecal cotiform
       Volatile Organics              Pest   Ipesticides and PCs O                        ther =   other organics N  H3 NH  4   ammonia            Total CoIi =      total  coIiform
                                                      Flow = flow or stage meas.          Cl   = chlorides           N02 N03  = nitrate-nitrite   H OD 5 =5-`day biochemical
                                                      TKN   = total Kjeldhal nitrogen     pH    = pH                                                        oxygen demand

                                                                                           9-13

                                                              Sample Stations: Columbia

      Station  ITemp I DO   1 pH ISattlCondtl TSS ITurbIColorITransIALklIHardI BOD5 1NH3   I N02 ITKN I TP ITOC I CL I Phen IMetalslPest  IOther  ITotal IFecallFlow I Sed  ISed I
       No.            I    I    I    I     I      II         I     II         I      INH4I NI3                  I                    IPCBs  IOrg*  I CoL  ICoLiI          I     IOrq*I

       S-149    M    M                                  M                M                   M m          M                   I      I      I                  M

       S-150  MI             M I    I I       I   M  I       I     I    I    I       I  I      I M          I    I    I  I        I         I I                M I  I  I              I

       S-151      M    m I   M I  I        I I      I     I     I     I    I     M   I      I     I       I    I M     I      I      I      I       I   I       I         I           I

       5-152                         I     I      114        I     i    I    IMM              M 11                I    I      I      I      I       I       IM

       S-204    M  M                              II         I   111.1                      I   1111.1                        I    I I         A I M       I    I    IM0     A
       S-215   1114          41 M    M            114        I     I    I    IN    I                                                                           M114      III14

           I          liii                I  I mI I          I     ImI   I           I     I   I       1 1 1                  I      I MI           I MI           I      I     I MI

       S-213   I     I M      II   I              I m  I     I     III   I                I        1 1I 1I M             I    I       I      I       I     I      I       I

       S-223   I      I M       I    I     I      I    I     I     I    I    I       I      I     I M        I    I    I      I       I M           I        I M          I     I     A
       S-260  111414    I M                       14    I   INA  M  IMIMIMINO                                          I   I   II                           IN    M IAI
       S-27 0     M  I       I           I I     I M      I     I     I    I   I                 I     I I M      I     I     I I    *I     I       I       I       I I  I  I

       S-273      M     I       I    I M  I         I        I     I    I    I       I      I M           I A     I    I      I          I  I       I        I      I M      I        A

       S-27           I    4    I        I          I        I     I     I    I      I      I     I    I     I    I    I      I M     I     I       I        I MI         I M         A
           I-7 111 HI IM IMAJ 1.11 I II~a 111   I I I I I I I

       5-26  141414 I                      II  114 IH    IMIAIM  II  MINIMIOI   I                                                0    I   I    I N   I  IAI     I

           I-7        til             II           II IM              I I   IM             I       1 1          1       IIIP         I      I       I       I       I     I     I

       -27 1             I         9 I             I      9        I I I             I      I M  M                            I A  I    I  I MI             I         I      AM        A

       S-280                                         M    M      M l  I                             I 1                 I             I  I      I       I       IM     I     I   A
                                                     Temp  =temperature                   Salt  =salinity              Trans= transparency             Sed   sediment (routine)
    M = monthly, 0 = quarterly, A   annually    n       o    = dissolved oxygen              Condt   conductivity        Alk   = alkalinity               Sed Org = sediment organics
                                                     TSS   = total suspended solids        Hard  = hardness            TP    = total phosphorus   M      etaLs = heavy metals
    *Base-Neutrat and Acid Extractable, and            Phen  =phenols                        Turb  = turbidity           TOC = total organic carbon       Fecal Coli = fecal coliform
       Volatile Organics                               Pest  =pesticides and PCBs           Other = other organics       NH3 NH  4 amnonia               Total Coli = total coliform
                                                     Flow  = flow or stage meas.          Cl    = chlorides            NO  N03  = nitrate-nitrite      BOO  = 5-day biochemical
                                                     TKN   =total Kjeldhal nitrogen       pH    = pH                                                            oxygen demand

                                                                                          B-14

                                                                    SampLe Stations: CoLumbia

                I I I I I I' I I I I I I I I I I I I
                                                                                                                                         I I I                                       I I I I I I
     Station ITemp I DO I pH ISaLtlCondtl  tSS ITurblCoLorlTrenslAtkLIHardl  SODs II  NH3                                                                                              NO2   ITKN I TP ITOC I Cl   I  Phen IRetalslPest I Other I Total   I
                                                                                                                                                                            FecaLlFLo. I Sed I Sed I
       .o. I I                                 I          I I I                               I          I I I I I NH4                                                                 "% I I I I I I IPCBs I  Org* J Coti I Coti I I I
                                                                                                                                                                                                  org*l
                I I I I                                     I I I I I I I                                                                      I              I                        I          I         I I I
                                                                                                                                         I I I I I I I I I
                I I I I I                                                I            I         I I I I I I I I I                                                                                                      I
                                                                                                                                 I I .I                                    I                I                I              I            I            I           I
       s-287            I M IM I MI I I IM I I I I I M                                                                                                                I I I    MI I I I I I I I
                                                                                                                                                                             M I I I I
                I I                    I         I I I I I I I I I I I I I                                                                                                                                             I          I              I
                                                                                                                                                 I I I I                                                      I            I I I
       S-290 I M IM I MI I I IM I I                                                                                               IM I AIM I  M I MI  .1 el I I    o I I I
                                                                                                                                                                          I M I I A I I
                I I I I I I I                                                                   I            I I I I I I                                                                          I I I I I
                                                                                                                                                 I           I                I I I                                        I I I
       S-~4 I M IM   I  MI I I  M   IM I I IM   I AIM I M                                                                                                                                       I  MI MI  Ol I I   O I I I
                                                                                                                                                                          I M I    M I I                                       I

                                                            Temp = tenperature Salt - salinity Trans = transparency Sed = sediment (routine)
    H -- monthly, Q = quarterly, A -- annually DO -- dissolved oxygen Condt = conductivity Ark = alkalinity Sed Org = sediment organics
                                                            TSS = total susl~qlded solids Hard = hardness TP = total phosphorus HetaLs = hea~f metals
    � Base-Neutral and Acid Extractable, and Phen = phenols Turb = turbidity TOC = total organic carbon FecaL Coti= feca[ cotiform
       Volatile Organics Pest = pesticides and  PCBs Other = other organics NH3 NH4 = ammonia Total CoLi = Total CoLiform
                                                            FLow = flow or stage meas. CL = chlorides NO2 NO3 = nitrate-nitrite BOO5 = 5-day biochemical
                                                            TKN = total KjeLdhaL nitrogen pH = pH oxygen demand

                                                                                                     B-15 ~.

                                                              Sample Stations: Florence

      Station  ITenp I DO I pH ISaltCondtl TSS ITurbjColorITransIAlklIHardl BOD5 O  H3 I  N0 2 ITKN I TP ITOC  I Cl   Phen IMetalslPest  Other I Total   FecaltFLow  Sed I Sed I
       No.     J                                                                   NH4 I NO3      I                            PBS  Org*   Coli  I Co               I   Org*

      MD-073   I MIM  I   MI   I M              I   I    I       IM I   I                        I     I   I      I                   I I    I  I   I                        I

          MD-0 I    I    I  I   II             I    I     I     I    I    I     I     I     I    I    I    I    I      I      I     I       I       I      I    I     I     i

      MD-07       M  I M  IM I M i I M             1       IM   I M       I M       M   M  I    1 M          I                  I  M                       I1    I    I    I M

        MD HI        li   I   I          I    I  I    I    I   I   I    I   I   I                                      I      I    I        I       I      I    I    I    I

      MD-07  IM             M IMIM        IM         I    I       MIA  I M   I MIM MI M I               M I I   I       I                              M I    I  I           I

      MD-0    |  M  IM    MI M    M      I     M   II                                   I M  I   i MI    I   I          I      I    I       I       I            I    I  I

          M08I      i Im     I  I m            I  I I     I    III           I           M    I            I   I       I      I    I        I       I      I    I    I    I

      MD-077     MII M SIIMI              I    IMI    I    I   I    I              M  1         M   MI 0  I   I         I      I    I       I                                I4 m

          MD-0 I    I   I II             I    II          I    I   I   I         I  I   I    i   i                     I      I    I        I       I      I    I    I    I

      MD-08      M M1I MIMIMIM IMM                        I             A I1M         M  I  IMI M         I      I      I      I    I       I       I      I I  I
               i     I        I II                  I I i                 II     II    I  I  I    I I I  I  I                 IIi  II  I  I    I  I  I                 i    I

      MD-107  I    I  M              I M  M    I      M  I           II          I                  M I   I   I         I      I    I       I       I      I    I
          ID08      I   I   I114 I41 I4    I1I            I    I   I   I        I I  114         I1I   I   i           I      i    I        I       IN    I    I    I    I

      MD-110     M  I M    M I       M I M      I M  I     I    I   I   I M   I    I M               M I   I   I                                      I    I                 I

      MD-1108    M I MI  M I M I M  I4 M  I    I    I   I   I M                           M         M       I   I       I      I    I        I      I M

                         I I I~Tep =temI                       perature                 Salt I I  I    i    II  lI I    I      I    I        I       I      I    I    I    Ine)

    M = monthly, 0 = quarterly, A = annually        DO    = dissolved oxygen            Condt  conductivi ty      Atk  = alkalinity              Sed Org  sediment organics
                 MD-089ITSS   =total suspended solids                                  Hard I  hardness           TP    = total phosphorus      Metals   heavy metals

    *Base-Neutraand Acid Extractable, and           Phen = phenos                       Turb = turbidity          TOC = total organic carbon    Fecal Col = fecal coliform
       Volatile Organics                            Pest =  pesticides and PCBs         Other  other organics     NH 3 NH 4 = ammonia            Total Coli = total coliform
          MD01 I M lIM I MIMIM  I    I MI                 I    I   I   I M I    1 M 1I           I11I I1               I      I    I        I       I M I    I    I          I

                        Flo  =flo or stage meas.                                        C       chlorides          N2 N03  = nitrate-nitrite      B 5    day biohe11ica1                1 1
          MD17 I M lIM I MIMIMI                IMI        I I    I       I I    II    I   I    I   11I1         I      I      I    I        I       I M I    I    I    I

                         -09  1TKN   = total Kjeldhal nitrogen                          pH      pH                                                       oxygen demand

                                  I  I  I  I    I  I  I    I     I    I    I      I     I     I    I   I    I    I      I      I     I       I       I      I     I     I -16
          MD11 I M 1 MI  1IM             I    I MI        I    III    |         I  I M  I I11I               1         I      I    I        I       I M I    I    I          I

          MD14 I M lIM I MIMIM  I              I MI       I    IMI  AI   M I MI M 11MI1 IQ 1                           I  QI AI             I       I M I MI AI    I

                                                     Temp  = temrperature               Salt  = salinity           Trans =transparency           Sed = sediment (routine)
    M4 = monthly, 0 = quarterly, A =arnually        DO    =dissolved oxygen             Condt =conductivity       Alk   = alkalinity             Sed Org =sediment organics
                                                     TSS   = total suspended solids     Hard  = hardness           TP    = total phosphorus      Metals = heavy metals
    *Base-.Neutral and Acid Extractable, and        Phen  = phenols                     Turb  = turbidity         TOC = total organic carbon     Fecal Coli = fecal coliform
       Volatile Organics                            Pest  = pesticides and PCBs         Other = other organics    NH3 NH4 = amrmonia             Total Coli = total coliform
                                                     Flow  = flow or stage meas.        Cl    = chlorides          NO2 NO3 = nitrate-nitrite     BOO5 = 5-day biochemical
                                                     TKN   = total Kjeldhal nitrogen    pH    = pH                                                       oxygen demand

                                                                                         B-16

                                                                                            SampLe Stations- FLorence

                     I I I I I I I I I I I I I I I I I                                                                                                                                                      I I I I I I I I I                                                                                                    I I
       Stati~ IXemp I 00 { pH {Satt{CondtI XSS ITurblCoLorlTranslAtktlHardl 8005 II ..3 11 "02 ITK" t TP ITOC I CL I Phen IMetatslPest I Other { TotaL { FecatlFto. I Sed I seal I
        ,o. I                       I I I I I I I                                                             I I I                                           H,4         ,o] I
                                                                                                                I I I I I I                                                                                            IPCBs I Org* [ CoLi I coti I I
                                                                                                                                                                                                                                                               I org*l
                     I I                  I I I I I I I I I I '1 I I I                                                                                                                             I I I I I I I I                                                                                        I           I          I           I
                     I          I         I         I         I           I           I        I           I          I         I         I             I          I I I I I                                           I            I I I I I I                                                                       I I
       MD-125 I M IN I .1 al 14   I IN I I I I I M I I M I I .1 I I I I I I M I M I I I
                     I          I         I         I         I           I           I        I           I          I         I         I            I           I I I                           I         I         I            I I I                                    I               I            I           I           I
       MD-127 I M                    IM I M I    H I    M                     I           IM        I I I MI AIM                                            I    M     I    M      I    H I    M I    Q I I I Q I I I M I M                                                                                    I          I A I I
                     I          I         I'        I         I           I          I         I           I          I         I         I            I           I           I         I         I         I         I            I             I           I              I               I            I           I I I
       MD-136 I M IM I M I    .1 M I IM I I I I I M I I    M                                                                                                                       I I M I I I I                                                      I I I I M I I I I
                     I          I         I         I         I           I           I        {           I          I         I         I             I          I           I         I         I         I         I            I             I           I              I               I             I          I           I           I
       MD-137 I # IN I MI MI M I IM I I I I                                                                                                   I    M I I M I I M I I I I I I I                                                                                                                   I    t4       I          I I I
                     I          I         I         I I I' I I I I                                                              I         I             I          I           I         (         I         I         I            I             I           I              I               I             I          I           I           I
       MD-138 I M                    IM I H I    H I    M I IN I I I I                                                                        I    t4       I I M I I H I I I I I. I I                                                                                                           I    t4       I I I                              I
                     I          I         I         I         I           I           I        I           I          I         I         I             I          I           I         I I I                         I            I I I I I I I I I
       M0-146 I M I# I M I M I M I IM I I M I A I M I M I M I M I M I 0 I M I I 0 I I I I # I I A  I I
                     I I I I I I I I I I I I I I I i                                                                                                                                               I         I         I I I I I I I I                                                                                            I           I
       MD-149    I  M IN I M I M I  M I IM I I I M I A I M I M I M   I  M I t4 I a I I I Q   I I I I M I I I I
                     I I I                          I         I           I I I I I I I I I I I I I                                                                                                                    I            I             I I I I I I                                                                     I I
       M0-158 I 14 IN                          I    141 14 1    t4    I                   IM I I I I AIM I I M I I MI I I I A I I I I M I I A I I
                     I          I         I         I         I           I           I        I           I          I         t         I             {          {           I         I         I         {         {            I             I           I              I               I             I          {           I           I
       t4o-162         'l    14      IM       I    1,41    M   I    t4    I               IM        I          I' I    M   I    A I M                       I    M      I    M I M   I    M I e I I I Q I I I M I # . I    M I A I I
                     I          I I I                         I           I           I I I ! I                                           I I I I I I                                                        I I I I I I I                                                                                 I I I I
       PO-012            I    fl    IM        I    M I            I           I           It4    I             I           I    H I AI    14                I    14    I    M      I    141    M I    e l                  I             I      Q     I A I                       I I M I M I A I I
                     I          I         I         I I I I I                                              I                    I         I I I I I I I I i I I'.                                                                                                            I               I I I I I
       PD-014 I M I M I #1 I                                                  I           I  M      I          I                    f         I    M        I           I    M     I         I    M   I          I         I             I            I           I              I I M                         I ....l,               I           J
                     I I I I                                  I           I I I I I I I                                                                            I I I                           I I ! I                                        I           I              I I I                                    I I I
       PD-015 I  M   IM   I MI I I IM.J~                                                                       [~                   I AIfi    i                         I  ~ I I  .1 I                                     I             I    A   I               I              I               I  M          I I I                              I
                     I I I                          I         i I I I I I I I I I I I I I I I                                                                                                                                                                 I              I I I                                    I I I
       PO-016 I M                    IM I MI I I IM I I I I M                                                                                               I I M I                          I    M I I' I I                                          I           I              I               I ff I                    I          I           I
                     I          I         I         I         I           I I I I I                                                       I I I I I I                                                        I         I I I I I I I                                                                                  I I I
       PD-017A I M                  IM I t41 I I IM I I                                                                             I I M                   I I M I I    M I I I I I                                                                              I I I M I I                                                         I           I
                     I          I         I         I         I           I '1                 I           I                    I         I             I          I I I                           I         I         I I I I                                               I I I I I I
       PO-021            I    14    IM        {    141            I           I           IM       {           I           I    14 1 A{    M                J    14    I    14    I    t41    H {    Q I                   I             I      Q     I           I              I               I    t4       {    14    I           J           I
                                                                              Temp = temperature SaLt = salinity Trans = transparency Seal = sediment (routine)
    14 = monthly, Q = quarterly, A = ar~uatty DO = dissolved oxygen Condt = conductivity ALk = aLkaLinity ' Sed Org = sediment organics
                                                                              TSS = total suspended solids Hard = hardness TP = total phosphorus MetaLs = heavy metals
    � Base-NeutraL and Acid ExtractabLe, and                                                        Phen = phenols Tt]rb = turbidity TOC [] total organic carbon FecaL CoLi =fecaL coLiform
        VoLatiLe Organics Pest = pest(cides and Peas Other = other organics NH3 HH4 = ammonia Total CoLi -- total co[Jform
                                                                              FLow = flow or stage meas. CL = chlorides
                                                                                                                                                                              NO2 NO3 = nitrate-nitrite BOO5 = 5-day biochemical
                                                                              TKN   = total KjeLdhaL nitrogen pH = pH oxygen demand

                                                                                                                                   B-17

                                                                 Sample Stations: Florence

      Station  ITemp I- DO I pH ISaltICondtI TSS ITurbIColorITransIALkljHardI BOO5 1NH3 I 402 ITKN I TP ITOC I CL I Phen IMetalslPest  I Other I Total I FecatIFLow I'Sed I Sed I
       No.                                                                         "INH4INO3I                     N IPCBsIOrg*  IColi" Co"i                                   1Org~j

      PD-023          li I  M       I                                                    I    I       I                                                  I I   I I   A M  M  I M    M  I  I  I
      P0-02314114 II Ii    111                                     IMIAIM            INIMIMIMlal                     I       I a   I      I       I       1411 I                    I
      PD-025    MI           I M        I M      I    I      I     IM     I                    I     I     I A       I M  I    I           I M        I M        I M       I 0      I

      PD-027   M     M       M        M     M    m  I                M     A     M     N     M       M N    M                  0     A            A          M   M         A A
      PD-028   1141414    I                         I                I       t               M M       MIQI          I       10A          I       I        1141141 M A

      PD-029 E    I   l                    I     II          I        I        I        I         1 1 1 1 I              I    I       I       I      I      I      I               I

      PD-030        1                1141141141    I   IMImAIM                               M                       I    1   IAI  A                      In  IA

      PD-031      M   M      M                     mnl       I     I            M            M           M                                                   MI I

      PD-035      M   M      M                     Mwl       I     I            M            M           M                                                   MII I

      PO-036   M    N        M                   (H(         II     M           M            N           N                                                   MI    II

      PD-037      M     I   M   IM   I     I     I     I     I     I    I    I      IM      I M  I         I    I    I       I      I     I       I        I      I           I     I

      PD-038      M M   I    I          M           I       I m  II M                                 I I      I I                            A I M  I M  I M  I M      I I   I A

      PD-039           I             I I         I     I I  I           I I  I  I   I     I                I    I    I I  I     I      I       I      I      I                I     I

      PD-      I41                         I     I          I          IM          I         I MI I            I M                 I     I       I        I      I M         I A

      PD-042      M 1                              I I       I     I I I            I      I      11                         I      I     I       I        I      I A M        A
                                                        Te0p  = teperture                    Salt    salinity            Trans = transparency            Sed 1  sediment (routine)
    M = monthly, Q = quarterly, A  annually           DO    = dissolved oxygen             Condt  conductivity         Atk   = alkalinity               Sed Org  sediment organics
                                                        TSS   = total suspended solids       Hard  hardness              TP    = total phosphorus        Metals  heavy metals
    *Base-Neutral and Acid Extractable, and           Phen  = phenols                      Turb  turbidity             TOC = total organic carbon       Fecal Coli = fecal cotiform
       Volatile organics                              Pest =  pesticides and PCBs          Other = other organics NHJ NHq  ammonia                     Total Coli = total coliform
                                                        Flow=   flow or stage meas.          Cl =    chorides            NO2 NI3 I  nitrate-nitrite      BID5 =5-day biochemical
                                                        TKN   = total Kietcdhat nitrogen     pH   =- pH                                                          oxygen demand

                                                                                            lB-18I

                                                                  Sample Stations: Florence

      Station  ITemp I DO I pH ISaltlCondtl TSS lTurbjCotorlTranslALkllHardl ROD5 I NH3 1 NO2 ITKN I TP ITOC I Ct IPhen IMetalsiPest IOther I Total I FecallFLow I Sed ISed I
       No.            I    I    I    I      I      II         I      II        I      INH4INO3                                          IPCBsIOrg*  IColi IColi                 I I Org*

      PD-043      M Mi        M                     M                 M IA        M       M     m M         M IP                    a                                    M    M IH'  A

      PD-044      M   M       M                     M                             M   I I       M           M                                                     mI I

      PD-045      M M M       M                     M                             mI   I I      M           MI                                                     m

      PD-052         M    M  MI                              M        M    A      M    M        M    M  m    0                      aI        I        I              M  M      A

      PD-055       I   M   I      M         I      I    I    I    I    I   M    I        I         I     I I   M    I        I          I I     I              I I  I    I               I

      PD-061      M 1.              1       I MI              I       l                I M    M      11A                        I M           I MMI            I  A I        I     IA   A

      PD-0691141141141   I   I M1                                    IMIN         M  IMIMIMIMIal   I    I 01    I                                      I       II                         I

      PD-085    M  I             1 I  M  I              'I    I  I M  I    I     I    I    I M              I         I   m   I    I                   I I  I     I      I                I

      PD-016 A IMIM                I        I      114        I      I          I           I           1          I    I      I       I     I        I       In    I       I     I      I

      PD-087  I        I      i             I     1.1         I     I I I             I     I       1 1 1 1 1                  I       I     I        I       I MI          I            I
      PD-045   11414114               I     I      1141       I      I    I    I       I     114         114        I    I      I       I     I        I       114           I

      PD-091A          l i ii               I         I        I  I       It                      I      I M                    I       I     I        I       I M           I M    A

      PD-097      M I  l I ii MI                         I        I    II     I        I     I           1          I A         I       I     I        I       I       I     I     I      I
           ID09        I       i i          I      I        In        IMI I            I     I       t 1         1       *        II P        I        II n   I              I     I

           P-0    I M l i l                 I      II          I      it                        I   1 1 1 1                     I       I     I        II              I     I

                                                        Temrp  = temrperature                 Salt  = salinity             Trans = transparency             Sed sediment (routine)
    M = monthly, Q   quarterly, A  annually         DO        = dissolved oxygen              Condt = conductivity         Alk:  = alkalinity               Sed Org  sediment organics
                                                        TSS   = total suspended solids        Hard  = hardness             TP  =   total phosphorus         Metals  heavy metals
    *Base-Neutrat and Acid Extractable, and             Phen  = phenots                      'Turb  = turbidity            TOC = total organic carbon       Fecal Coli = fecal coliform
       Volatile Organics                      Pest I psticides and PCBI                       other 114ther organics NHI3 '4  =ammoia  Tota I14   I total cotiforI
                                                        Flow =  flow or stage meas.           Cl =    chlorides N02 N03 =nitrate-nitrite                   R OD15 =5-day  biochemical
                                                        TKN   = total KjetdhaL nitrogen       pH    = pH                                                            oxygen demand

                                                                                               B-19

                                                                Sample Stations: Florence

      Station  ITemp I00 I pH ISaLtlCondtI TSS ITurbIColorITransIALkLIHardj BOD5 1 NH3 1N     O ITKN I TP ITOC I CL I Phen IMetalslPest I Other I Total I FecalIFLow I Sed ISed J
       No.                                  N I   I  i  I                   I IN                   I              I          I  JPCBs I Org*  I Coli  I Coli       I     IIarg*I

      PD-098      M    M     M                    mI             I            M            M          MI                                                   M

      PD-103        I      M        I I M  I         I       I     I    I      I    I                I    I M     I   I      I   M        I       I       I   M

      PD-106      M            I                II IMI    I    I                  I                  I                   I      I     I       1 M         I        I M  M

      PD-107     M  I    M    I M              I     I   I      I I            I    I          1           1       I   I    I       I      I      I      I      I              I

      P0-112      M IMI   M I       I     I  I14    I         I    I    I       I            1     114   I    I          I  I      I          I          I      I              I

      PD-115     M    M       I  1              I    I        I    I   I                I       I I    I        I        I      I     I       I       I      I     I     I    I

      PD-116      M  II  1                I        I    I     I    I      IM  I              I    I                      I      I I  I     I      I      I      I              I

      PD-107   114114114    I                I  1       I     I    I    I M I           1          1            I   I      I      I     I        1       I      I m

      PD-14       111  I                        II         I        I        I        I        1 1 1 1  I             I    I       I      I      I      I      I              I

      PD-143          l        I                II I                 I            I I  1     I        I43 I                   I     I          I     I      I      I M

      PD-159   1141414    I               I     1141          I    I    I 1                  1         1  I    I      I      I     I      I       Im         I  I   A

      PD-'168     M  M                                 M              M       M            m                      I      I      I        M               M

      PD-169   I     I    I    I    I     I     IM   I     I         I       I      I         I   I   I      I I    I           I I  I                I I  I  I    I

      PD-170                        I     I     11               I   I           1      1          1       I      I      I      I     I       I       IM      I     I M         I

      PD-172     Ii I M  I H                 I  I   I      I     I   I    I       I     I I        I   I    I    I       I      I     I       I        II           I     I 4
                                                      Temp  =temiperature                 Salt  = salinity           Trans = transparency           Sed= sediment (routine)
    M    - monthly,  quarterly, A   annually D O           =dissolved oxygen             Condt =  conductivity      Ak  = alkalinity               Sed Org 1   sediment organics
                                                      TSS   = tots( suspended solids      Hard  = hardness           TP    = total phosphorus       Metals  heavy metals
    *Base-Neutrat and Acid Extractable, andl         Phen  = phenots                     Turb  = turbidity          TOC = total organic carbon     Fecal Coti = fecal cotiform
       Volatile Organics                             Pest  = pesticides and PC~s         other = other organics     NH3 N =  ammonia               Total Coti = total coliform
                                                       Flow  = flow or stage meas.         Ct   = chlorides      NO2  N03 = nitrate-nitrite          BOD5 = 5-day biochemical
                                                      TKN   = total Kjetdhat nitrogen     pH    = pH                                                        oxygen demand

                                                                                            B-20

                                                                                                    Safi~ole Stations: FLorence

                      I           I         I          t         I           I           I          I           I            I         I          I             I                        I         I         I         I         I              I             I            I               I                I              I           I           I            [
       Station ITemp  I O0 I pH ISa[tlCondtl TSS  ITurblColorfTranslAlkLlHard~ BOO5  I NH3                                                                                                             I
                                                                                                                                                                     TP ITOC f C! J Phen J14eta[sJPest J Other J Total J FecaLJFlow J Sed J Sed J
                                                                                                                                                   "02 ITKN
         .o. I I I I I I I I I I I I N"4    "�3 I I I I I I IPCBs i org* I Coli I Coti I I I Org*l
                      I I I I I I I I I I I                                                                                                       I             I I I I                                                I         I I I                                     I I I I I I                                                                          I
                      I           I         I          I         I           I           I          I           I            I         I          I             I                        I*        I         I         I         I              I             I            I                I               I              I           I           I            I
       PD-176 I 14 IM I MI I I IM I I I I I M I M I I    M I I I I I I                                                                                                                                                                                                                          I I H I I I I
                      I I. I I I I I I I I I I I I I I I I I I I I I I I I I
       PO-1T'/'           I    ~      114       I    M I             I           I           IM         I            I           I         I I M                    I                 H      I         I    141 I                     I             I             I            I                I               I H I I I                                           I
                      I I I I I I I I I I I I                                                                                                                   I I I I I I I I I I I I I                                                                                                                                                           I           I
       PD-186 I M                     IM        I MI                 I I IM I I I I I H I M I I MI I I I I I I I ,                                                                                                                                                                                                             I           I I I
                      I           I         I          I         I           I            I         I            I           I         I          I             I                        I         I         I          I         I             I             I            I                I               I              I I I                                I
       PD-187 I M IH I HI I I 114    I I I I I M I M I                                                                                                                                                 I  M  I I I I I I I I M I I' I I
                      I I I I I I I                                                                 { I I I I I I I                                                                                          I I I I I I I                                                                                  I I t I I
       P0-189 I M 114   I  141 I                                                 I           IM    I                 I           I  141 AIM                         I  14             M   I  141  141  el  141    Q   I    Q   I                                               I                I                I  H          I  M   I  A    I                     I
                      I           I I I I I I I I I I I I I I I I I I I I                                                                                                                                                                                                                   I I I I I                                                           I
       PO-190 I HIM   I  HI I I IM I I I I I  14 I 14 I I 141 I I                                                                                                                                                                                   I I t I I H                                                                I           I            I           I
                      I I I                           I I I I I I I I I                                                                                         I                        I         I         I          I         I             I             I            I                I               I              I           I            I           I
       P0-201 I H 114 I HI I I IM I i I I I H I M I I MI                                                                                                                                                                    I I I I I I I M I I I I
                      I I I I I I I I                                                                           I I I I I I I                                                                                I          I I I I I I I I I I I
       P0-202 I ti                    IN I 141 I    14                           I    #      IM         I            I           I    H I AI    H                   I    14           M      114       I    14 1    M I               I             I    O         I A I A I                                     I    14       I    14    I    A        I    A      I
                      I I I I I I I I I I I I                                                                                                                   I I I I I I I I I I                                                                                                                         I I I I I
       PO-203             ~    14     I  M      I    14   I          I           J           I  14      J            I           I         I          I    H        {                 14     I         J    H   ~           I         I             I              I           I                I                I    14       |           J            I           I
                      I           I         I         I          I           I           I          I           I            I         I          I             I                        I         I         I          I         I             I             I            I                I               I              I           I            J           I
       PD-227 I H IH   I  HI                                         I I IH   I I I HI AI H I H                                                                                       H IH   I  HI  OI I I O                                                       I A I I I  H                                                I  H   I A I I
                      I I I i                                    I I I                              I           I            I         I I I I I I I                                                                              I             I             I I I I I I I                                                                                     I
       P0-229 I H                     IH        I    H I I I IH                                         I            I           (         I          I    14       I                 14     I         I    14 1            I         I          'l                I           I                I                I    14       I           I            I           I
                      I           I         I          I         I           I           I          I           I            I         I          I             I                        I         I         I          I         I             I             I            I                I                I             I           I            I           I
       P0-230 I H IH I HI I I IM I I I I I  H I H   I I 141                                                                                                                                                                 I I I I                                            I                I I 14                         I I I I
                      I I I                           I          (           f           I          I           I            I         I          I             I                        I         I         f          (         (             f             I            I                I                I             I           I            I           I
       P0-231 I M IM I MI I I IM I I I I I M I H I I    M I                                                                                                                                                                 I         I             I I I                                       I I H I I I I
                   I I I I I I I                                                                     I           I            I         I I I I I I I                                                                             I I I I I I I I                                                                                                    I           I
       P0;236 I    H                  IM I    H I I I IH                                                I            I           I         I          I    H        I                 14     I         I    14 1            I         I             I              I           I                I                I    H        I            I           I           I
                      I           I I I I I I I I I I I I I I I I I I I I I I                                                                                                                                                                                                                                              I I I I
       PD-239 I H IH I HI I I IH I I I I I H I M I I HI                                                                                                                                                                     I I I I I I I H                                                                                    I I I I
                                                                                     Tenso = teffl~erature Salt = salinfty Trans = transparency Sed = sediment (routine)
    14 = monthly, Q = quarterly, A = annually DO = dissolved oxygen Condt = conductivity Atk = alkalinity Sed Org = sediment organics
                                                                                     TSS -- total suspended solids Hard = hardness TP = total phosphorus 14etaLs = hemW metals
    *Base-Neutral and Acid Extractable, and Phen =pheno[s Turb = turbidity ?OC = total organic carbon Fecal CoLi r. fecai coLiform
         Volatile Organics Pest = pesticides and PCBs Other = other organics NH3 NH4 = ammonia Total CoLi = total coLiform
                                                                                     Flow  r. flow or stage meas. Ci = chlorides
                                                                                                                                                                                              NO2 NO3 = nitrate-nitrite BOO5 = 5-day biochemical
                                                                                     TKN = tote[  Kjeldha! nitrogen pH =ptt oxygen demand

                                                                                                                                                 B-21

                                                               Sample Stations: Florence

      Station  ITemp  IDO I pH ISaltlCondtl TSS ITurbjColorITransAlkLkIHardj BOO  1NH    NO2 ITKN I TP ITOC  CL IPhen IMetalsiPest  I Other  I Total I FecalilFow I Sed  ISed I
       No.               NH4                                                          1 NO3  1   1   1   1   1        1      IPCBs  Org*  ICoLi  ICoLi               I Org*l

      PD-255   14141  4    I                I 1        I    I    I   I           I    1         1         I   I    I    I       I      IM     I      I               I

      PD-256   I M  IN I   MI    I I           IN  I    I    I   I A I4  I    I N  I I               1    I   I       I  A  I    I        I       I 1   I    I A  I    I

      PD-258         1111  I                   II         i    I   I   I        I    I          1             I           I    I  I    I      I      I     I M

      PD-258     M          I            I    1      I  I           I M   I       1    I   I                  I    I    I       I                 1       I  I  Im

      PD-281         I       Ii                          I IM           I m       I I                     I I  I 1              I      I M        I A       I I    I A

      PD-3068       INMI                      I    I              I   I       1           1         1  I       I  I      I      I     I           1       I  I M

      PD-310111  I                             II    I    I    I   I    I             I                 1             I I    I  I      I      I      I      I              I,

      PD-319         li      ii  I             II         I        I       I        I        1111 I                      I    I  I    I      I      I      I              I

      PD-320611414141                       I 1141           I    I   I 1             1          114      I   I       I      I    I       I       I      I M

      PD-321         li      ii  I             II            I       I       I                   1                    I      I I       I      I       IM    I    I   A

      ST018          lI     ii  I             II    I    I    I         I      I    I       1                I           I    I  I     I     I      I      I              I

      ST-024     M     I   M       I I         I M             I    I    I      I     I   .   I      I    I    I      I      I     I      I       I      I     I     I a
                                                      Temp =temrperature           S alt = salinity                Trans = transparency          Sed= sediment (routine)
    M = monthly, - = quarterly, A  Iannually D           =dissolved oxygen             Condt = conductivity A14        = alkalinity            Sed Org  sediment  organics
                                                      TSS  =�total suspended solids      Hard = hardness           TP   = total phosphorus       Metals  heavy metals
    *Base-Neutral and Acid Extractable, and        Phen = phenols                      Turb = turbidity          TOC = total organic carbon    Fecal toli = fecaL coliform
       Volatile Organics                                                                                                 Pest =pesticides  and PCBs  Other  = other organics    NH3 NH 4 = ammonia  Total CoHI= total coIiforI
                                                      Flow =1flow or stage me1s. CI =Ichlorides                    NO2N 03 I  nitrate-nitrite    BOD1 = 5-day biochemical
                                                      TKN  = total Kjeldhat nitrogen    pH   = pH                                                        oxygen demand

                                                                                           B-22

                                                             Sample Stations: Greenville

                     I   I   I   I  I     I     I   I     I     I    I    I      I     I    I    I    I    I    I      I     I     I       I       I'
      Station  ITemp I Do  I pH ISaltICondtl TSS ITurbjColorITransjAlklIHardj BOD5 1NH3 I N02 ITKN I TP ITOC I ClI  Phen IMetalsIPest I Other I Total IFecalIFlow  ISed  ISed I
       No.                                 N I  N        I I      I I      I                  I IPCBsIOrg*  ICol   ICoLi                                       I    IIrga

      8-00I              I    I I        I     I    I     I    I    I   M       I  A        I M      I    I    I      I      I     I      I       I    M    M   A
           I-0        1111I              I    II                I llIM             M  I I        I llPI                   I     I      I       I  I      I    I  I         I

      I-012      M     I  m        I M   I       I    I        I M  I   I    I    I              I   I    I   I       I I   I             I I  I     I     I M

      6-019    1141414    I                 I      1   I    I    I       1141           M        1      I   I    I       I      I      I             I      I M

      I-020          I   I    I      I         I    I     I    I    I    I       .    I     I        I    I    I      I      I     I      I       I            I

      B-02           I   I    I       I          I   M         I    I    I      I     I       I    I  I   I    I             I     I       I      I M          IM    I

      B-026   M11                  I                   M            M           MI111I                                I      I M                   114        I    I    A

      I-028              I   I    I    I I          I    I    II I              I    I    I                   I           I    I  I     I     I      I      I              I

      B-035          1111  I                   II   I           I         I         I         11I            I        I I    I  I   I      I    I       I      IM

      B-037          li      ii  I             II   I           I       I             I      1                        I I    I  I   I      I    I       I                  I M

      B-028    1141414 IM                     I             I    I   I 1                 1      1      I   I    I       I      I      I1                 I  I

      B-041       M      I I       I I         I          I      I M  I              I I  I  A     I M    I M         I      I     I       I      I      I     I     I     A

      I-097           1111               I    I           I       I    I    II I    IM                         I                            I  I               I    I M

      B-099A        I    I    I                I    I           I   I    I      I     I     I    I   I    I    I      I      I     I       I      I      I

      B-0998    MI       1               I    II          I    I   I   I        I    I       111             1        I      I    I        I       I m         I    I
                                                     Temrp =temperature                 Salt  = slinity           Tra~ns = transparency          Sed= sediment (routine)
    M = monthly, 0 = quarterly, A  annually        00    = dissolved oxygen            Condt = conductivity      AMk  = alkalinity              Sed Org s  ediment organics
                                                     TSS  = total suspended solids      Hard = hardness           TP   = total phosphorus       Metals  heavy metals
    *Base-Neutral and Acid Extractable, and        Phen = phenots                      Turb = turbidity          TOC = total organic carbon    Fecal Coli = fecal cotiform
       Volatile organics                            Pest  = pesticides and PC~s    o ther = other organics    NH3 NH 4=ammonia                  Total Coli = total coliform
                                                     Flow  = flow or stage meas.        CL . = chlorides      NO2 N03 = nitrate-nitrite         SOD5 = 5-day biochemical
                                                     TKN  = totaL Kjeldhat nitrogen    'pH   = pH                                                       oxygen demand

                                                                                          B-23

                                                            Sample Stations: Greenville

      Station  ITemp I DO I pH ISaltlCondtl TSS ITurbjCotorITransIAlklIHardj BOD5 1 NH3 I NO2  JTKN I TP JTOC I CL IPhen IMetalslPest I Other I Total IFecatiFtow I Sed I Sed I
       No.                                           I I I I I I I II           INH4IOI              I         I0            I P~l~g   )Cl              I~        IOrg~I
       No.03        I    I    I    I     I     I    I    I     I    I    I      I     I     I    I   I    I    I      I      I    I       I       I I  I    I              I

      -1011                             I    I3I        I    I I I             I    I       11111                    I      I    I       I       I      I M

      8-113    1                   I I         1M4 I                          11 I      I     I II I M                                            11 M  M                  I

      -14           M    M    I iii                                    I    I  I        I I           I    I M                      I I    I  I   I      I    I    I A

      8-149    1141414    I                 I 1 4        I    I        I      1       1           1     I   I    I       I      I     I              I      I              I

      B-162A    IiM                          I I M I   IM    I  I    II I   M         I          1 I  1               I      I    I       I       I      I    I    I    I

      B-163A I       11            I           I  I         I    III    I M                  I1111                    I      I    I       I       I      I    I    I    I

      8-164    1     1I4M I    I1                        I    I   I    IMM           1           14      I   I       I      I    I       I N         I M      I           I

      B-186    1 M  I  I M                       I       II              I   I   I M       I    I            1        I      I    I       I       I      I    I    I    I

      B-191      n  I    I    I    I M         I    I    I     I    I    I      I     I I        I    I I  I M  I  I                      I I            I  I     I        I

      8-219    11414111              I         1141         I    I   I 1              1             1  I            I    I      I                 1       I  I  IM

      B-221    I     li      ii  I             II        I         I       I        I        1111 I                      I    I  I     I     I      I      I              I

      B-231          li      ii                     I I          I III                       I   II                   I      I         I      I  I m           I    1

      -2135     HI  I         I          I M     I       I     I    IM  I       I I         I    I ,I     I    I      I      1     I      I       I      I     I     I     I

      B-241    1M  I M1            I           I   I    I    I I           I        I       I   I   III  I                I    I     I       I    I         I   M  I
                                                     Temp ~=temperature                 Salt = salinity           Trans = transparency           Sed sediment (routine)
    N = monthly, 0  quarterly, A  annually         DO     dissolved oxygen             Condt = conductivity      ALk  = alkalinity             Sed Org  sediment organics
                                                     TSS  total suspended solids        Hard = hardness           TP   = total phosphorus        Metals  heavy metals
    *Base-Neutrat and Acid Extractable, and        Phen   phenots                      Turb = turbidity          TOC = total organic carbon    Fecal Coll = fecal coliform
       Volatile organics                            Pest   pesticides and P1           Other 1  other organics    NH3 IH4 =   ammonia           Total Coli    total oliform
                                                     Flow  flow or stage meas.          Ct   = chlorides      N    02 N03  = nitrate-nitrite     BCD 5  =5-day biochem~ical
                                                     TKN3    total Kjeldhat nitrogen    pH   = pH                                                        oxygen demand

                                                                                         B-24

                                                             Saniple Stations: Greenville

      Station  ITelp I  DO I pH jSaLtjCondtj TSS ITurbIColorITransIAlklIHardI BOO5  NH3   NO2 ITKN I IP ITOC I CL I Phen IMetalslPest IOther I Total I FecalIFLow I Sed I Sed I
       No.                                        I I     I I            I            I I     I I I       I IIH4INO3I  I   I   I  I JPCBsIOrg*ColiIColi      I   I IOrg~

      B-242      M   I        I I        I I     I     I    I    M  I      I      I         I   I M     I    I  m     I     I             I I            I     I I        I

      B-259      M   m             M                M                                   MIMII            M                                           M

      B-263      M   M      M                   MI        I    I            M           M          mI     I I         I                              M

      8-277      m I         IIH           M N  N                           m                      MI                                                  m

      9-278      M I M I iiiI                  II mI    II I                    I    I           1I    I    I                I    I       I       I      IM  I

      5-301    1141141141                  I MI    1        I    I   I IM                    I    IMI    I      I I      I      I     I       I I        I                 I

      U-302      M  I MliI I             I m        I    I I    II I                       I    I                    I      I    I       I       I M    I    I    I A

      B-315    1 M  I   111                 I II    I    I         II      I        I        (     I M        I           I    I  I    I      I      I     I               I

      8-317    1 M1141141    I    I    1141                                                   I      I     I IIII  K  MI    I M  I    I   I       1141         I    II

      8-321    1     I   I  M  M  I         I    I     I M          I I  I   I    ' I  I MI MI       I    I    I      I I      a I    I       I          I     I I         I

     SE-001   I        4   I4                       M                                 I M  I  I I1I1M  I   I                                             II  I A  I14  II I  I   I    IM I  11I1A  I    I

     IE-007           l                  I    I      I      I    I              I            1111 I    I    I               I      I      I    I       I                  I

     BE-009      MIMIMI            I     I      1         I    I   I    1             IM         114 1    I    I         I      I      I      I        1       I

     BE-0,15    MI   l                   I    II          I        I        I       I        1111I                 I    I      I      I      I      I      I M

     SE-018           lI     ii  I             II         I    I I I            I I          11         1          I    I    I  I      I      I      I      I              I
                                                     Temrp =temrperature                Salt = salinity           Trans = transparency          Sed sediment (routine)
    M = monthly, Q = quarterly, A  annually        DO   = dissolved oxygen             Condt = conductivity      Atk(  = alkalinity            Sed Org  sediment organics
                                                     TSS  = total suspended solids      Hard = hardness           TP   = total phosphorus    Metals  heavy metals
    *Base-Neutrat and Acid Extractable, and        Phen m phenols                      Turb = turbidity          TOC = total organic carbon    Fecal Coli = fecal coliform
      Volatile Organics                            Pest =  pesticides and PCes        Other = other organics    NH3 NHq  ammonlia             Total Cotj = total coliform
                                                     Flow = flow or stage meas.         CL   = chlorides      N    O2 N03   nitrate-nitrite     BOD5 = 5-day biochemical
                                                     TKN  = total Kjeldhat nitrogen    pH   = pH                                                        oxygen demand

                                                                                          B-25

                                                              Sample Stations: Greenville

      Station  ITemp i  DO I pH ISaltICondtI TSS ITurbICoLorITransIAlktlHardj BOD5 1 NH3  I NO2 ITKN I TP ITOC I CtI Phen IMetalslPest  IOther I Total I FecalFlow I Sed I Sed I
       No.  N             iN i            I     II         I     I      I            H    I         lI         i            I                   CPCBsg IOrg*I I Coli  IColi I I Or

     BE-020               I    I    I     I     I    I     I     I    I    I   M              I      I       I    I      I      I     I       I       I      I

     IE-024           1111    I                 II         I       I    I                I     I               1         I      I     I       I       I      I    I      I

     BE-035      MIMIM                    I     IMI        I     I    I    I      I     I            MI    I   I         I      I     I       I       IN                 I

     BE-039          i      i            I    II          I      11        ,         I            1                     I I  I  I     I      I      I          I              I

     BE-040      IN     M I   I              I   f      I     I    I    I        I      I          IMI    I   I          I      I     I       I       IN

     BL-001          I 111                   I  II            I     I   I I       I     I      1  I               I M          I     I  IM           I M    I    I      I    I

     BL-005      M    IM            I I         INI   I          I    I    I      I       MI    INI    I   I             I      I     I       I       I            I

     BP-0lI             I        I       I     II         I     I I I            I     I      1                I    I    I        I       I      I      IM                    I

      S-004     I II MI             II           IM           I       I           I      I         IMI       I   I       I      I     I       I       IN    I

      S-00s    I       i      ii  I             I5I        I      II         I        I        1 1 1 1  I                   I    I  I     I      I      I      I              I

      S-007       MIMIMI                  I I   I          I     I       I I      I     1t41       IMI    I   I  A              I     I M             I      I    I A A

      S-01o    I       I      I I         I     I0I        I      II         I        I        1 1 1 1  I                   I    I  I     I      I      I      I              I

      S-013       M  I M     I   I           I  INI        I     I    lIM         I M        I     IM  M I  I   I        I      I     I I             I I       I     I        I

      s-a     MM       M m       M   m      M   M                IM      A   M       M    M    M      M    M                 0     A      A              M      Mn I    A A

      S-021    IM I M       MI                          I II I                    I    I I    I   I   IN               I A      I I           I I     IN    I  I          I  AA
                                                       Temp  =temperature                  Salt  = salinity           Trans = transparency           Sed= sediment (routine)
    M = monthly, 0   quarterly, A  annually          DO   = dissolved oxygen          Condt = conductivity          AMk  = alkalinity              Sed Org  sediment organics
                                                       TSS  = total suspended solids       Hard = hardness            TP   = total phosphorus        metals  heavy metals .
    *Base-Neutral and Acid Extractable, and          Phen = phenols                      Turb = turbidity           TOC = total organic carbon     Fecal CoUl = fecal coliform
       olatile organics                              Pest  I pesticides and PCBs         Other                           I other organics    NH3  NH  =ammonia  Total Coll = total oliformI
                                                       Flow  = flow or stage meas.         Ct   = chlorides      N     02 N03   = nitrate-nitrite    BOD5 M 5-day biochemical
                                                      TKN =total KjeIdhaI  nitrogen    pH   = pH                                                            oxygen demand

                                                                                            B-26

                                                              Sample Stations: GreenviLle

      Station  ITemp  IDO I pH lSaltlCondtl TSS lTurbICoLorITranslAlkllHardl BOO5 1 NH3 1 NO2 ITKN I TP ITOC ICL I Phen IMetalsiPest IOther I Total I FecaLiFlow ISed I Sed I
       No.               I                 I     II I              III              INHI    I         1 1 NOI                       IPCBs I Org*  I CoLi  I CoLi        I I Or9*1

      S-06 7         I    I     I I        I     I I   I           I I  I  I     I     I m                 I    I M  I    I     I      I       I      I      I      I               I

      S-073           li      ii  I              IM         I        II I           I           I 1 1         1             A I           I I       I     I         I    M  M

      S-084       MIMIMI             I           I 1            I    I    I       1            1      111    I    I          I      I     I       I       1             I
                            liii� I                   Ii       I  I     I       I      I1                1        1 I  I    I               I  I  I  I      I      I

      S-083       MIM    IMI                     I     I          I    IMM    I             MMIQI                    I             I        I             1    I       IM

      S-088       Hl        Iii                  M        M        M i                            I    I A M                              I       I       I M           I a

      S-091       MIMIMI             I                       i     I    I    IM   I       11                    I    I       I      I     I       I       IN    I

      S-096          I                     I     I          I              I        I     I        I    I I     I    I              I     I       I       I       I M  MI
      5-063     IMIMIMI              I     I     114        I      I      I IN    I       11           M      I      I       I      I     I       I        IN    I

      S-0 9       7         *           I           i        I     lit I       I                  1                          I I    I  I    I      I     I      I      Im
      S-067    141414                 II    114 In                  MI A         I 114    111         14 I       MI I           I      I      I       I   111             I         II

          5-091l~               I     I          I MI  I            II II      I         I        1 1 1 1 1 I             I    I        I      I             I      I         I

      S-Ofl    1141414 II                  I     11         I      I    I    114          114         111       I    I       I      I     I       I       114           I

           I          liiiI     I                iiM   I            il I    I                     til I  I                    I    I  I     I      I     I      I       I

      -119I                  ii  I              II          I     I          I         I        1 1 1 1  I              I    I        I      I      I      I      I               I

      S-125           I    I    I    I        M  I                         A    M      M     M     M    M I  I I  I I     I I      I *        I       I A            I  I     I A
                                                       Temp = temperature                   Salt   salinity             Trans= transparency             Sed sediment (routine)
    M = monthly, 0 = quarterly, A  annually           DO    = dissolved oxygen             Condt = conductivity        Alk(  = alkalinity               Sed Org  sediment organics
                                                       TSS   = total suspended solids       Hard = hardness             TP    = total phosphorus        Metals  heavy metals
    *Base-Neutrat and Acid Extractable, and           Phen = phenots                       Turb = turbidity            TOC = total organic carbon       Fecal Coti = fecal coliform
       Volati9 e O rganics                            Pest  = pesticides and P4 Other =   other organics Nu3 NH   4 =ammonia                           Total oli = total coliform
                                                       Flow = flow or stage meas.           Ct    =chlorides NO             N03  = nitrate-nitrite BOBSI       5-day biocheI ical
                                                       TKN   = total Kjetdhat nitrogen      pH    = pH                                                          oxygen demand

                                                                                            B-27

                                                               Sample Stations: Greenville

      Station  ITemp I DO I pH ISaltjCondtI TSS ITurbIColorITransIAlklIHardI BOD5  NHH3   N NO2 ITKN  TP 'TOC I CL I Phen IMetalsiPest IOther I Total I FecaLiFtow i Sed I Sed I
       No.       4INH4I NO3                                                                                                      PCBs I Org*    I CoiI  Coli             I Org*l

      S-135      M    mI    M                                       M                 M    M          M                                                  M

      S-138    I     I    I    I      I         I    I     I     I    I    I      I     I     I    I    I    I         I    I       I      I      I      I      I          AM
                6 I    I       I    I      I    1     I     I     I    I    I      I     I     I    I    I    I    I      I      I     I       I       I      I     I     I     I
      S-1        M I M I MI   I              I I14         I     I       I I            I      M           I   I         I  I         I       I I        I      I M

      S-171      MI M            I        I     II         I         I       I        I  m                      I      I    I       I                 I I          I I         I

      S-138   M114141141                    I MI    1         I    I   I IM                 IQM                   I        I      I  I        I     I   M

      S-231 I        1.I NI                     II  I        III       I     I               I    I M               I     I     I       I      I     I      I      I M

      S-251    1 M14114 4I I                          I 1          I I    I       IM                         I I      I  IA    I       I       I        1 I         I     I A

      S-252      M  I M                 I I        I I     I    I         I     IM   I    I     I    I      I  I.      I M          I      I I        I      I I

      S-264   M  I    IM    M I   I             I    I I         I    I    I  A         I M        I I       I I    I           I I  I      I             A I   I               I

      S-267    1                    I     I     14         I     I       I       1      1          11        I   I       I M1          I       I       IN                 I

      S-289           li     ii  I              II         I         I       I        I        1 1 1 1 1                  I    I  I    I      I     I      I      IM
           s-     I W 1111                I     IMI         I     II          I        I       1 1 1 1 1                  I I    I  I       I     I      I       I              I

      I-291          I       1         I   m    I I        I    III MI I                       11 1                   A  IA I          I I               M I        I     I     I

      I-292        1 MIM               I           I       IM       III M      I A       I                     IM  I MI          I  A I           M      M I  I    I      I

      S-296               1               I     II         I     I I I            I     I    I    JI l l              I      I         I I         A  I  I      I          A
                                                      Temrp mtemperature                  Salt  =salinity            Trans = transparency           Sed sediment (routine)
    N = monthly, 0 = quarterly, A  annually    DO   = dissolved oxygen                   Condt  conductivi ty       Atk   = alkalinity�             Sed Org  sediment organics
                                                      TSS   = total suspended solids      Hard   hardness            TP  total phosphorus           Metals 1heavy metals
    *Base-Neutral and Acid Extractable, and          Phen  = phenols                     Turb  turbidity            TOC = total organic carbon      Fecal Cali = fecal cotiform
       Volatile organics                             Pest =  pesticides and PC~s other =         other organics No  3 I  I  = aImonia               Total Cali = total oliform
                                                      Flow =Sfl ow  or stage Ieas.        Cl   = chlorides N02 N03 =           nitrate-nitrite B115 1      5-day biNhemical
                                                      TKN   = total Kjetdhal nitrogen    pH   = pH                                                          oxygen demand

                                                                                           B-28

                                                             Sample Stations: GreenvilLe

      Station  ITemp I DO I pH lSaltICondtl TSS lTurbtColorlTransiALkllHardl BOO5 I NH3  NO2 JTKN I TP ITOC  ICL IPhen iMetaislPest I Other I Total I FeCallFiow I Sed  ISed'
       No.                                                                         NH4          I                               IPCB I  Org*  I CoLi  IColi           I IOrg*1

                          SV-00~~~ ~ ~   ~4 M

      SV-017    M     M    M                      m                                                                              M  M  M                 M
      SV-031      I   M     I        M  I         I            I I  I     I    I     I             I    I    I    I      I      I M           I M            I     I     I     I

      SV-037     M I  liM     i                I      I       I      I            I I       I      1 1 1 1 I    I                     I I  I   I     I      I      I M

      SV-00114              4    I           I 1141        I        II     IM    I      14M    M   1141      I "             I     I      I       I  I       I     I     I MI

      SV-043     MIMINI                   I I   1          I     I   IM    I M             M       lI        I   I       I      101                   I              Al       I

      SV-052   MI    II                         I    I    I      I   I    I       I     I     II    I                 I      I    I        I      I      I      I              I

      SV-07   3MIMINI               I            1         I     I   I    1             1          1141      I   I       I      I     I       i                 I              I
          sv-os~    MI M11.11             I     I MI       I     I   I   I                   I    I    111               I      I      I       I       I     I

      SV-0531    IM I MI      I        I     I  114    I      I     MI AI  IM    IM MM IMII                     I1 1 I              I      IN                14 I              I

      SV-098      M l        i            I     IiM                MIll           I     I      1 1         1 1           I      I     I       I       I      I    I A A

      sv_100   I      l        I                1' I    Il                       I I          1                         I      I     I I        I    I        IM  I           I

      SV-106   1141414    I                  I  1       I     I    I    I        I           1     1              I I    I    I     I      I      I      I      I              I
                     M         I I  I    I      I    I     I     I    I    I      I     I     I    I    I    I    I      I      I     I       I   I          I A         I     I
      SV-104    1141141141  I                I  114    I      I    I    I M I           114        14        I I    I         I    I     I            IN    I  I       I        I

      sv~111    I M            I                II I              III  I     I                 1  I M                  I      I                       I I  I  I    I

                                                     Temp  =te1perat ure                 Salt  =salinity            Trans= transparency            Sed sediment (routine)
    M  monthly, 0 = quarterly, A  annually           Do   = dissolved oxygen             Condt = conductivity       Alk  = alkalinity              Sed Org  sediment organics
                                                     TSS   = total suspended solids      Hard = hardness            TP   = total phosphorus        Metals  heavy metals
    *Base-Neutral and Acid Extractable, and          Phan = phenots                      Turb = turbidity           TOC = total organic carbon    Fecal Coil = fee&[ coliform
       Votatile Organics                             Pest =pesticides and PCBs           Other = other organics     NH NH ammonia                  Total CoIi = total coliform

                                                     Flow mflowu or stage meas.          CL  =  chlorides NO    2  N03- nitrate-nitrite            BOD 5 = 5-day biochemiceal
                                                     TKNl   = total Kjeldhat nitrogen    pH   = pH'                                                        oxygen demand

                                                                                          B-29

                                                                            San~oLe Stations: GreenviLLe

                   I I I I I I I I I I I I I I I I I I                                                                                                                                                            I I I I I I I I I
       Station ITen~o   I DO   I pH ISattlCondtl TSS   ITurblCoLorlTranslALktlHardl BOD5 II NH3                                                               NO2   ITKN   I TP   ITOC I  Cl  I Phen IHetatslPest I Other I Total  I  FecatlFtow   I  Sed I Sed   I
         No.
                   I I I                       I        I I I I I I I I NH4 "�3 I I I I I I IPCSs I Org* I Coti I Coti I I I
                                                                                                                                                                                                                        Org*l
                   I         I I I I I I I I I I I I I I I I I I I I '1 I I I I                                                                                                                                                                                                                                    I
                   I I I I I I I I I I I I I I I I                                                                                                                                          I I I I I                                                   I             I I I I I
       SV-121 I M IM I M.I I I IM I I I MI  AIM    I  M                                                                                                         M I MI MI QI I I o I A I A** I I M I I A I A I
                   I I I I                              I          I I I I I                                          I I I I I                                                    I        I        I            I           I I I I i                                                       I I I
       sv-122 I M IM    I   M I I I IM I I I   MI AI   H                                                                                        I   M           M     I   M I   #1 QI I                                I     Q I A I A**                     I             I   M I I A I A                              I
                   I I I I I I I I I I I I                                                                                                  I                    I        I        I I I I I I I I I I I I
       SV-135 I M IM                       I   M   I         I I I'M I I I I                                                        I   M I M    I                             I   M I I I I I I I I M I I I I
                   I I I I I I I I I I I I I I                                                                                                                            I        I     '1 I I                                I I I I                                             I          I I I
       SV-136 , I M IM I M I I I IM I I I I I M I M    I I M I I I I I I I                                                                                                                                                                                                 I M I I I                                    I
                   I I I I I I I I I I I I I I I I I I I I I I I I I I I
       SV-137 I M IM I M I I I IM I I I I                                                                                           I   M I M I I M   I I I I I I I I M                                                                                                                 I I A                I          I
                   I I I I I I I I I I I I I I I I I I I I I I I I I I I
       SV-139 I M IM I M I I I IM I I I I I   M I M I I M I I I                                                                                                                                                        I I I I I M I I                                                                       I I
                   I I I I I I I I I I I I I I I I I I I I I I I I                                                                                                                                                                                                                            I I I
       sv-140 I M                 IM I M I I I IM I I I                                                                    I I M I M I I M I I                                                            I I I .I I I   M I I                                                                               I I
                   I I I I I I I I I I I I I I I                                                                                                                                   I I I I                                     I          I             I I I I I I
       sv-141 I M                 IM    I   M I I I IM I I I I I   M I M I I   M   I I I I I I I I # I I I I
                   I I I                       I I I I I I I I I I I I I I I I I I I I I I I I
       SV-181 I M I M I M I I I IM I I I I I M                                                                                                 '1 M I I   # I I I I I I I I   # I I I                                                                                                                                   I
                   I I I I I I. I I I I I I I I I                                                                                                                                  I        I I I I I I I I I I I
       SV-200 I   M IM    I   M I I' I IM I I I I A I M I M                                                                                                           I I M I I I I                                          A     I I I '1 M I I                                                            I I
                   I I I I I I I I I I I I I I I I I I I I I I I I I I I
       SV-203 I M I M I M I I I IM I I I I I M I M   I I M  I I I I I I I I M I I I I
                   I         I        I        I I I I                                 I I I I I I I I I                                                                                    I I I I                                       I I I I I I.                                                              I
       SV-206 I   M               IM I MI I I IN I I                                                              I        I I M I M I I #1 I I I I I I I   M I i                                                                                                                                            I          I
                   I I I I                              I I I I I I                                                   I        I            I                    I I I I I I                                                   I I I I                                             I I I                            I
       SV-227          I   M IM I MI I I IN                                                 I I I MI AIM I M M I   MI HI OI I                                                                                          I     O I A I I I   M I #                                                   I A I I
                   I I I I I I I                                                       I I I I I I I I I I I                                                                                                      I            I          I             I I I I I I
       SV-230 I   M               IM I M I                   I I M IN                       I I I M I Am M I M                                                  M I MI M I   O l                          I            I     e I A I I I M I I I I

                                                                   Temp ~- tenperature SaLt = salinity Trans = transparency Sed = sediment (routine)
     M = monthly, Q = quarterly, A = annuaLLy DO = dissolved oxygen Condt = conductivity Ark = aLkaLinity Sed Org = sedimnt organics
                                                                   TSS       = total suspended sotids Hard = hardness TP                                                                       c total phosphorus MetaLs = heaw/laeta[s
     *Base-Neutrat and Acid Extractabte, and                                                 Phen = phenols Turb = turbidity TOC -- totaL organic carbon Fecat Coti = fecat coLiform
         VoLatiLe Organics Pest = pesticides and PCBs Other = other organics Ntl3 #H4 = ammonia Totat Coti= total cotiform
                                                                   FLow = ftow or stage meas. Ct = chlorides
                                                                                                                                                   NO2 NO3 = nitrate-nitrite 80D5 = 5-day biochemicat
    **organics Listed above plus dioxotane TKH = ~otat KjeLdhat nitrogen pfi. = pH oxygen de~ncl
          i somers.

                                                                                                                B-30

                                                             Sample Stations: Greenville

      Station  ITemp I DO I pH  ISaltICondtj TSS ITurbIColorITransIAlrkLHardI BOD5 1 NH3  1 NO ITKN I TP ITOC I C1 IPhen I     ~etalslPest I Other I Total I FecatiFlow I Sed I Sed I
       No.                                                                          N I   N I I                                 I I I  I IPCi I IrINHIIN I  I  CoI   I  I  (r e I
                                                                                        4

      SV-236      M     M    M                   m                                          M  m   M                           M

      SV- 239     M   M      M                   M M                          M            M          M 1I                                               M

      Sv-241      M    I  I    I    I     I     I I  IM       I    I    I     I         I     I    I    I  I    I        I I    I       I                M I  I  I             I

      SV-245   I       I    M I   I    I  I M  I    I                I           I     I I   I   I 1 1    1             I      I     I       I       I      I     I     I     I

      SV-249     MIMI   MI                I             I IM                     I  I1I1          I A4      I MI               I M           I       1         I MI

      SV-282     MIMl        I I          I    I   I       I     I  I   I     I      I       I                           I MI    I  I   I M                  I  I    I         I

      SV-288     MIMIMI    I                      I            IM     I    1141        M           1141      I   I           I     I      I       I  IM   I A            I     I

      SV-301   I       i     i        I         II         I        I        I        I        1 1 1 1  I                   I    I           I I  I     I      I              I

      SV-303     MIMIM    I                  I 1        I     I    I       111          1          1141      I      I        I    I     I1                     I  I  Im

      SV-308   I     I          I            I II          I        I        I        I        1 1 1 1  I                   I    I  I     I      I      I      I              I

      SV-311 41 I                         1      1  I            I   I MM               1          1141                I    I       I I M  A          1            I I         I

      SV-312     M    M                                                                                                            I      I       I       I M      I           I
                  I  I 1I *       I       I    I  I        I    I   I I           II    I     I    1. 111                I      i     I       I       I      I    'I     I     I

      SV-313         I       ii  I              I    I     I     III          I                    I M1    1                    I A           I IM              M

      SV-316         I M       I    I I         I    I I  I M   I     I     I     I    I                I    I    I      I I  I               I I  I     I      I               I

      SV-322'  M1        1                      1     I  IM   M     MIAIM            M    MIMIMIOI    I                                              I   M
                                                      Temp =temperature                   Salt  =salinity            Trans = transparency           Sed sediment (routine)
    M = monthly, Q = quarterly, A  annually          DO    = dissolved oxygen            Condt  conductivity        ARk   = alkalinity             Sed Org  sediment organics
                                                      TSS   = total suspended solids      Hard  hardness             TP   = total phosphorus        Metals  heavy metats
    *Base-Neutrat and Acid Extractable, and          Phen  = phenols                     Turb  turbidity            TOC = total organic carbon     Fecal Coti = fecal cotiform
       Volatile Organics                             Pest =  pesticides and PCBs         Other = other organics     NH 3 NH 4 =ammonia             Total Coli = total coliform
                                                      Flow = flow or stage mneas.         CL =   chlorides       N    02 M03 = nitrate-nitrite      BOD 5  = -day biochemical
                                                      TKN   = total Kleldhal nitrogen     pH    = pH                                                        oxygen demand

                                                                                           B-31

                                                               Sample Stations: Lancaster

      Station  ITeap IDO I pH ISaltICondtI TSS ITurbIColorjTransIAlkLIHardj BOD5 I NH3 I NO2 ITKN I TP ITOC I Cl I Phen IMetalsiPest I other  I Total I FecaljFlow  ISed ISed I
       No.                                                                          INH4I NO3         I         I 1    1            JPCBs I Org*  I Coli  I Coli        I     IOr9l

       B-042      M    M  I      M     I         I    I     IM     I    I    I M                I A     I M     I M             I M       I       I       I M        I        IM  A

       8-044      M I         i            I     II               I I      IM  M  M  MI i i !                                I      I     I       I        I            I MI A

       0-046      MIM        M I    M         mI M                   M I INIAIM      ININIMINIOI I                           I     IAI            I        IA     I    IA  I A

       B-048      M Ml        I    I       I     IM          I       IMI            I     I       1 1 1 1 1                  I      I     I       I MI              .1M  M  A

       5-051     INI IN           I           I   NM                 M IIA IM          MINIMIMIOI                    I       101          I       I        IN    INIAI     A

       B-056      M IM                    I     II    I        I      II       M   I             11M  I                    I        I           I   I       I      I     I        I

       -057       MM I l      Ii           I     I I         IM       I IM  I I M             I A     I       i                             I I  I MI             I     I     I

       8-059      M  IM               I          II          I     I   I       I I             I                             I I          I       I I  I  I  I     I M

       6-062    ININ NI              II          IM      I      I    IN     IN                 MI NIOI               I       101          I       I        IM       mKMAI           I

       B-064      M   M      M                     M~              I            M            M           M                                                   M   I I1I

       0-067A\    M   M      M                     Mn        1     I            M            M             mI                             I                   M

       B -067B    M M M      M                     mMI       I     I            M            M           M� M                                                M

       -074       M  IM    I    I    I I         I    I      I     I    I    I   M         I     I    I    I    I    I       I      I     I       I        I      I     I           I

       B-075          l         I                II    I            III  I     I    I                 I    III I          I    I        I      I      I      I       I               I

       B-086     IKI IN           I           I  INI         I     I    I    I  I          IMI        IMI       I                   I     I       I             I          A I  I
                                                       Temp~ =temrperature                  Salt  = salinity            Trans = transparency            Sed= sediment (routine)
    M  monthly, Q   quarterly, A  annually            DO    m dissolved oxygen              Condt = conductivity       Alk   = alkalinity               Sed Org  sediment organics
                                                       TSS   = total suspended solids       Hard = hardness             TP    = total phosphorus        Metals  heavy metals
    *Base-Neutral and Acid Extractable,  and          Phen  = phenots                       Turb  = turbidity          TOC = total organic carbon       Fecal Coti = fecal coliform
       Volatile organics                              Pest  = pesticides and PCes          Other = other organics      NH3 NH 4 = ammonia               Total CoH =. total cotiform
                                                       Flow =flow or stage meas. CI                 =chlorides          N02 M03  = nitrate-nitrite      B(DI  = 5-day biochemIical
                                                       TKN   = total Kjeldhal nitrogen      pH                                            =                       Hoxygen demand

                                                                                            B-32

                                                              Sanmle Stations: Lancaster

      Station  ITenm I DO I pH ISaltICondtl TSS lTurbIColorITransjlnkLlHardI 80O I NH3 I NO  ITKN I TP ITOC I C I Phen IMetalslPest  IOther I Total I FecallFlow ISed  ISed I
       No.                                         I N I   N I    I    I    I    I   IPC NH I  IrI                 I                          CI   I  Org*I  Col    Coli

       B-088     MM      M I                     H             M     M                   M m         M                  1      I     I                 M

       0-095   1    M I M  I   I               I    I     I     I    I    I      I       I   I    I    I    I    I      I      I    I       I       I      I M

       B-100     M    M    M                     M                       A       M        M          N                    A                            m AII

       B-119        M    M m             M  m       M        M    M    A  M         M    M  M    M   0   0   0P)          M      0      0IP            M            A    A

       B-128     M     M    M                                                M     M      m          M           I      I      I                       M

       B-133     M    M    M                                       M                 M    M          m  I I I           I                              M

       8-159     M   M         I i                I    I  I       I I   l        I             I            I   I       I      I     I       I       I     I    I    I    I

       B-199     M IM                    I    I  I        I    III               I    I       11 I    I                 I      I     I       I      I MI    I    I

       8-211    141141141          I    I      1141       I    I   I    IM   I    1               1141      I   I       I      I     I       I            1            I

       B-243     M     M    M                    M                                                                             M  m  M                 M

       B-286     M   I M       IM   I       I     I       I I      I     I    I              I M       I    I    I  I      I         I I     I      I      I           l     I

       8-2871001141141                I    I 114          I    I       I        I      1          1141      I   I       I      I     I       I      1            IAI M

       B-323     M   I M       IM                         I M         I     I       I             t    I    I I         I I   I              I I    I      I           *     I
                      *1  lilt                    I    I  I        I lit               I    I    111I I    I                      I       I     I      I      I      I�

       -325      1  M I    I   I    I I        I     I  I       I    I    I        M   I     I       M    I  I   I      I      I     I       I       I      I     I          I

       8-32631141141  4            I    I      1141       I    I   I    IM  I               1     1141    I   I         I      I     I       I       1       M
                                                     Temrp = temperature                Salt  =salinity            Trans = transparency           Sed= sediment (routine)
    M monmthly, 0   quarterly, A a nnually      DO        = dissolved oxygen            Condt  conductivity        AM   = alkalinity              Sed Org  sediment organics
                                                     TSS   = total suspended solids     Hard  hardness             TP   = total phosphorus        Metals h  eavy metals .
    *Base-Neutrat and Acid Extractable, and         Phen = phenots                      Turb  turbidity            TOC = total organic carbon    Fecal Coti = fecal cotiform
       Volatile Organics                            Pest = pesticides and PCBsI Other = other organics             NH3   NH 4 =ammonia            Total Coli I      total  coIifor
                                                      2low =  flow or stage mes. CI    1   Ihlorides NI2  N13               = nitrat e -nitrite    ROD41= 5-day biochemical
                                                     TKN   = total KjeIdhaI nitrogen    pH    = pH                                                        oxygen demand

                                                                                          B-33

                                                             Sample Stations: Lancaster

      Station  |Temp I OO I pH ISaltCondtj  TSS ITurbIColorITransIAlklIHardj BOD5  :H3 H    NO2 ITKN I TP |TOC I Cl I Phen IMetalslPest I Other I Total I FecaliFlow  ISed ISed I
       No.                                           I I   I    I    I   I    I  I   I   I  IH4NO3I I   I   I   I      I       PCBs I Org* I Coli  I Coli           I I Org*

           I-330  M  I                                                     I   I  I  I  I                  I I  I  I  I  I   I  I     I    I       I    MI       I          I

      BF-007    MI   11                        II         I         I       I        I        liiiI                 I    I       I      I      I      I     I               I

      OF-008     N    N    m                     mIM      I     I            M            M          M

      cw_002     M    M    M                     M                 M    A     M     M     M    M    M    0                 0Ia      A                  m     M
      CWB-330   I M  I M    M      I           I M  I     I    I   I    I M              M 1     I       I    I    I     I      I       I     I     I       M   I

      -008   I M  I M    M               I    IM  I       I    I M        I M   I    I M  I    I M I             I      I  .        I                     I I M

      BF-00    I M  I M  I M I    I    I                                                             IM  I  I    I   I  IM   I    I 1  I I   I  I  I    I  I  I M   I I  I   I

        CWolI        1111                I     I mI MI I MI                  I                                                      I M  I    I       . I  I  I I  I  I    I    I    I

      CW-013    I M  I M    I M I   I    I    I M  I               M I A I M   I M  I M    I M   I M      I   I         i     I A  I        I       I n   I     I    I    I

          I          W      0I M         I    I   I       I    I   I    I MI    I    I    I   I    I   I               I A    I I   I       I       I M         I    IAI
      CW-016F 11141 M    M                     114                 M IN A       M I      NM IM IQ M0                        QiA             I   A N        14

          CW01 M         II         IMI                   I                      I M        I   I   I I1.                           I       I       I M  M            I*

      CW-006   1 M  I M    M I                 I          I     I   I    I I             M I  m1  I              I  I                I      I A            I     I    I    I

      CW-003   I M  I M    M I                 I M                 M I A I M        M    M    M  M I   I    III    I       a  I I    I      I       I      I M  I    I    I
                             I  (II~     ~         I      I     I    I      I II   I    I         1       1         I      I      I      I      I       I     I    I ' I
      CW-00927   M       I  I IM  I M I        I    I                     I      I             I  I I  IA  I I                              I          M   I    I    I    I

                                                    Temrp = temperature                Salt  = salinity           Trans = transparency           Sed= sediment (routine)
    M = monthly, 0   quarterly, A  annually         DO   = dissolved oxygen             Condt = conductivity      Alk(  = alkalinity             Sed Org  sediment organics
                        TSS   = total suspended solids                                 Hard = hardness            TP   = total phosphorus        etals   heavy metals
      CW-011  I1M4I1M4I1M1         I    I    I1M4I        I    I   I    I M   I    I14 M  I       M         I   I       I     I     I       I       I M   I    I    I    I

    *Base-Neutrtl and Acid Extractable, and         Phen = phenols                      Tmrb = turbidity          TOC = total organic carbon     Fecal Col = fecal  altiform
          CW03 I M 11MI    I I    I    I MI               I    IMI  AI   M I MI MI MI MIQI   I                         I  QI AI             I       I M I    I AI    I

       Volatile organics                            Pest  = pesticides and PCBs         Other            = other organics  NU 3   NH       4      ammonia  Total CoLi  = total coliform
          CW06 I M    I M I MI IM  I MI MI MI    IMI  AI   M I MI M    MIIMIMI   I* I                                      Q  I AI  A I             I M I MI AIAI

               I     I   I    I    I     I     I    I     I     I    I    I      I     I     I    I    I    I   I      I      I     I       I       I      I     1     1.    1

                                                    Flow = flow or stage meas.         cL   = chlorides           NO2 N03  = nitrate-nitrite ROD 5 =5-day biochemnical
          CW-16FIM     I M I MI I    I    I MI             I    I IM|AI   M I MI M 11MI11IQ 1                           I  QI        I       I       I M I    I AI    I

      CW-017  I1M4I1MI1M1I1           I    I   M14    I      I I        I   14 I14 M I    IM             I    IM|      I      I      IN    I  I              I              I

                                                    TKN  total Kjedha  nitrogen        pH    = pH                                                        oxygen demand               I        I

                          CU-019  I1M1II   I    I    I I  I    I   IAIM    I               1 M1-3          I   I       I  A         I       I              I    IAI          I
               I        I i     I       I    I   I       II    I    II          I     I     I   ((       I   I        I      I     I       I       I      I    1    1.    1
          CW03 I   M I M I   M I   I     I     I M  I     I     I   M I   A I   M I   M I   M I   I   M I   a     I    I   Q  I     I       I       I   M  I   M I   A I   A I

      CW-027  I1M4I1M4I1M1         I    I    IM  II          I    I lAINM   I    I14 M            114M1     I   I       I  AlI    I          I      I M   I    I AI          I
                                                    Temp  = temperature                Salt  - salinity           Trans =transparency            Sed = sediment (routine)
    M4 = monthly, Q0  quarterly, A = annually       DO    = dissolved oxygen            Condt = conductivity      Alk   =alkalinity              Sed Org =sediment organics
                                                    TSS   = total suspended solids     Hard  = hardness           TP   =total phosphorus         Metals = heavy metals
    *Base-Neutral and Acid Extractable, and         Phen  = phenols                     Turb  = turbidity         TOC = total organic carbon     Fecal Coli =fecal coliform
       Volatile Organics                            Pest  = pesticides and PCBs         other = other organics     NH3 NH  = armionia            Total Coli = total coliform
                                                    Flow  = flow or stage mreas.       Cl    = chlorides          NO2 NO3  nitrate-nitrite       BOO5   5-day biochemical
                                                    TKN   = total Kjeldhal nitrogen    pH    =pH                                                         oxygen demand

                                                                                        B-34

                                                                                                   SampLe Stations: Lancaster

                       I            I I I                            I            I I I I                                           I I I I I                                                       I I I I I I I I I I I I I                                                                                                                                                         I
       station IT~.P I DO I pH ISattlCondtl TSS ITurblCotorlTranslAtkLIHardI soo5 II .H3 [ .02 IT[. I TP ITOC I CL [Phen IMetaLslPest ( Other I Total I FecatlFt�w I Sod J Sed I
         .o. I I I I I I I I I I I I HH4                                                                                                                                                       "03 I I I I I I IPcas I ors* I coti   I coLi I I                                                                                                                              I Org*l
                       I I I I I I I                                                                      I            I I I                              I               I            I I I I                                       I          I I I I                                                      I                 I              I            I             I            I
                       I            I          I I I                              I            I I I I I I I I                                                                                      I          I I I I I                                                       I I I                                           I I I I I
         o4-029 I M I M I M  I                                           I            I            I M    I I I M  I A I  M                                                   I  M I M I M I M I O  I I I O I I                                                                                                  I                 I  M           I  M    I                  I            f
                       I            I          I          I          I            I            I          I            I            I          I I I I I I I I I I I I I I I I                                                                                                                                                                                           I            I
         CU-036            I    M       IM         I    M    I I I                                 IM         I            I            I           I          I    M         I            I    M       I          I    M    I           I          I              I               I            I                I                 I    M          I            I            I            I
                       I            I          I          I          I            I            I          I            I            I I I                                 I            I I I I                                       I I I' I I I I I I                                                                                                                  I I
         cu-041 I M I M I M I I I I M I  M I I H  I A I M    I  M I M I H I 14 I O I I                                                                                                                                                                             I   O   I I I I M I M I A I I
                       I            I          I          I          I            I            I          I            I            I          I          I               I            I            I I I                            I I I I I I I                                                                                            I I I I
         C14-047 I M IM I H                                   I          I            I            IM I I I I I M                                                             I I M I                              I    H     I I I                                I I I I I    M                                                                  I I I I
                       I            I          I          I          I            I            I          I            I            I          I          I               I            I            I          I          I          I          I I I I I                                                                      I              I I I                                   I
         cu-057 I M   IM I HI                                            I I IM   I I I HI  AI 14                                                                             I  14 I M IH I 141  01 I I    O I I I I  M I I A I I
                       I            I          I          I          I            I            I          I            I            I          I          '1 I                         I            I          I          I          I          I              I               I            I I I I I I I
         CW-064    I 14 IM I 141 I I IM I I I I I 14 I I   14 I I MI                                                                                                                                                                     I I I I I I I M I I I I
                       I I I                              I          I'           I            I          I            I            I          I          I               I            I            I I I                            I          I              I               I            I                I '1                              I I I I
         C14-080 I  14 114   I  141 I I IM I I I I I 14 I I  14 I I 141 I I '1 I I I I M    I I I I
                       I I I I I                                                  I            I I I                                I          I          I               I            I            I I I                            I          I              I               I            I                I                 I               I            I            I            I
         CU-083 I  M    IM I 141 I I M    IM    I I I I I M I I  M    I I 141 I                                                                                                                                                                     I               I I I I I M                                                                    I            I            I. I
                       I I I I I I I I I                                                                                            I          I          I               I            I            I          I          I          I          I              I               I            I                 I                J               I            I            I            I
         CW-088   I  14   IM   I  141 I I IM I I I I I M I I  14 I I MI I I I I I I I M I I I I
                       I I I I I I I I I I                                                                                                     I          I               I            I            I          I          I          I          I              I               I            I                 I                I               I            I            I            I
         04-096   I  14    IM I 14  I I I                                                          114    I I I I I 14                                                        I            I M I I 14 I I I I I A   I    A                                                                                        I                I  M            I            I I I
                       I I I I I I I I I I I                                                                                                              I               I            I I I I I                                                I              I               I            I                I                 I               I            I            I I
         CU-105 I M 114    I  141 I                                                   I 114 I I I I 1,14 I I   14 I I  141 I I I I I I                                                                                                                                                                                             I   14          I            I            I. I
                       I I I                              I          I I I I I I I I                                                                                      I I I I I                                                  I          I              I               I            I                 I                I               I            I .I                      I
         CU-131 I M   I H I M  I I I                                                               114 I I I I I 14 I I 14 I I 14 I I I I I I I I  M I I I I
                       I I I I I I I I I I I I                                                                                                                            I I I I I I                                                           I               I              I            I                 I                I               I            I            I            I
         cu-134   I  14 114 I H I I I 114 I I I I I M I I  14 I I 14 I I I I                                                                                                                                                                                                       I I I I M I I I I
                       I I I I I I I I I                                                                                            I          I          I               I I I I I                                                  I          I               I              I I I                                           I               I            I            I             I
         CU-151 I  14   IM   I  14 I I I                                                           114 I I I I I 14 I I 14   I I 14 I I I I I I I I 14 I I '1 I
                       I            I          I          I          I            I            I          I            I            I          I           I              I            I' I                    I          I          I          I               I I I                                         I                I I J                                     I             I
         Ct,/-152          I    H       I  M       I    H    I           I            I 114                   I            I I H    I A I    14 I 14                                       I    14       I    14    I    M    I    O    I I I                               O      I A I                          I                 I    M         I            I A I                      I
                                                                                      Temp = temperature Salt = salinity Trans = transparency Sed = sediment (routine)
    M = monthly, Q = quarterly, A = annually DO = dissolved oxygen Condt = conductivity Alk = alkalinity Sed Org = sediment organics'
                                                                                      TSS = total suspended solids Hard = hardness TP = total phosphorus Metals = heavy metals
    *Base-Neutral and Acid Extractab[e~ and Phen = phenols Turb = turbidity TOC -- total organic carbon Feca[ Coti= feca[ cotiform
         VoLati.te Organics Pest = pesticides and Pegs Other = other organics HH3  NH4 = ammonia Total Co[i= total cotiform
                                                                                      FLow = ftou or stage togas. CI = chlorides
                                                                                                                                                                                               NO2 NO3 = nitrate-nitrite 8005 = 5-day biochmicaL
                                                                                      TKtl -= total Kjetdhat nitrogen pH = pH oxygen demand

                                                                                                                                                  B-35

                                                                  Samrple Stations: Lancaster

      Station  ITemp   DO pH   ISalttCondtI TSS ITurblColorITransIALkltHardj   BOD5 1 NH3 I NO2 ITKN I TP ITOC  ICl I Phen IMetalsiPest I Other I Total I FecalIFlow  ISed  ISed I
       No.                                                                              NH4INO3I         I I       I    I       I      JPCBsIOrg*  ICoLi  ICoLi                 I  Io Irg

       W-153                                                  I      I    I         I M          I       I I                                                          I      I     I m

       CW-154   MI   l      iI                                I      III               I     I                   1           I  I    I                         I I  I    I                I

       CW-155IMIMIM                   I           IMI         I     I    I  AIM                M           MI      I                   I      I       I        IM   I        I  A

       CW-17 I I              l l          I     I I         I     I ll               I     I      1 1 1 1 1                   I       I     I        I       I      I      I     I

       CW-174 IMIM                   II           IMI         I     I    I    IM                M          MI      I    I       I      I      I       I        I             I

       CW-175     MIH1 1              I           I I         I      I          I          I         1 1 1 1  I              I    I       I       I      I       I      I                I

       CW-1765 M              I MI                                  I       AIM M                        I        I       I              I I  I  Al  I M       I             I            I

       CW-185  1      Il                                                                  I M                  I I M  I                                               I

       CW-192   IMIMIM                I           IMI         I      I    I    IM m                        MI       I    I      I       I     I        I       Im

       CW-197          l         I                II    I      mI             I        I     I       1 1 1 1 1                            A            I       I         I    M      A

       CW-198      I I      MI        II          IMI         I           IIMIM                          I                 I            I  A           IM      I      I M       A         I

       CW-200   MI   l      I                     I I         I         I         I        I         1 1 1            I     I    I        I       I      I       I                I M

       CW-01    M   I M  IM I               I I   I                       I m  I MI            A I M  I IMI  IMI I              I       I     I        I       IN M                I
                CWI 2     1 2         I M                     I II            I     III         I    I II  Im                   I       I     I        I       I       I     I      I
       CW-2185MinI           MI      I      I        IN       I      I    I    INM   I       INI            I!      I    I      I       I     I        I       IN    I

                                                         Temrp = temrperature                  Salt  = salinity             Trans = transparency             Sed sediment (routine)
    M = monthly, Q   quarterly, A  annually             DO    = dissolved oxygen              Candt = conductivity         Alk   = alkalinity               Sed Org  sediment organics
                                                         TSS   = total suspended solids        Hard  = hardness             TP    = total phosphorus         Metals  heavy metals
    *Base-Neutral and Acid Extractable,  and            Phen  = phenots                       Turb  = turbidity            TOC = total organic carbon       Fecal Coti = fecal coliform
       Volatile Organics                               Pest  = pesticides and PCBs        o    ther = other organics       NH3 NH4 = ammonia                Total Cotj   = total coliform
                                                         Flow  = flow or stage meas.           Ct   = chlorides             N02 N03  = nitrate-nitrite       BOO 5 =5-daey biochemical
                                                         TKN   = total Kjetdhat nitrogen       pH    = pH                                                             oxygen demand

                                                                                                 B-36

                                                              Sanple Stations: Lancaster

      Station  ITemp IDO I pH ISaLtICondti TSS ITurbICoLorITransIALklIHardI BOD5 1 NH3 1 NO2  ITKN I TP ITOC  ICL IPhen IMetalsiPest  IOther  ITotal IFecaliFlow  ISed  ISed I
       No.     N                                                      4 3 I  I    I I    4                                      IpcsI         IColi IColiI         I    IOr"9*

       CW-213    MI#         MI IMI    I    I   I    I                            I I         I         I    I    I      I      I     I       I       I      I    I      I     I

       CW-214111                                   I IM       I M           I         I        1 1 1 1 1 I M                I       I      I      I      I      I              I

       CW-22        1                IM  I       11        I    I   I    IN    I M11                         I    I      I       I     I      I       I      I    I      I    I

       CW�1-223   IM                I           IMI        I    III               I     I     I     I I      I    I      I       I     I      I       I      I     I     I    I

       CW-224          4           I      IM    I14 I    I    I    Im  I                     1 I  M             I     I      I      I     I       I         I M  I    I        I

       CW-225      I M              I           II    I    I        II       I        I            1M          1 I     I    I       I      I      I      I      I MI A

       CW-226         1             IM  I     I M  I    I    I    IM              I M I A   I                   I         I      I     I       I      1I4 I         M  I I A

       CW-22 I        711                 I     II         I    I I I             I     I      1 1 1          1       I      I      I      I          I  I         I     I    I

       PD-004 I31    IM                   I    1                 I             I       I I 1    I   I        III I        I      I     I      I       I I       I     I        I

       PD-005I        i      i M                II    I              I      I  I                   1 I                           I M  I  I  I  I     I      I      I

       PD-006  I M2 1  IMI 1                                  I                      I I14           I      I     I IN    AI M  I14  I    I  I  I  I  I  IN    I     AI        I

       PD-009    M1 IM        I M         I     I  I       I        I         m I IM I    I                              I      I     I       I      I      I     I     I    I

       PD-066   I         I I    I  I           I A        I     I      I   I              M I     I I  I              I     I     A    I      I I        I      I   A   I     I

       PD-067   MI   l     i                    II         I        I        I        I           I          I I       I  I    I    I       I     I      I      I              I

       PD-068    M        IM   I M           I     I    I     I       I    I               M I  I    I     I    I     I      I      I    I     I       I      I
                                                      Temp, = temperature                 Salt  = salinity           Trans = transparency           Sed  sediment (routine)
    M = monthly, 0  quarterly, A  annually           DO   = dissolved oxygen             Condt = conductivity       Alk   = alkalinity              Sed Org  sediment organics
                                                      TSS   = total suspended solids      Hard  = hardness           TP    = total phosphorus    Metals  heavy metals
    *Base-Neutral and A cid Extractable, and         Phen = phenols                      Turb  = turbidity          TOC = total organic carbon    Fecal Coti = fecal cotiform
       volatile organics                             Pest =  pesticides and PCBs         Other =  other organics NH3 NH 141414ia                   Total CoI = 1  I  totN  coiform
                                                      Ilow m Row or stage meas.           Cl   =chlorides N2  N03= nitrate-nitrite RO I5 =                 5-day biochemical
                                                      TKN  = total Kjetcdhal nitrogen     pH    = pH                                                        oxygen demand

                                                                                           B-37

                                                              Sample Stations: Lancaster

      Station  ITemp I DO I    pH ISaltICondtI TSS jTurbICotorITransjALkljNardj DOo5 1 NH3  I NO2 JTKNI TP ITOC I Cl  I Phen IMetalsiPest I Other ITotal IFecaLIFlow I Sed I Sed I
       No.     N          I                                 N I  I                                       1 I        1 IC I  INH4I NOCi                     I~ I    I   I     Org j

      PD-080 M          I  M      I  M                      I    I I  I  I                 I I      I M            I    A  I M           I M       I M         I I   I a

      PD-113      M     M    M                    M                  M    A     M     M     M     M    M    0                 QIa    A                     M   M A

      PD-152      M    m  M             M                                 A          M            M    m                      A                            M            A

      PD-179      M   M      M                    M M                          M            m          MI                                                   M

      PD-180    M I       i    I M       I            I      M     III I      I                 t I          I                    I I  I     I      I      I      I M      I
      PD-215    IMIMIMI             I      I     1141       I     IMIAIM    INIMIMIMIOI                             I      I  al M  M                                  A
      PD-24 6     M  I    I I       I I          I    I  I     I    I     I     I    M          I    I*     I    I   M     I     I        I             I I  I    I               I

      PD-247           M       I i              I     II       I    II I           I     1I                    I    I      I      I     I       I       I      I     I      I     I

      PO-250 I        (M  II   I           I     I  I       I     III              I     I M   I       I                                I I  I             M I       I      I     I

      PD-271 M               I        M          I14 I    I    I    I M  I  IMI M       I                        A I M   I M      I     I       I M            I            I     I

      PD-328  I        MI     i        I         II         I       I M     I   I I            I 1 1 I m             I            I     I       I       I m   I       I     I     I
      P0-180    IMI MIN I                   I      I 41          I    I    IN    I      114         114       I    I      I      I     I       I       IN    I

      P1-329                               1    11          I     I I I                       I    I                      I      I     I       IM      I M          I      I

      PD-333          lI      ii  I              II         I        I        I         I        1 1 1 1  I            I    I        I      I      I      I      I               I

      PD-334** I M     i i i                       I II          I   I I M    I       I     I    I A I               I       I     I                    I I  I  I    I m

      PD-335      M IM    I    I    I I          I    I     I     I    I    I   M        I      I    I   I     I    I      I      I     I       I       I       I   'I         I
                                                      Temp  =temperature                  Salt  = salinity            Trans = transparency           Sed= sediment (routine)
    M = monthly, 0 = quarterly, A  annually          DO    = dissolved oxygen             Condt = conductivity        Alk   = alkalinity             Sed Org  sediment organics
                                                      TSS   = total suspended solids      Hard  = hardness            TP  =   total phosphorus       Metals  heavy metals
    *Base-Neutral and Acid Extractable, and          Phen  = phenols                      Turb  = turbidity           TOC = total organic carbon     Fecal Coti = fecal cotiform
       Volatile Organics                             Pest =  pesticides and PCes      o    ther = other organics N lH3 NH4 = anwonia                 Total CoU =� total cotiform
                                                      Flow = flow or stage me~as.         C1   = chlorides            No NO3 = nitrate-nitrite SOD   = 5-day biochemical
    "*Monthly for cyanide at this station             TKN   = total Kjeldhat nitrogen     pH    = pH                                  25                     oxygen demand

                                                                                           B-38

                APPENDIX C

    TREND BIOLOGICAL MONITORING PROGRAM
           STATION DESCRIPTIONS

                    Fixed-Station Biological Network (70 Stations)

    Station   Station
    Number    Status           Descriotion                             County

    B-046     BWMP*       Broad River at Union Co. Road 389          Union/Chester

    B-054     BWMP        Enoree River at Newberry County
                          Road 45                                   Newberry

    B-236     BWMP        Broad River 2 km downstream                Fairfield/Richland
                          of SC Hwy 213

    BL-001    BWMP        Lawson's Fork Creek at Spartanburg
                          County Road 108                           Spartanburg

    C-007     BWMP        Congaree River at US Hwy 601               Richland/Calhoun

    CSB-001   BWMP        Congaree River 5 km downstream             Richland/Lexington
                          from US Hwy 176

    CSTL-098  BWMP        Combahee River 1 km upstream               Colleton/Beaufort
                          from US Hwy 17

    CSTL-109  BWMP        Coosawhatchie River at Hampton
                          County Road 27                            Hampton

    CW-016    BWMP        Catawba River at SC Hwy 9                  Chester/Lancaster

    CW-206    BWMP        Wateree River at US Hwy 76                 Richland/Sumter
                          and 378

    E-008     BWMP        North Fork Edisto River at
                          Orangeburg County Road 39                 Orangeburg

    E-015     BWMP        Edisto River at SC Hwy 61                  Dorchester/Colleton

    E-100     BWMP        Four Holes Swamp at US Hwy 78              Dorchester

    MD-048    BWMP        Collected as estuarine station
                          MD-214                                    Charleston

    MD-080    BWMP        Collected as estuarine station
                          MD-213                                    Georgetown

    PD-027    BWMP        Black Creek at Darlington County
                          Road 35                                   Darlington

    PD-028    BWMP        Pee Dee River at SC Hwy 34                 Darlington/Marlboro

    PD-038    BWMP        Lumber River at US Hwy 76                  Marion/Horry

    PD-061    BWMP        Pee Dee River at US Hwy 701                Horry/Georgetown

    * Basic Water Monitoring Program

                                           C-1

    Station   Station
    Number    Status                 Descriotion                       County

    D-202     BWMP        Pocotaligo River at SW Bridge                 Sumter
                          of Sumter"County Road 32

    S-018     BWMP        Reedy River at Greenville County
                          Road 448                                      Greenville

    S-125     BWMP        Saluda River at US Hwy 25 by-pass             Laurens

    ST-O01    BWMP        Santee River at US Hwy 17A                    Berkeley

    SV-118    BWMP        Savannah River at US Hwy. 301                 Allendale
    SV-291    BWMP        Clarks Hill Reservoir in Savannah             Aiken
                          River channel at US Hwy 378 (fish
                          tissue only)

    SV-323    BWMP        Savannah River 2 km downstream                Aiken
                          from dam at New Savannah Bluff
                          Lock and Dam

    CW-214    Special    Wateree River at 1-26                          Kershaw

    CW-222    Special    Wateree River upstream from                    Richland
                          Little River confluence

    MD-900    Special    Off-shore coastal waters; for                  Coastal
                          pelagic finfish tissue analyses
                          only.

    ST-507    Special    Lake Marion around Billy Elliott
                          landing immediately downlake of GSX           Sumter
                          hazardous waste disposal site

    ST-518    Special    Lake Marion in Otter Flats at                  Sumter
                          northwestern end of lake, uplake from
                          the GSX hazardous waste disposal site

    ST-519    Special    Lake Marion near the Rimini trestle,           Sumter
                         downlake from the GSX hazardous
                         waste disposal site

    ST-030    Special    Lake Marion near Wilson Dam                    Sumter
                          around Wyboo and Potato Creeks

    SV-531    Special    Langley Pond                                   Aiken

    SV-532    Special    Lake Hartwell near confluence of               Pickens
                         Seneca River and Eighteen Mile Creek

                                           C-2

    Station   Station
    Number    Status              Description                          County

    MD-212    Estuarine      Murrells Inlet-100 m south               Georgetown
                            of Marker 23, west bank at mouth
                            of small creek

    MD-213    Estuarine      Winyah Bay-off South Island              Georgetown
                            across from lighthouse

    MD-214    Estuarine      Charleston Harbor-off north              Charleston
                            point of Shute's Folly Island

    MD-215    Estuarine      Broad River-1.5 km south of              Beaufort
                            Archers Creek

    MD-216    Estuarine      South Edisto River off                   Charleston
                            northeast shore of Raccoon
                             Island - 500 m southeast of
                            Marker 157

    MD-538    Estuarine      Campbell Creek - east bank at            Beaufort
                            confluence with Whale Branch

    MD-632    Estuarine      May River-south bank 1 km                Beaufort
                            east of Bull Creek

    MD-633    Estuarine      Trenchards Inlet - Phillips              Beaufort
                             Island 1.5 km south of mouth
                            of Station Creek

    MD-634    Estuarine-    St. Helena Sound/Coosaw River-            Beaufort
                            Morgan Island at mouth of
                            Parrot Creek

    MD-635    Estuarine      Stono River - Snake I'sland              Charleston
                            at confluence of Stono and
                            Kiawah Rivers

    MD-636    Estuarine      Wando River - south bank                Charleston
                             I km SW of SC Hwy 41 below
                            power line

    MD-637    Estuarine      North Inlet - east bank of               Georgetown
                            Old Man Creek across from
                            mouth of Bly Creek

    MD-638    Estuarine      Little River Inlet - Goat Is.           Horry
                            at mouth of Horse Ford Creek

    MD-639    Estuarine      South Santee River - south               Charleston
                            bank across from southern tip
                            of Drum Island

    MD-640    Estuarine      Bulls Bay - at mouth of Long          Charleston
                            Creek, across from Morants Point

                                           C-3

    Station    Station
    Number     Status              Descriotion                        County

    MD-655    Estuarine      Savannah River - off Oyster              Jasper
                             Bed Island across from Coast
                            Guard Station

                                           C-4

                    APPENDIX D

    SHELLFISH STATION DESCRIPTIONS LISTED BY AREA

                                      AREA 1

    Station  #1    Little River Jetty

    Station  #2    Mouth of Dunn Sound Creek

    Station  #3    AIWW - Marker 9

    Station  #4    Mouth of Calabash Creek at AIWW

    Station  #5    Big Bend up Dunn Sound

    Station  #6    Bridge to Waties Island

    Station  #7    Hog Inlet

    Station  #8    AIWW - Marker 116

    Station  #9    AIWW - Marker 6

    Station #10    AIWW at U. S. Highway 17

    Station #11    Dock - Bird Island, North Carolina

    Station #12    Clayton Creek at Little River Inlet

    Station #13    Boat Landing - Bonaparte Landing, North Carolina

    Station #14    Palmetto Shores Marina Entrance

    Station #15    Ocean Drive Outfall and AIWW

    Station #16    50 yards north of Ocean Drive Outfall

    Station #17    42nd Avenue - Cherry Grove

    Station #17A   53rd Avenue Bridge on Canal

    Station #18    Dunn Sound at Hog Inlet

    Station #19    53rd Avenue at Main Creek

    Total    20

                                          AREA 2

    Station #1      White Point Swash

    Station #2      Singleton Swash

    Station #3      Canepatch Swash

    Total    3

                                          D-2

                                         AREA 3

    Station #1     Withers Swash

    Station #2      Pebble Beach - Midway Swash

    Total    2

                                         D-3

                                         AREA 4

    Station  #1    Main Creek at Atlantic Avenue Bridge

    Station  #1A   Main Creek at Stanley Drive

    Station  #2    Main Creek at Mickey Spillane's Home

    Station  #3    Main Creek at Captain Dick's Marina

    Station  #4    Main Creek at Marlin Quay Marina

    Station  #5    Murrells Inlet - Range Marker

    Station  #6    Allston Creek at Weston Flat

    Station  #7    Allston Creek POG - Hughes Landing

    Station  #8    Parsonnage Creek at Nance's Dock

    Station  #8A   Shell Landing at Huntingtoon Beach State Park

    Station  #9    Clubhouse Creek at Litchfield Boulevard Bridge

    Station #10    Shell Avenue and Pawley's Island Creek

    Station #11    North Causeway Bridge at Pawley's Island Creek

    Station #12    South Causeway Bridge at Pawley's Island

    Station #13    Pawley's Inlet

    Station #14    Dock - End of Sportsman Boulevard

    Station #15    Midway Inlet

    Station #16    Parsonnage Creek at Chicken Farm Ditch

    Station #17    Parsonnage Creek at Inlet Port Basin

    Station #18    North Boundary of Clambank Flats POG

    Station #19    Clubhouse Creek - First bend south of Salt Marsh Cove

    Station #21    South Pawley's Island Boat Landing

    Station #22    Huntington State Park Pond Outfall

    Station #23    Main Creek at Oyster Cove

    Station #24    Oaks Creek at First Curve

    Total    25

                                        D-4

                                         AREA 5

    Station  #1    Jones Creek at Nancy Creek

    Station  #2    Noble Slough

    Station  #3    North Inlet

    Station  #4    Town Creek at Debidue Creek

    Station  #5    Oyster Bay near Cut-off Creek

    Station  #6    No Man's Friend Creek and Mud Bay

    Station  #7    Jones Creek and Mud Bay

    Station  #8    Town Creek at Sixty Bass Creek

    Station  #9    Town Creek at Southern Entrance to Clambank Creek

    Station #10    Jones Creek at Duck Creek

    Station #11    Town Creek at Bread and Butter Creek

    Station #12    Confluence of Old Man Creek and Sea Creek Bay

    Station #13    Debidue Creek at Marina

    Station #14    Mid Channel Island - Bly Creek

    Station #15    Debidue Creek and Cooks Creek

    Station #16    Debidue Creek and Bass Hole Bay

    Station #20    Winyah Bay Main Channel - Buoy 19A, Range A E

    Station #21    Winyah Bay - Buoy 17, Range E

    Station #24    Winyah Bay Main Channel - Coast Guard Dock, Range C

    Station #25    Western Channel   Tip of Western Channel Island

    Total    20

                                        D-5

                                         AREA 6A

    Station  #1    South Santee River at Alligator Creek

    Station  #2    South Santee Inlet

    Station  #3    North Santee River at Crow Island and Cane Island

    Station  #4    North Santee Inlet

    Station  #5    North Santee River and Mosquito Creek

    Station #11    AIWW at Mimim Creek

    Total     6

                                        D-6

                                         AREA 6B

    Station  #6    Alligator Creek and Ocean Inlet

    Station  #7    Alligator Creek at Marker 26

    Station  #8    Casino Creek at Marker 29

    Station  #9    Dupree Creek at Marker 30

    Station #10    AIWW at Marker 32

    Station #12    Alligator Creek State Shellfish Ground

    Station #13    Alligator Creek nearest South Santee River between
                   Markers 24 and 25

    Station #14    Horsehead Creek at confluence with Cape Romain Harbor

    Station #15    Casino Creek at Cape Romain Harbor

    Station #16    Closer Line on Casino Creek

    Station #17    Congaree Creek at Tower Creek

    Station #18    Confluence of Dupree Creek and Clubhouse Creek

    Total    12

                                        D-7

                                         AREA 7

    Station  #1    Yenning Creek - First creek on left past Marker 64 Southbound

    Station  #1A   Venning Creek - Bulls Bay

    Station  #2    Graham Creek at Marker 64

    Station  #2A   Graham Creek and Bulls Bay

    Station  #3    Awendaw Creek at Marker 57

    Station  #4    Harbor River at Marker 48

    Station  #4A   Harbor River - Bulls Bay

    Station  #5    Tibwin Creek at Marker 42

    Station  #6    Five Fathom Creek at Marker 20

    Station  #6A   Five Fathom Creek at Bull River

    Station  #7    Jeremy Creek - Opposite fire tower

    Station  #8    Clubhouse Creek - 1/4 mile north of Five Fathom Creek

    Station  #8A   Oyster Bay at Muddy Bay

    Station  #9    Doehall Creek - 100 yards north of Marker 46

    Station #11    Five Fathom Creek at Marker 11

    Station #12    Confluence of Raccoon Creek and Romain River

    Station #13    Romain River at confluence of S Creek

    Total    17

                                        D-8

                                         AREA 8

    Station  #1    Morgan Creek at northernmost confluence with AIWW

    Station  #2    Hamlin Sound

    Station  #3    Dewees Inlet at AIWW - Marker 10

    Station  #4    Bull Yard Sound - Marker 104

    Station  #5    Whiteside Creek - Marker 96

    Station  #6    Mark Bay - Marker 90

    Station  #7    Price's Inlet

    Station  #8    AIWW - Marker 82

    Station  #9    Moore's Landing

    Station #10    1000 feet north of Isle of Palms STP outfall in AIWW

    Station #11    Isle of Palms STP Outfall at 41st Street

    Station #12    Morgan Creek at 41st Street Marina

    Station #13    Sewee Bay POG - Sewee Bay at-Hickory Bay

    Station #14    Dewees Island - 1/4 mile up Horsebend Creek

    Station #15    Dewees Island - Mouth of Watermelon Creek

    Total    15

                                        D-9

                                         AREA 9A

    Station  #1    Hamlin Creek at AIWW

    Station  #2    Upper end of Hamlin Creek at POG

    Station  #3    Upper end of Swinton Creek

    Station  #5    Shortcut - Swinton Creek

    Station  #6    Inlet Creek and Gentide Creek

    Station  #7    Inlet Creek and AIWW

    Station  #8    Breech Inlet

    Station  #9    Ben Sawyer Bridge

    Station #10    Marker 126 - AIWW at the Cove STP Outfall

    Station #11    End of 10th Street at Hamlin Creek

    Station #12    Swinton Creek and Hamlin Creek

    Station #14    Swinton Creek at AIWW

    Station #15    AIWW between Inlet and Swinton Creeks

    Station #17    Conch Creek State Shellfish Ground - Mt. Pleasant side

    Station #17A   Conch Creek State Shellfish Ground - Sullivan's Island side

    Station #18    AIWW adjacent to Wild Dunes Golf Course storm drainage outfall

    Station #19    AIWW at 25th Street - Isle of Palms

    Total    17

                                         AREA 9B

    Station  #1    Wando River at Neuell Creek

    Station  #2    Wando River at Horlbeck Creek

    Station  #3    Wando River at S.C. Highway 41 Bridge

    Station  #4    Wando River at Deep Creek

    Station  #5    Wando River opposite Big Paradise Island

    Station  #6    Wando River at Paradise Boat Landing

    Station  #7    Boone Hall Creek opposite County Recreation Area

    Station  #8    Wando River - Buoy 23

    Station  #9    Deep Creek - 1 mile from confluence with Wando River

    Station #10    Alston Creek STP Outfall

    Station #11    Wando River at Guerin Creek

    Station #12    Guerin Creek at Old House Creek

    Total    12

                                        AREA 10A

    Station  #1    Overhead Power Cable - Folly Creek

    Station  #2    Folly Creek Bridge

    Station  #3    Bowen Island Dock in Folly Creek

    Station  #4    Backman Creek at Folly Creek

    Station  #5    King Flats and Folly Creek

    Station  #6    Opposite Little Island in Folly Creek

    Station  #7    South boundary of CSZ - Folly Marina

    Station  #8    Folly River Bridge

    Station  #9    Last dock north in Folly River

    Station #11    Lighthouse Creek and Folly Creek at Rat Island Creek

    Station #13    First creek on left in Folly Creek - North of Pollution Line

    Station #14    Lighthouse Creek at Pollution Line

    Station #15    Secessionville Creek at Private Docks

    Station #15A   Folly Creek at Secessionville Pollution Line

    Station #16    Clark Sound at Ocean View Flats

    Station #16A   Fludd's Creek - Clark Sound

    Station #18    Mouth of Schooner Creek

    Station #18A   Charleston Harbor at Schooner Creek

    Station #19    Just inside Clark Sound from Schooner Creek

    Station #20    Backman's Commercial Dock in Backman Creek

    Station #22    Folly River State Shellfish Ground - opposite Folly Island

    Station #23    Lighthouse Creek SSG - Mouth of First Sister Creek

    Station #24    Cole Creek State Shellfish Ground

    Station #25    Folly Marina

    Total    24

                                        D-12

                                       AREA lOB

    Station  #1    Mouth of Charleston Harbor at Buoy 25

    Station  #2    200 yards east of mouth of Ft. Johnson Boat Basin

    Station  #2A   Off the end of James Island Yacht Club Dock

    Station  #3    Mouth of James Island Creek

    Station  #4    Ashley River at Buoy 2 - Red Nun Buoy

    Station  #5    Off the tip of The Battery at White Danger Marker

    Station  #6    Center of channel off Charleston Yacht Club

    Station  #7 Off old pier pilings at Castle Pinckney Ruins

    Station  #8    Center of Charleston Harbor at Buoy 3 - Green Can Buoy

    Station  #9    Mouth of Shem Creek at Marker 16   Red

    Station #10    Mt. Pleasant channel at Marker 18 - Red

    Station #11    AIWW at tip of Sullivan's Island Marker 127 - Green

    Total    12

                                        0-13

                                         AREA 11

    Station  #1    Elliott Cut at Stono River

    Station  #2    Stono Bridge at S.C. Highway 700

    Station  #3    Windmill - between Markers 10 and 11 in Stono River

    Station  #5    Mouth of Abbapoola Creek

    Station  #6    Up Abbapoola Creek at first large bend

    Station  #7    Green Creek at Stono River

    Station  #8    Mouth of Kiawah River

    Station #10    Kiawah River at Kiawah Island Boat Landing

    Station #11    AIWW - Marker 21A

    Station #12    SCL Railroad - Marker 27

    Station #15    Stono River - Marker 63

    Station #16    Stono River - Marker 54

    Station #17    Log Bridge Creek - Marker 51

    Station #18    Rantowles Creek at Stono River

    Station #19    Middle of Stono Inlet

    Station #20    Ashley River at Wappoo Cut

    Station #21    On the flats - South Kiawah River

    Station #22    Kiawah River POG - Mingo Point

    Station #23    Captain Sam's Creek and Kiawah River

    Station #24    Captain Sam's Creek at south tip of Long Island

    Station #26    Coburg Dairy on Wappoo Creek

    Station #27    Stono River at Mouth of creek near Marker 25

    Total    22

                                        D-14

                                         AREA 12

    Station  #1    Mouth of Church Creek - Marker 77'

    Station  #2    Goshen Point - Marker 69

    Station  #3    Yonges Island Creek - Marker 90

    Station  #4    Toogoodoo Creek - Marker 106

    Station  #5    Dawho Creek - Marker 110

    Station  #6    Steamboat Creek - Marker 2

    Station  #7    Westbank Creek at North Edisto River, opposite Leadenwah Creek

    Station  #8    Leadenwah Creek at North Edisto River

    Station  #9    Adams Creek at Bohicket Creek

    Station #10    Rockville Boat Landing

    Station #11    Adams Creek between Botany Bay Marina and Shrimp Dock

    Station #12    Leadenwah Creek 1 mile from confluence of North Edisto River

    Station #13    Bohicket Creek at Fickling Creek

    Station #14    S.C. Highway 700 bridge over Bohicket Creek

    Station #20    Bohicket Creek opposite Hoopstick Island at Pollution Line

    Station #21    Opposite old dam behind Rast House Restaurant

    Station #22    Opposite Boy Scout Camp

    Station #29    Raven Point Creek at Pollution Line

    Station #31    Bohicket Marina

    Station #32    Privateer Creek up 1/2 mile at fork

    Station #33    Confluence of Ocella Creek and South Creek

    Station #34    Toogoodoo Creek SSG at last creek before fork

    Station #35    Public Boat Ramp - Lower Toogoodoo Creek

    Station #36    Confluence of Tom Point Creek and North Edisto River

    Total    24

                                        D-15

                                         AREA 13

    Station  #1    Up Big Bay Creek at the mound

    Station  #2    Mouth of Big Bay Creek

    Station  #3    Mouth of St. Pierre Creek

    Station  #4    St. Pierre Creek at Peters Point

    Station  #5    Fishing Creek at Sandy Creek

    Station  #6    Confluence of Shingle Creek and Bailey Creek

    Station  #7    Store Creek opposite house with docks on right

    Station  #8    Edisto River at Ashepoo River

    Station  #9    Fishing Creek at Oyster Plant

    Station #10    Fishing Creek at Pollution Line

    Station #12    Headwaters of Fishing Creek past Oyster Plant

    Total    11

                                        D-16

                                         AREA 14

    Station  #2    Campbell Creek at Whale Branch

    Station  #4    Bull River Inlet and Coosaw River

    Station  #5    Combahee River Inlet and Coosaw River

    Station  #8    Ashepoo River at St. Helena Sound - Black Can Buoy

    Station  #9    St. Helena Sound at Morgan Back Creek

    Station #10    Parrot Creek and Coosaw River - Marker 1

    Station #11    Sam's Point and Coosaw River

    Station #12A   Confluence of Coosaw and Whale Branch

    Station #13    Halfmoon Creek at Whale Branch

    Station #14    Huspah Creek at railroad trestle

    Station #16A   2000 feet southeast of mouth of Fish Creek

    Statioh #17    Confluence of Wimbee Creek and South Wimbee Creek

    Station #18    Huspah Creek at Bull Point - Whale Branch POG

    Station #19    Ashepoo River POG

    Total    14

                                        D-17

                                         AREA 15

    Station  #1    Brickyard Point at Range Marker

    Station  #1A   McCaulley's Creek at Pawkie Island

    Station  #2    Mulligan Creek at Brickyard Creek

    Station  #3    Albergottie Creek at Beaufort River

    Station  #4    Broomfield Creek at Beaufort River

    Station #10    Battery Creek at Five Points Creek

    Station #14    Parris Island STP Outfall

    Station #15    Ballast Creek at Beaufort River

    Station #16    Station Creek at Beaufort River

    Station #17    Cat Island Creek at Cowan Creek

    Station #18    Second Middle Marsh in Cowan Creek

    Station #19    Battery Creek 1000 feet below Rabbit Island

    Station #20    Capers Creek SSG at Penn Community Services Retreat Center

    Station #21    Unnamed creek at discharge of BC High and Cherry Hill High

    Station #23    Distant Island State Shellfish Ground

    Total    15

                                         AREA 16

    Station  #2    Trenchard's Inlet at mouth of Station Creek

    Station  #3    Club Bridge Creek at Harbor River Sound

    Station  #4    Story River at Fripp Island

    Station  #5    Old House Creek at Fripp Inlet

    Station  #6    Harbor River at Marker A-13

    Station  #6F   Unnamed creek - Fripp Canal at Old House Creek

    Station  #8    Morgan River at Village Creek

    Station  #9    Edding Creek at Morgan River

    Station #11    Jenkins Creek at Morgan River

    Station #13    Lucy Point Creek at Rocky Springs Creek

    Station #13A   South edge of Lucy Point Creek CSZ at Pollution Line

    Station #13B   North edge of Lucy Point'Creek CSZ at Pollution Line

    Station #14    Doe Creek behind Coastal Seafood - Behind Dataw Island

    Station #17    Station Creek State Shellfish Ground - Beaufort County Landing

    Station #18   -Edding Creek at Shrimp Dock

    Total    15

                                        D-19

                                         AREA 17

    Station  #1    Broad River at S.A.L. Railroad Bridge

    Station  #2    Boyd Creek at Broad River

    Station  #3    Broad River at Whale Branch

    Station  #4E   Laurel Bay CSZ - Ebb Tide at South Pollution Line

    Station  #4F   Laurel Bay CSZ - Flood Tide at North Pollution Line

    Station  #7    Mouth of Chechessee Creek at Chechessee River

    Station  #8    Chechessee River Bridge

    Station  #9    Mouth of Euhaw Creek at Hazzard Creek

    Station #10A   Archers Creek 1000 feet west of bridge

    Station #12A   Ballast Creek near Page Field Road Causeway

    Station #13    Broad River at creek below Ballast Creek

    Station #14    Broad River at Parris Island Spit

    Station #16    Broad River at Corn Island - Mouth of creek

    Station #17    Hazzard Creek at Chechessee River

    Station #18    Hazzard Creek at Chelsea Plantation Clubhouse

    Station #19    Drainage canal at Hazzard Creek - U.S. Highway 278

    Station #19A   Drainage ditch by Hickory Hill Landfill

    Station #21    Confluence of Middle Creek and Whale Branch

    Total    18

                                        D-20

                                         AREA 18

    Station #1      Okatee River at Camp St. Mary's dock

    Station #2      Okatee River behind Bailey's Oyster Plant

    Station #3      Chechessee Creek at Okatee River

    Station #4      Callawassie Creek at Colleton River - Mouth of creek

    Station #5      Victoria Bluff - Colleton River at tree line

    Station #6      Sawmill Creek at Colleton River

    Station #7      Okatee River at Indigo Plantation

    Station #8      Okatee River at dock without house

    Total    8

                                        D-21

                                         AREA 19

    Station  #1    May River south of Palmetto'Bluff - Marker 8

    Station  #2    Unnamed creek at Jack Crow Island in Cooper River

    Station  #2A   Cooper River at New River

    Station  #3    Ramshorn Creek at Cooper River

    Station  #4    Cooper River at Marker 41 - Daufuskie Island

    Station  #5    Bloody Point at Mungen Creek

    Station  #6    Wright River - Marker 43

    Station  #7    Ramshorn Creek at New River

    Station  #8    First creek on left up New River - Pollution Line

    Station  #9    Bull Creek and Cooper River

    Station #11    Bull Creek at Savage Creek

    Station #12    Bull Creek and May River

    Station #16    May River behind Bluffton Oyster Co-op

    Station #17E   Cooper River Marina at edge of CSZ - Ebb Tide

    Station #17F   Cooper River Marina at edge of CSZ - Flood Tide

    Station #18    May River below Drainage Canals - Markers 22 and 23

    Station #19    May River below Drainage Canals - Marker 20

    Station #20    1.5 miles up Wright River from Fields Cut

    Station #21    2.5 miles up New River from Station 19-02A

    Total    19

                                        D-22

                                         AREA 20

    Station  #1    Braddock Point - South end of Hilton Head Island

    Station  #2    Calibogue Sound - Marker 32

    Station  #3    Shark Bank and Broad Creek - Marker 2 - CSZ Sea Pines STP

    Station  #4E   Broad Creek at Palmetto Bay Marina CSZ   Ebb Tide

    Station  #4F   Broad Creek at Palmetto Bay Marina CSZ   Flood Tide

    Station  #5    May River at Calibogue Sound

    Station  #6    Jarvis Creek at Calibogue Sound

    Station  #7    Buckingham Landing at bridge

    Station  #9    Mackey's Creek and Chechessee River

    Station #10    Skull Creek at Small Creek from Mariner's Cove

    Station #11    Skull Creek - Marker 19

    Station #12    Skull Creek behind Hilton Head Seafood Company

    Station #13    Skull Creek and Port Royal Sound

    Station #14E   500 feet north of Barnard Cove and Braddock Creek - Ebb Tide

    Station #14F   500 feet south of Barnard Cove and Braddock Creek - Flood Tide

    Station #15A   Broad Creek at Calibogue Sound - North end of Buck Island

    Station #16    Creek behind Lynn Smith's Oyster Plant at Broad Creek

    Station #16B   Canal from Palmetto Dunes at U.S. Highway 278 NE

    Station #16C   Canal at headwaters of Broad Creek off Matthews Drive

    Station #17A   Canal entering Broad Creek between Long Cove and Wexford
                   Plantation

    Station #17E   Broad Creek at Broad Creek Marina CSZ - Ebb Tide

    Station #17F   Broad Creek at Broad Creek Marina CSZ - Flood Tide

    Station #18    Shelter Cove Marina

    Station #18A   Canal from Palmetto Dunes at U.S. Highway 278 SW

    Station #19E   Broad Creek at Harbor Town Marina CSZ - Ebb Tide

    Station #19F   Broad Creek at Harbor Town Marina CSZ - Flood Tide

    Station #20E   Moss Creek Marina CSZ - Ebb Tide

                                        D-23

    AREA 20 (continued)

    Station #20F   Moss Creek Marina CSZ - Flood Tide

    station #21    Fish Haul Creek at Port Royal Sound

    Station #22    Old House Creek at Calibogue Sound

    Total    30

                                         D-24

                                 APPENDIX E

    LIST OF FACILITIES REQUIRING FEDERAL COMPLIANCE SAMPLING INSPECTIONS
                               BY EQC DISTRICT

                                County Codes

    01   Abbeville
    03   Aiken
    05   Allendale
    07   Anderson
    09   Bamberg
    11   Barnwell
    13   Beaufort
    15   Berkeley
    17   Calhoun
    19   Charleston
    21   Cherokee
    23   Chester
    25   Chesterfield
    27   Clarendon
    29   Colleton
    31   Darlington
    33   Dillon
    35   Dorchester
    37   Edgefield
    39   Fairfield
    41   Florence
    43   Georgetown
    45   Greenville
    47   Greenwood
    49   Hampton
    51   Horry
    53   Jasper
    55   Kershaw
    57   Lancaster
    59   Laurens
    61   Lee
    63   Lexington
    65   McCormick
     67   Marion
     69   Marlboro
     71   Newberry
     73   Oconee
     75   Orangeburg
     77   Pickens
     79   Richland
     81   Sal uda
     83   Spartanburg
     85   Sumter
     87   Union
     89   Williamsburg
     91   York

                                       E-1

                     CSI Inspections for Appalachia I (Al) District

                                          FY 1990

                                                                         Month
    NPDES #         Facility Name                             County #  Planned    Date

    SC0000281   Badische Corporation/Anderson                     07        Feb

        00400   Owens-Corning Fiberglas                          07         Feb

        00426   Blair Mills Inc.                                 07         Dec

        00477   Milliken & Co./Pendleton Finish                  07         Oct

        00485   Mount Vernon Mill/LaFrance Division              07         Apr

        00515   Duke Power/Oconee Nuclear Station                73         Mar

        00591   J.P. Stevens/Clemson Plant                       73         Dec

        01082   Ingersoll Rand/Torrington Plant                  07         Jul

        02291   Duke Power/Lee Steam Station                     07         May

        26701   Michelin Tire/Sandy Springs                      07         Apr

        23744   Anderson/Rocky River Plant                       07         Jan

        23752   Anderson/Generostee Creek Plt                    07         Jan

        23906   WCRSA/Piedmont Plant                             07         May

        25976   Williamston/South Plant                          07         Jun

        33553   Oconee County Sewer Comm./Coneross Crk           73         Mar

        35700   Pendleton - Clemson Regional Sewer               07         Oct

        39853   Easley/Middle Branch                             07         Sep

                                                                            Total 17

                                            E-2

                      CSI Inspections for Appalachia II (A2) District

                                           FY 1990

                                                                          Month     Date
    NPDES #         Facility Name                              County #  Planned  InsDected

    SC0000141   Cornell-Dubilier Marketing Inc                    77         Apr

        00264   Greenwood Mills/Liberty Plant #1                  77        Apr

        00302   BASF Corp./Fibers Division                        77        Aug

        01155   Platt Saco Lowell/Easley Plant                    77        Nov

        01791   Hoechst Celanese Corporation                      45        Mar

        03191   Milliken & Co./Gayley Mill                        45        Jan

        20010   Clemson/Main Plant                                77        Sep

        23035   Easley/Golden Creek Lagoon                       77         Jul

        23043   Easley/Georges Creek Lagoon                      77         Jul

        23922   WCRSA/Travelers Rest-East Lagoon                 45         Jan

        24261   WCRSA/Lower Reedy River Plant                    45         Jun

        24309   WCRSA/Taylors Area Plant                         45         Feb

        24317   WCRSA/Grove Creek Plant                          45         Jun

        33804   WCRSA/Wade Hampton Plant                         45         Nov

        37451   WCRSA/Parker Plant                               45         Oct

        37460   WCRSA/Lakeside Plant                             45         Oct

        40525   WCRSA/Gilder Creek                               45         Sep

        41211   WCRSA/Mauldin Road (New)                         45         Feb

                                                                            Total 18

                                            E-3

                     CSI Inspections for Appalachia III (A3) District

                                           FY 1990

                                                                          Month     Date
    NPDES #         Facility Name                              County #  Planned  InsDected

    SC0001368   Cone Mills/Carlisle Plant                         87         Dec

        01503   Reeves Brothers/Vulcan Urethane                   83         Jul

        02321   ABCO Industries Inc                               83         Feb

        02429   Spartan Mills/Montgomery Mill                     83         Dec

        02453   Spartan Mills/Startex Mill                        83         May

        02461   Spartanburg Steel Products Co.                    83         Aug

        02798   Hoechst Fibers Inc.                               83         Apr

        03051-  Milliken & Co./Lockhart Mill                      87         Dec

        03107   Phillips Fibers Corp.                             83         Aug

        03182   Milliken & Co./Magnolia Finish                    21         Mar

        03581   Milliken & Co./Milliken Chem                      83         Mar

        20427   SSSD/Lawson Fork Plant                            83         Jan

        20435   SSSD/Fairforest Plant                             83         Jan

        20478   Gaffney/Peoples Creek                             21         Sep

        20508   Gaffney/Providence Creek                          21         Sep

        20737   Woodruff/Dildine Creek                            83         Nov

        20761   Greer/Maple Creek Plant                           83         Oct

        20770   Greer/South Tyger River Plant                     83         Oct

        21172   Union/Toschs Creek Plant                          87         Oct

        21199   Union/Meng Creek Plant                            87         Oct

        21300   Lyman/Town of                                     83         May

        21601   Inman/City of                                     83         Jun

        23540   Milliken & Co./New Prospect Plant                 83         Sep

        24414   Inman Mills Water District                        83         Jun

        25763   Chesnee/Main Plant                                83         Sep

                                             E-4

    Appalachia III (continued)

                                                                         Month     Date
    NPDES #         Facility Name                              County #  Planned  Insoected

    SC0026042   Blacksburg/Canoe Creek                            21         May

        31551   Gaffney/Thicketty Creek                           21        Sep

        33855   Groce Laboratories                                83        Jul

        35734   Riverdale Mills Water District (New)             83         Dec

        35947   Spring City Knitting Company                      21        Mar

        36145   DNS Electronic Materials Inc.                     83        Dec

        37826   Speciality Ind. Prod. Inc.                       83         Nov

        40517   Thermal Oxid Corp./GSX                           83         Feb

                                                                            Total 33

                                            E-5

                         CSI Inspections for Catawba (CT) District

                                          FY 1990

                                                                         Month     Date
    NPDES #         Facility Name                             County #  Planned  Insoected

    SCO001015   Bowater Inc./Carolina Corporation                91         May

        01783   Hoechst Celanese/Celriver Plant                  91        Jun

        03255   Springs Mills/Grace Finishing                    57        Feb

        04278   Duke Power/Catawba Nuclear Station               91        Apr

        20303   Clover/Calabash Creek Plant                      91        Feb

        20371   Fort Mill/Harris & Jackson Street               91         Jan

        20443   Rock Hill/Manchester Creek                       91        Oct

        21211   Great Falls/Town of                              23        Aug

        22080   Lancaster/Town of                                57        Jul

        35360   R-M Industries, Inc.                             91        Apr

        36056   Chester/Rocky Creek Plant                        23        Jul

        36081   Chester/Sandy River Plant                        23        Jul

        38156   York/Fishing Creek Plant (New)                   91        Jan

                                                                           Total 13

                                           E-6

                   CSI Inspections for Central Midlands (CM) District

                                           FY 1990

                                                                         Month     Date
    NPDES #         Facility Name                             County #  Planned  InsDected

    SC0001333   Carolina Eastman Company                         17         Oct

        01848   Westinghouse Electric/Columbia Plant             79         May

        02038   SCE&G/Wateree Station                            79        Oct

        02046   SCE&G/McMeekin Station                           63        Oct

        02402   J.B. Martin Company                              63         Sep

        03425   Mepco-Electra, Inc.                              63        Jul

        03557   Allied Corp./Allied-Signal Inc                   63        Jul

        04286   Square D Company                                 79        Apr

        20125   Winnsboro/Jackson Creek                          39        Aug

        20940   Columbia/Metro Plant                             79        Aug

        22390   Whitmire/Town of                                 71        Apr

        22900   Ridgeway/Town of                                 39        Nov

        24147   Cayce/Main Plant                                 63        Nov

        24465   Batesburg/Town of                                63        Jan

        24490   Newberry/Bush River                              71        Sep

        29483   Alpine Utilities                                 63        Jan

        30856   SCE&G/Summer Nuclear                             39         Feb

        33367   Teepak, Inc.                                     17        Mar

        34541   AT&T Nassau Metals Corporation                   63        Oct

        34762   Lindau Chemicals, Inc.                           79         Feb

        38121   Union Camp Corporation                           79        Apr

        38865   East Richland Co. PSD (New)                      79        Nov

        40631   Chapin/Town of                                  .63        Dec

        40860   Newberry Co. Plant #1/Bush river                 71        Mar

        41661   Richland Co./Nicholas Creek                      79        Jun

                                                                           Total 25
                                            E-7

                      CSI Inspections for Low Country (LC) District

                                          FY 1990

                                                                         Month     Date
    NPDES #         Facility Name                             Countv #  Planned  InsDected

    SC0000825   US Marines/Beaufort Air Station                  13         Aug

        00914   Lobeco Products, Inc.                            13        Feb

        01830   Westinghouse Electic/Hampton Plant               49        Dec

        02020   SCE&G/Canadys Station                            29        Apr

        02135   J.P. Stevens Industrial/Walterboro Plant         29        Mar

        02577   U.S. Marine Corp./Island Depot                   13        Feb

        21016   Beaufort/City of                                 13        Aug

        21318   Hampton/Town of                                  49        Dec

        24121   Sea Pines PSD                                    13        May

        25399   Estill/Town of                                   49        July

        25950   Yemassee/Town of                                 49        Nov

        34584   Hardeeville/Church Road                          53        Jul

        40436   Walterboro/City of                               29        Mar

                                                                           Total 13

                                           E-8

                     CSI Inspections for Lower Savannah (LS) District

                                           FY 1990

                                                                         Month     Date
    NPDES #         Facility Name                              County #  Planned  Insoected

    SC0000175   U.S. Department of Energy/Savannah River          11         Nov

        00221   Whitlock Combing Co.                              05        Jan

        00574   SCE&G/Urguart Steam Station                       03        Feb

        00582   Kimberly-Clark Corporation                       03         Jul

        01147   Georgia Pacific/Holly Hill Lumber                 75        Apr

        01163   Greenwood Mills/Liner Plant #17                  75         May

        01180   Ethyl Corp./Orangeburg Plant                      75        Mar

        03093   Milliken & Co./Barnwell Mill                      11        Jan

        03531   Greenwood Mills/Edisto Plant                     75         May

        03999   Shuron Inc                                        11        Sep

        24457   Aiken Co. PSA/Horse Creek                        03         Feb

        24481   Orangeburg/New Facility                          75         Aug

        25143   Barnwell/City of                                 11         Jul

        26417   Blackville/Town of                                11        Feb

        39918   Allendale/Town of                                05         May

        40215   Denmark/City of                                  09         Apr

    ND0063061   Williston/Town of                                 11        Sep

                                                                           Total 19

                                            E-9

                         CSI Inspections for Pee Dee (PD) District

                                           FY 1990

                                                                          Month     Date
    NPDES #         Facility Name                              County #  Planned  InsDected

    SC0000876   Stone Container Corp./Florence                    41         May

        01473   L-Tec Company                                     41         Jan

        01805   Mohasco Ind/Dixiana Mill                          33         Aug

        01872   AVM of S.C.                                       67         Feb

        02151   Delta Mills Inc/Delta Plt. 2 & 3                  69         Jul

        02500   Dixie Yarns Inc/Caro Knit Plt.                    25         Nov

        02704   Galey & Lord Inc/Society Hill                     31         Sep

        02917   DuPont/Florence Plant                             41         Dec

        02925   Carolina PWR/HB Robinson SS                       31         Jan

        03042   Sonoco Products/Hartsville #11                    31         Nov

        04162   Fiber Industries Inc                              31         Apr

        20249   Cheraw/Town of                                    25         Oct

        20257   Marion/South Main Street Plant                    67         Nov

        21580   Hartwville/City of                                31         Oct

        21776   Dillon/Little Pee Dee River Plant                 33         Aug

        22128   Florence/Main Plant                               41         Sep

        24767   Jefferson/Town of                                 25         Nov

        25178   Bennettsville/Town of                             69         May

        25232   Chesterfield/Thompson Creek                       25         Dec

        25356   Timmonsville/Town of                              41         Apr

        25933   Johnsonville/East Plant                           41         Jan

        29408   Mullins/White Oak Creek Plant                     67         Nov

        38164   Lake City/Lake Swamp Plant                        41         Jul

        39624   Darlington/WWTF-Black Creek                       31         Feb

                                                                            Total 24

                                            E-10

                         CSI Inspections for Trident (TD) District

                                           FY 1990

                                                                         Month     Date
    NPDES #         Facility Name                             County #  Planned  InsDected

    SC0000990   Plusa Inc                                        15         Apr

        01091   SC Public Service/Jeffries Steam                 15         May

        01759   Westvaco Corp./Charleston Mill                   19         Nov

        02011   SCE&G/Hagood Station                             19         Sep

        03115   Ga Pacific/Russeliville Plant                    15        May

        03441   Mobay Chemical/Bushy Park Plant                  15         Feb

        03883   SCE&G/Williams Station                           15         Feb

        26506   DuPont/Cooper River Plant                        15        Jan

        28584   Amoco Chemical Co./Cooper River                  15        Apr

        38555   Showa Denko, Inc.                                35        Oct

        21041   Hanahan/Town of                                  15        Nov

        21229   Charleston/Plum Island Plant                     19        Jan

        21296   Mt. Pleasant/Main Plant                          19        Aug

        21598   Moncks Corner/Town of                            15        Jul

        24783   NCSD/Felix C. Davis WWTP                         19        Sep

        25844   St. George/Town of                               35        Oct

        26051   St. Andrews PSD/Savage Road Plant                19        Jan

        26069   St. Andrews PSD/Pierpont Plant                   19        Jan

        37541   Summerville/Ox Pond (New)                        35        Jun

        38032   DCW&SA/Lower Berkeley WTP                        15        Dec

        38822   Dorchester PW/Lower Dorchester                   35        Jun

        39764   BCW&SA/Central Berkeley WTP                      15        Jul

                                                                           Total 22

                                           E-11

                    CSI Inspections for Upper Savannah (US) District

                                           FY 1990

                                                                         Month     Date
    NPDES #         Facility Name                             County #  Planned  InsDected

    SC0000299   Fieldcrest Cannon/Rocky River                     01        Sep

        00353   Milliken & Company/Abbeville Mill                01         Feb

        00396   Milliken & Company/McCormick Mill                65         Apr

        20214   Ware Shoals/Dairy Street Plant                   47         Nov

        20702   Laurens/Town of                                  59         Mar

        21709   Greenwood/Wilson Creek Plant                     47         Aug

        22268   Ridge Spring/South Lagoon 1                      81         Mar

        22381   Saluda/Town of                                   81         Jan

        22403   Due West/Town of                                 01         Nov

        22870   Greenwood/West Alexander Plant                   47         Mar

        25330   ECW&SA/Brooks Avenue Plant                       37         Oct

        25691   ECW&SA/Johnston #1                               37         Jul

        25721   Calhoun Falls/Town of                            01         May

        36048   Ninety-six/Town of                               47         Dec

        37974   Laurens Co. WRC/Clinton-Joanna                   59         Aug

        40002   WCRSA/Durbin Creek                               59         Dec

        40614   Abbeville/Long Cane Crek                         01         Oct

                                                                           Total 17

                                            E-12

                        CSI Inspections for Waccamaw (WM) District

                                           FY 1990

                                                                          Month     Date
    NPDES #         Facility Name                              County #  Planned  InsDected

    SC0000868   International Paper Company                       43         Oct

        01104   SC Public Service/Grainger Steam                  51        Feb

        01431   Georgetown Steel Corporation                      43        Jun

        02780   Wolverine Brass Works Conway                      51        Nov

        22471   SC Public Service/Winyah Steam Station            43        Mar

        21733   Conway Oxidation Pond #3                         51         Jan

        22152   N. Myrtle Beach/Ocean Drive Plant                 51        Jul

        22161   N. Myrtle Beach/Crescent Beach                   51         Jul

        25135   Andrews/Town of                                  43         Mar

        25348   Loris/Town of                                    51         Dec

        35971   Kingstree/New Plant                              89         Sep

        37753   GSW&SA/Schwartz Plant                            51         Aug

        39039   Myrtle Beach/Main Plant (New)                     51        May

        39900   GSW&SA/Central Wetlands Plant                    51         Apr

        40029   Georgetown/City of                               43         Oct

                                                                            Total 1'5

                                            E-13

                         CSI Inspections for Wateree (WR) District

                                           FY 1990

                                                                          Month     Date
    NPDES #         Facility Name                              County #  Planned  Insoected

    SC0000795   Campbell Soup Company                             85         Jul

        01341   Veratec Inc/Bethune Plant                         55         Sep

        01490   Reeves Bros/Bishopville Finish                    61         May

        02518   Hermitage Industries                              55         Nov

        02585   DuPont/May Plant                                  55         Dec

        02682   Hardwick Chemical Company                         55         Mar

        20419   Manning/Town of                                   27         Feb

        21032   Camden/City of                                    55         Aug

        24554   Crescent/Div. Cooper Industries                   85         Jun

        27707   Sumter/Pocataligo River Plant                     85         Mar

        35378   Bishopville/Town of                               61         Oct

        39870   Kershaw Co/Lugoff Plant                           55         Apr

                                                                            Total - 12

                                            E-14