47
Telecommunication
5
1998-10-01
1998-10-01
false

Frequencies for narrow-band direct-printing (NBDP), radioprinter and data transmissions.
80.361

Section 80.361
SAFETY AND SPECIAL RADIO SERVICES
STATIONS IN THE MARITIME SERVICES
Frequencies
Radiotelegraphy
§ 80.361
Frequencies for narrow-band direct-printing (NBDP), radioprinter and data transmissions.
(a) Paired channels. (1) The following frequencies are available for assignment to public coast stations for narrow-band direct-printing (NBDP) and data transmissions. The paired ship frequencies are available for use by authorized ship stations for NBDP and data transmissions.
Ch. no. | Paired frequencies for NBDP and data transmissions (kHz) | 4 MHz | Coast | Ship | 6 MHz | Coast | Ship | 8 MHz | Coast | Ship | 12 MHz | Coast | Ship | 16 MHz | Coast | Ship | 18/19 MHz | Coast | Ship | 22 MHz | Coast | Ship | 25/26 MHz | Coast | Ship
1 | 4210.5 | 4172.5 | 6314.5 | 6263.0 | | | 12579.5 | 12477.0 | 16807.0 | 16683.5 | 19681.0 | 18870.5 | 22376.5 | 22284.5 | 26101.0 | 25173.0
2 | 4211.0 | 4173.0 | 6315.0 | 6263.5 | 8417.0 | 8377.0 | 12580.0 | 12477.5 | 16807.5 | 16684.0 | 19681.5 | 18871.0 | 22377.0 | 22285.0 | 26101.5 | 25173.5
3 | 4211.5 | 4173.5 | 6315.5 | 6264.0 | 8417.5 | 8377.5 | 12580.5 | 12478.0 | 16808.0 | 16684.5 | 19682.0 | 18871.5 | 22377.5 | 22285.5 | 26102.0 | 25174.0
4 | 4212.0 | 4174.0 | 6316.0 | 6264.5 | 8418.0 | 8378.0 | 12581.0 | 12478.5 | 16808.5 | 16685.0 | 19682.5 | 18872.0 | 22378.0 | 22286.0 | 26102.5 | 25174.5
5 | 4212.5 | 4174.5 | 6316.5 | 6265.0 | 8418.5 | 8378.5 | 12581.5 | 12479.0 | 16809.0 | 16685.5 | 19683.0 | 18872.5 | 22378.5 | 22286.5 | 26103.0 | 25175.0
6 | 4213.0 | 4175.0 | 6317.0 | 6265.5 | 8419.0 | 8379.0 | 12582.0 | 12479.5 | 16809.5 | 16686.0 | 19683.5 | 18873.0 | 22379.0 | 22287.0 | 26103.5 | 25175.5
7 | 4213.5 | 4175.5 | 6317.5 | 6266.0 | 8419.5 | 8379.5 | 12582.5 | 12480.0 | 16810.0 | 16686.5 | 19684.0 | 18873.5 | 22379.5 | 22287.5 | 26104.0 | 25176.0
8 | 4214.0 | 4176.0 | 6318.0 | 6266.5 | 8420.0 | 8380.0 | 12583.0 | 12480.5 | 16810.5 | 16687.0 | 19684.5 | 18874.0 | 22380.0 | 22288.0 | 26104.5 | 25176.5
9 | 4214.5 | 4176.5 | 6318.5 | 6267.0 | 8420.5 | 8380.5 | 12583.5 | 12481.0 | 16811.0 | 16687.5 | 19685.0 | 18874.5 | 22380.5 | 22288.5 | 26105.0 | 25177.0
10 | 4215.0 | 4177.0 | 6319.0 | 6267.5 | 8421.0 | 8381.0 | 12584.0 | 12481.5 | 16811.5 | 16688.0 | 19685.5 | 18875.0 | 22381.0 | 22289.0 | 26105.5 | 25177.5
11 | | | | | 8421.5 | 8381.5 | 12584.5 | 12482.0 | 16812.0 | 16688.5 | 19686.0 | 18875.5 | 22381.5 | 22289.5 | 26106.0 | 25178.0
12 | 4215.5 | 4178.0 | 6319.5 | 6268.5 | 8422.0 | 8382.0 | 12585.0 | 12482.5 | 16812.5 | 16689.0 | 19686.5 | 18876.0 | 22382.0 | 22290.0 | 26106.5 | 25178.5
13 | 4216.0 | 4178.5 | 6320.0 | 6269.0 | 8422.5 | 8382.5 | 12585.5 | 12483.0 | 16813.0 | 16689.5 | 19687.0 | 18876.5 | 22382.5 | 22290.5 | 26107.0 | 25179.0
14 | 4216.5 | 4179.0 | 6320.5 | 6269.5 | 8423.0 | 8383.0 | 12586.0 | 12483.5 | 16813.5 | 16690.0 | 19687.5 | 18877.0 | 22383.0 | 22291.0 | 26107.5 | 25179.5
15 | 4217.0 | 4179.5 | 6321.0 | 6270.0 | 8423.5 | 8383.5 | 12586.5 | 12484.0 | 16814.0 | 16690.5 | 19688.0 | 18877.5 | 22383.5 | 22291.5 | 26108.0 | 25180.0
16 | 4217.5 | 4180.0 | 6321.5 | 6270.5 | 8424.0 | 8384.0 | 12587.0 | 12484.5 | 16814.5 | 16691.0 | 19688.5 | 18878.0 | 22384.0 | 22292.0 | 26108.5 | 25180.5
17 | 4218.0 | 4180.5 | 6322.0 | 6271.0 | 8424.5 | 8384.5 | 12587.5 | 12485.0 | 16815.0 | 16691.5 | 19689.0 | 18878.5 | 22384.5 | 22292.5 | 26109.0 | 25181.0
18 | | | 6322.5 | 6271.5 | 8425.0 | 8385.0 | 12588.0 | 12485.5 | 16815.5 | 16992.0 | 19689.5 | 18879.0 | 22385.0 | 22293.0 | 26109.5 | 25181.5
19 | | | 6323.0 | 6272.0 | 8425.5 | 8385.5 | 12588.5 | 12486.0 | 16816.0 | 16692.5 | 19690.0 | 18879.5 | 22385.5 | 22293.5 | 26110.0 | 25182.0
20 | | | 6323.5 | 6272.5 | 8426.0 | 8386.0 | 12589.0 | 12486.5 | 16816.5 | 16693.0 | 19690.5 | 18880.0 | 22386.0 | 22294.0 | 26110.5 | 25182.5
21 | | | 6324.0 | 6273.0 | 8426.5 | 8386.5 | 12589.5 | 12487.0 | 16817.0 | 16693.5 | 19691.0 | 18880.5 | 22386.5 | 22294.5 | |
22 | | | 6324.5 | 6273.5 | 8427.0 | 8387.0 | 12590.0 | 12487.5 | 16817.5 | 16694.0 | 19691.5 | 18881.0 | 22387.0 | 22295.0 | |
23 | | | 6325.0 | 6274.0 | 8427.5 | 8387.5 | 12590.5 | 12488.0 | 16818.0 | 16694.5 | | | 22387.5 | 22295.5 | |
24 | | | 6325.5 | 6274.5 | 8428.0 | 8388.0 | 12591.0 | 12488.5 | | | | | 22388.0 | 22296.0 | |
25 | | | 6326.0 | 6275.0 | 8428.5 | 8388.5 | 12591.5 | 12489.0 | 16818.5 | 16695.5 | | | 22388.5 | 22296.5 | |
26 | | | 6326.5 | 6275.5 | 8429.0 | 8389.0 | 12592.0 | 12489.5 | 16819.0 | 16696.0 | | | 22389.0 | 22297.0 | |
27 | | | 6327.0 | 6281.0 | 8429.5 | 8389.5 | 12592.5 | 12490.0 | 16819.5 | 16696.5 | | | 22389.5 | 22297.5 | |
28 | | | 6327.5 | 6281.5 | 8430.0 | 8390.0 | 12593.0 | 12490.5 | 16820.0 | 16697.0 | | | 22390.0 | 22298.0 | |
29 | | | 6328.0 | 6282.0 | 8430.5 | 8390.5 | 12593.5 | 12491.0 | 16820.5 | 16697.5 | | | 22390.5 | 22298.5 | |
30 | | | | | 8431.0 | 8391.0 | 12594.0 | 12491.5 | 16821.0 | 16698.0 | | | 22391.0 | 22299.0 | |
31 | | | | | 8431.5 | 8391.5 | 12594.5 | 12492.0 | 16821.5 | 16698.5 | | | 22391.5 | 22299.5 | |
32 | | | | | 8432.0 | 8392.0 | 12595.0 | 12492.5 | 16822.0 | 16699.0 | | | 22392.0 | 22300.0 | |
33 | | | | | 8432.5 | 8392.5 | 12595.5 | 12493.0 | 16822.5 | 16699.5 | | | 22392.5 | 22300.5 | |
34 | | | | | 8433.0 | 8393.0 | 12596.0 | 12493.5 | 16823.0 | 16700.0 | | | 22393.0 | 22301.0 | |
35 | | | | | | | 12596.5 | 12494.0 | 16823.5 | 16700.5 | | | 22393.5 | 22301.5 | |
36 | | | | | | | 12597.0 | 12494.5 | 16824.0 | 16701.0 | | | 22394.0 | 22302.0 | |
37 | | | | | | | 12597.5 | 12495.0 | 16824.5 | 16701.5 | | | 22394.5 | 22302.5 | |
38 | | | | | | | 12598.0 | 12495.5 | 16825.0 | 16702.0 | | | 22395.0 | 22303.0 | |
39 | | | | | | | 12598.5 | 12496.0 | 16825.5 | 16702.5 | | | 22395.5 | 22303.5 | |
40 | | | | | | | 12599.0 | 12496.5 | 16826.0 | 16703.0 | | | 22396.0 | 22304.0 | |
41 | | | | | | | 12599.5 | 12497.0 | 16826.5 | 16703.5 | | | 22396.5 | 22304.5 | |
42 | | | | | | | 12600.0 | 12497.5 | 16827.0 | 16704.0 | | | 22397.0 | 22305.0 | |
43 | | | | | | | 12600.5 | 12498.0 | 16827.5 | 16704.5 | | | 22397.5 | 22305.5 | |
44 | | | | | | | 12601.0 | 12498.5 | 16828.0 | 16705.0 | | | 22398.0 | 22306.0 | |
45 | | | | | | | 12601.5 | 12499.0 | 16828.5 | 16705.5 | | | 22398.5 | 22306.5 | |
| 46 | | | | | | | 12602.0 | 12499.5 | 16829.0 | 16706.0 | | | 22399.0 | 22307.0 | |
47 | | | | | | | 12602.5 | 12500.0 | 16829.5 | 16706.5 | | | 22399.5 | 22307.5 | |
48 | | | | | | | 12603.0 | 12500.5 | 16830.0 | 16707.0 | | | 22400.0 | 22308.0 | |
49 | | | | | | | 12603.5 | 12501.0 | 16830.5 | 16707.5 | | | 22400.5 | 22308.5 | |
50 | | | | | | | 12604.0 | 12501.5 | 16831.0 | 16708.0 | | | 22401.0 | 22309.0 | |
51 | | | | | | | 12604.5 | 12502.0 | 16831.5 | 16708.5 | | | 22401.5 | 22309.5 | |
52 | | | | | | | 12605.0 | 12502.5 | 16832.0 | 16709.0 | | | 22402.0 | 22310.0 | |
53 | | | | | | | 12605.5 | 12503.0 | 16832.5 | 16709.5 | | | 22402.5 | 22310.5 | |
54 | | | | | | | 12606.0 | 12503.5 | 16833.0 | 16710.0 | | | 22403.0 | 22311.0 | |
55 | | | | | | | 12606.5 | 12504.0 | 16833.5 | 16710.5 | | | 22403.5 | 22311.5 | |
56 | | | | | | | 12607.0 | 12504.5 | 16834.0 | 16711.0 | | | 22404.0 | 22312.0 | |
57 | | | | | | | 12607.5 | 12505.0 | 16834.5 | 16711.5 | | | 22404.5 | 22312.5 | |
58 | | | | | | | 12608.0 | 12505.5 | 16835.0 | 16712.0 | | | 22405.0 | 22313.0 | |
59 | | | | | | | 12608.5 | 12506.0 | 16835.5 | 16712.5 | | | 22405.5 | 22313.5 | |
60 | | | | | | | 12609.0 | 12506.5 | 16836.0 | 16713.0 | | | 22406.0 | 22314.0 | |
61 | | | | | | | 12609.5 | 12507.0 | 16836.5 | 16713.5 | | | 22406.5 | 22314.5 | |
62 | | | | | | | 12610.0 | 12507.5 | 16837.0 | 16714.0 | | | 22407.0 | 22315.0 | |
63 | | | | | | | 12610.5 | 12508.0 | 16837.5 | 16714.5 | | | 22407.5 | 22315.5 | |
64 | | | | | | | 12611.0 | 12508.5 | 16838.0 | 16715.0 | | | 22408.0 | 22316.0 | |
65 | | | | | | | 12611.5 | 12509.0 | 16838.5 | 16715.5 | | | 22408.5 | 22316.5 | |
66 | | | | | | | 12612.0 | 12509.5 | 16839.0 | 16716.0 | | | 22409.0 | 22317.0 | |
67 | | | | | | | 12612.5 | 12510.0 | 16839.5 | 16716.5 | | | 22409.5 | 22317.5 | |
68 | | | | | | | 12613.0 | 12510.5 | 16400.0 | 16717.0 | | | 22410.0 | 22318.0 | |
69 | | | | | | | 12613.5 | 12511.0 | 16400.5 | 16717.5 | | | 22410.5 | 22318.5 | |
70 | | | | | | | 12614.0 | 12511.5 | 16411.0 | 16718.0 | | | 22411.0 | 22319.0 | |
71 | | | | | | | 12614.5 | 12512.0 | 16841.5 | 16718.5 | | | 22411.5 | 22319.5 | |
72 | | | | | | | 12615.0 | 12512.5 | 16842.0 | 16719.0 | | | 22412.0 | 22320.0 | |
73 | | | | | | | 12615.5 | 12513.0 | 16842.5 | 16719.5 | | | 22412.5 | 22320.5 | |
74 | | | | | | | 12616.0 | 12513.5 | 16843.0 | 16720.0 | | | 22413.0 | 22321.0 | |
75 | | | | | | | 12616.5 | 12514.0 | 16843.5 | 16720.5 | | | 22413.5 | 22321.5 | |
76 | | | | | | | 12617.0 | 12514.5 | 16844.0 | 16721.0 | | | 22414.0 | 22322.0 | |
77 | | | | | | | 12617.5 | 12515.0 | 16844.5 | 16721.5 | | | 22414.5 | 22322.5 | |
78 | | | | | | | 12618.0 | 12515.5 | 16845.0 | 16722.0 | | | 22415.0 | 22323.0 | |
79 | | | | | | | 12618.5 | 12516.0 | 16845.5 | 16722.5 | | | 22415.5 | 22323.5 | |
80 | | | | | | | 12619.0 | 12516.5 | 16846.0 | 16723.0 | | | 22416.0 | 22324.0 | |
81 | | | | | | | 12619.5 | 12517.0 | 16846.5 | 16723.5 | | | 22416.5 | 22324.5 | |
82 | | | | | | | 12620.0 | 12517.5 | 16847.0 | 16724.0 | | | 22417.0 | 22325.0 | |
83 | | | | | | | 12620.5 | 12518.0 | 16847.5 | 16724.5 | | | 22417.5 | 22325.5 | |
84 | | | | | | | 12621.0 | 12518.5 | 16848.0 | 16725.0 | | | 22418.0 | 22326.0 | |
85 | | | | | | | 12621.5 | 12519.0 | 16848.5 | 16725.5 | | | 22418.5 | 22326.5 | |
86 | | | | | | | 12622.0 | 12519.5 | 16849.0 | 16726.0 | | | 22419.0 | 22327.0 | |
87 | | | | | | | | | 16849.5 | 16726.5 | | | 22419.5 | 22327.5 | |
88 | | | | | | | 12622.5 | 12520.5 | 16850.0 | 16727.0 | | | 22420.0 | 22328.0 | |
89 | | | | | | | 12623.0 | 12521.0 | 16850.5 | 16727.5 | | | 22420.5 | 22328.5 | |
90 | | | | | | | 12623.5 | 12521.5 | 16851.0 | 16728.0 | | | 22421.0 | 22329.0 | |
| 91 | | | | | | | 12624.0 | 12522.0 | 16851.5 | 16728.5 | | | 22421.5 | 22329.5 | |
92 | | | | | | | 12624.5 | 12522.5 | 16852.0 | 16729.0 | | | 22422.0 | 22330.0 | |
93 | | | | | | | 12625.0 | 12523.0 | 16852.5 | 16729.5 | | | 22422.5 | 22330.5 | |
94 | | | | | | | 12625.5 | 12523.5 | 16853.0 | 16730.0 | | | 22423.0 | 22331.0 | |
95 | | | | | | | 12626.0 | 12524.0 | 16853.5 | 16730.5 | | | 22423.5 | 22331.5 | |
96 | | | | | | | 12626.5 | 12524.5 | 16854.0 | 16731.0 | | | 22424.0 | 22332.0 | |
97 | | | | | | | 12627.0 | 12525.0 | 16854.5 | 16731.5 | | | 22424.5 | 22332.5 | |
98 | | | | | | | 12627.5 | 12525.5 | 16855.0 | 16732.0 | | | 22425.0 | 22333.0 | |
99 | | | | | | | 12628.0 | 12526.0 | 16855.5 | 16732.5 | | | 22425.5 | 22333.5 | |
100 | | | | | | | 12628.5 | 12526.5 | 16856.0 | 16733.0 | | | 22426.0 | 22334.0 | |
101 | | | | | | | 12629.0 | 12527.0 | 16856.5 | 16733.5 | | | 22426.5 | 22334.5 | |
102 | | | | | | | 12629.5 | 12527.5 | 16857.0 | 16739.0 | | | | | |
103 | | | | | | | 12630.0 | 12528.0 | 16857.5 | 16739.5 | | | | | |
104 | | | | | | | 12630.5 | 12528.5 | 16858.0 | 16740.0 | | | | | |
105 | | | | | | | 12631.0 | 12529.0 | 16858.5 | 16740.5 | | | | | |
106 | | | | | | | 12631.5 | 12529.5 | 16859.0 | 16741.0 | | | | | |
107 | | | | | | | 12632.0 | 12530.0 | 16859.5 | 16741.5 | | | | | |
108 | | | | | | | | | 16860.0 | 16742.0 | | | | | |
109 | | | | | | | | | 16860.5 | 16742.5 | | | | | |
110 | | | | | | | | | 16861.0 | 16743.0 | | | | | |
111 | | | | | | | | | 16861.5 | 16743.5 | | | | | |
112 | | | | | | | | | 16862.0 | 16744.0 | | | | | |
113 | | | | | | | | | 16862.5 | 16744.5 | | | | | |
114 | | | | | | | | | 16863.0 | 16745.0 | | | | | |
115 | | | | | | | | | 16863.5 | 16745.5 | | | | | |
116 | | | | | | | | | 16864.0 | 16746.0 | | | | | |
117 | | | | | | | | | 16864.5 | 16746.5 | | | | | |
118 | | | | | | | | | 16865.0 | 16747.0 | | | | | |
119 | | | | | | | | | 16865.5 | 16747.5 | | | | | |
120 | | | | | | | | | 16866.0 | 16748.0 | | | | | |
121 | | | | | | | | | 16866.5 | 16748.5 | | | | | |
122 | | | | | | | | | 16867.0 | 16749.0 | | | | | |
123 | | | | | | | | | 16867.5 | 16749.5 | | | | | |
124 | | | | | | | | | 16868.0 | 16750.0 | | | | | |
125 | | | | | | | | | 16868.5 | 16750.5 | | | | | |
126 | | | | | | | | | 16869.0 | 16751.0 | | | | | |
127 | | | | | | | | | 16869.5 | 16751.5 | | | | | |
128 | | | | | | | | | 16870.0 | 16752.0 | | | | | |
129 | | | | | | | | | 16870.5 | 16752.5 | | | | | |
130 | | | | | | | | | 16871.0 | 16753.0 | | | | | |
131 | | | | | | | | | 16871.5 | 16753.5 | | | | | |
132 | | | | | | | | | 16872.0 | 16754.0 | | | | | |
(2) Applicants for these frequencies must submit a substantial showing of need based on the following factors:
(i) A schedule of each currently licensed NBDP frequency and the expected use of the proposed frequencies;
(ii) For additional frequencies within the same MHz band, a factual showing of the 3 busiest hours of any 4 days within a consecutive 10 day period for each of the 2 months immediately preceding the filing of the application indicating that the applicant has used its currently assigned frequencies within the same MHz band an aggregate average of at least 40% of the 3 busiest hours of each day for exchanging communications; and
(iii) Any other facts that support the need for the proposed assignment, e.g., evidence of radio interference by another station located near enough to render a currently licensed frequency substantially unusable.
(b) Non-paired channels. The following table describes the frequencies and Channel Series with F1B or J2B emission which are assignable to ship stations for NB-DP and data transmissions with other ship stations and public coast stations. Public coast stations may receive only on these frequencies.
Non-Paired NBDP Channels (kHz)
Channel series:
1 | 4202.5 | 6300.5 | 8396.5 | 12560.0 | 16785.0 | 18893.0 | 22352.0 | 25193.0
2 | 4203.0 | 6301.0 | 8397.0 | 12560.5 | 16785.5 | 18893.5 | 22352.5 | 25193.5
3 | 4203.5 | 6301.5 | 8397.5 | 12561.0 | 16786.0 | 18894.0 | 22353.0 | 25194.0
4 | 4204.0 | 6302.0 | 8398.0 | 12561.5 | 16786.5 | 18894.5 | 22353.5 | 25194.5
5 | 4204.5 | 6302.5 | 8398.5 | 12562.0 | 16787.0 | 18895.0 | 22354.0 | 25195.0
6 | 4205.0 | 6303.0 | 8399.0 | 12562.5 | 16787.5 | 18895.5 | 22354.5 | 25195.5
7 | 4205.5 | 6303.5 | 8399.5 | 12563.0 | 16788.0 | 18896.0 | 22355.0 | 25196.0
8 | 4206.0 | 6304.0 | 8400.0 | 12563.5 | 16788.5 | 18896.5 | 22355.5 | 25196.5
9 | 4206.5 | 6304.5 | 8400.5 | 12564.0 | 16789.0 | 18897.0 | 22356.0 | 25197.0
10 | 4207.0 | 6305.0 | 8401.0 | 12564.5 | 16789.5 | 18897.5 | 22356.5 | 25197.5
11 | | 6305.5 | 8401.5 | 12565.0 | 16790.0 | 18898.0 | 22357.0 | 25198.0
12 | | 6306.0 | 8402.0 | 12565.5 | 16790.5 | | 22357.5 | 25198.5
13 | | 6306.5 | 8402.5 | 12566.0 | 16791.0 | | 22358.0 | 25199.0
14 | | 6307.0 | 8403.0 | 12566.5 | 16791.5 | | 22358.5 | 25199.5
15 | | 6307.5 | 8403.5 | 12567.0 | 16792.0 | | 22359.0 | 25200.0
16 | | 6308.0 | 8404.0 | 12567.5 | 16792.5 | | 22359.5 | 25200.5
17 | | 6308.5 | 8404.5 | 12568.0 | 16793.0 | | 22360.0 | 25201.0
18 | | 6309.0 | 8405.0 | 12568.5 | 16793.5 | | 22360.5 | 25201.5
19 | | 6309.5 | 8405.5 | 12569.0 | 16794.0 | | 22361.0 | 25202.0
20 | | 6310.0 | 8406.0 | 12569.5 | 16794.5 | | 22361.5 | 25202.5
21 | | 6310.5 | 8406.5 | 12570.0 | 16795.0 | | 22362.0 | 25203.0
22 | | 6311.0 | 8407.0 | 12570.5 | 16795.5 | | 22362.5 | 25203.5
23 | | 6311.5 | 8407.5 | 12571.0 | 16796.0 | | 22363.0 | 25204.0
24 | | | 8408.0 | 12571.5 | 16796.5 | | 22363.5 | 25204.5
25 | | | 8408.5 | 12572.0 | 16797.0 | | 22364.0 | 25205.0
26 | | | 8409.0 | 12572.5 | 16797.5 | | 22364.5 | 25205.5
27 | | | 8409.5 | 12573.0 | 16798.0 | | 22365.0 | 25206.0
28 | | | 8410.0 | 12573.5 | 16798.5 | | 22365.5 | 25206.5
29 | | | 8410.5 | 12574.0 | 16799.0 | | 22366.0 | 25207.0
30 | | | 8411.0 | 12574.5 | 16799.5 | | 22366.5 | 25207.5
31 | | | 8411.5 | 12575.0 | 16800.0 | | 22367.0 | 25208.0
32 | | | 8412.0 | 12575.5 | 16800.5 | | 22367.5 |
33 | | | 8412.5 | 12576.0 | 16801.0 | | 22368.0 |
34 | | | 8413.0 | 12576.5 | 16801.5 | | 22368.5 |
35 | | | 8413.5 | | 16802.0 | | 22369.0 |
36 | | | 8414.0 | | 16802.5 | | 22369.5 |
37 | | | | | 16803.0 | | 22370.0 |
38 | | | | | 16803.5 | | 22370.5 |
39 | | | | | 16804.0 | | 22371.0 |
40 | | | | | | | 22371.5 |
41 | | | | | | | 22372.0 |
42 | | | | | | | 22372.5 |
43 | | | | | | | 22373.0 |
44 | | | | | | | 22373.5 |
45 | | | | | | | 22374.0 |
(c) Distress and calling. The frequencies 2174.5 kHz, 4177.5 kHz, 6268.0 kHz, 8376.5 kHz, 12520.0 kHz, and 16695.0 kHz may be used for NBDP and data transmissions by coast and ship stations on a simplex basis for distress and safety purposes.
(d) The frequencies in the 156-162 MHz band available for assignment to public coast stations that are contained in § 80.371(c) of this part are also available for radioprinter and data communications between ship and coast stations using F1B, F2B, F1D, or F2D emission.
[51 FR 31213, Sept. 2, 1986, as amended at 56 FR 9890, Mar. 8, 1991; 57 FR 43407, Sept. 21, 1992; 58 FR 16504, Mar. 29, 1993]